<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.2">
<drawing>
<board>
<plain>
<hole x="18.4785" y="26.8478" drill="2.54"/>
<hole x="21.8059" y="26.8986" drill="2.54"/>
<text>OMSI - ADN Puzzles</text>
<text>12/29/2014</text>
<text>thomas hudson</text>
<wire x1="57.15" y1="78.74" x2="57.15" y2="0" width="0.254" layer="20"/>
<wire x1="52.07" y1="-0.635" x2="12.065" y2="-0.635" width="0.254" layer="20"/>
<wire x1="12.065" y1="-0.635" x2="9.525" y2="-6.35" width="0.254" layer="20"/>
<hole x="39.37" y="25.4" drill="3.175"/>
<hole x="11.43" y="25.4" drill="3.175"/>
<hole x="6.35" y="-5.08" drill="3.175"/>
<hole x="54.61" y="1.27" drill="3.175"/>
<hole x="54.61" y="76.2" drill="3.175"/>
<hole x="6.35" y="77.47" drill="3.175"/>
<wire x1="3.81" y1="-6.985" x2="3.81" y2="78.74" width="0.254" layer="20"/>
<wire x1="52.07" y1="-0.635" x2="57.15" y2="0" width="0" layer="20" curve="83.358481"/>
<wire x1="9.525" y1="-6.35" x2="3.81" y2="-6.985" width="0" layer="20" curve="-96.641519"/>
<text>LIGHT</text>
<wire x1="10.16" y1="79.375" x2="53.34" y2="79.375" width="0.254" layer="20"/>
<wire x1="3.81" y1="78.74" x2="10.16" y2="79.375" width="0.254" layer="20" curve="-108.970408"/>
<wire x1="53.34" y1="79.375" x2="57.15" y2="78.74" width="0.254" layer="20" curve="-108.970408"/>
<text>GND</text>
<text>Color Matching, Make a 'T',</text>
<text>Hall Effect Sensors</text>
<text>Color Matching - 6 sensors</text>
<text>Make a 'T' - 5 sensors</text>
<text>5V</text>
<text>SENSOR 1</text>
<text>SENSOR 2</text>
<text>SENSOR 3</text>
<text>SENSOR 4</text>
<text>SENSOR 5</text>
<text>SENSOR 6</text>
<text>Hall Effect Sensor: US1881LSE-AAA-000-RE</text>
<text>TX</text>
<text>RX</text>
<text>5V</text>
<text>GND</text>
<text>A3</text>
<text>(2)</text>
<text>(3)</text>
<text>(4)</text>
<text>(5)</text>
<text>(6)</text>
<text>(7)</text>
<text>and 6 Blocks in a Box</text>
<text>6 Blocks in a Box - 2 sensors</text>
<text>LID Switch</text>
<text>Weight Switch</text>
<text>Backlight ON indicator</text>
</plain>
<libraries>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="OMSI - ADN">
<packages>
<package name="SO08">
</package>
<package name="1X01-16GAUGE">
</package>
<package name="S016M">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SCREWTERMINAL-5MM-2">
</package>
<package name="JST-4-PTH">
</package>
<package name="JST-3-PTH">
</package>
</packages>
</library>
<library name="SparkFun">
<packages>
<package name="0805">
</package>
<package name="LED-1206">
</package>
<package name="RELAY-S108T02">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="ARDUINOR3-BPLACE">
</package>
</packages>
</library>
<library name="Bee_Counter">
<description>Generated from &lt;b&gt;Bee_Counter.sch&lt;/b&gt;&lt;p&gt;
by exp-project-lbr.ulp</description>
<packages>
<package name="JUMPER_SJ">
<description>&lt;b&gt;Solder jumper&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="FET1.1" library="OMSI - ADN" package="SO08" value="MOSFET_ARRAY">
<attribute name="NAME"/>
</element>
<element name="GND" library="OMSI - ADN" package="1X01-16GAUGE" value="M01ADN">
<attribute name="NAME"/>
</element>
<element name="5V" library="OMSI - ADN" package="1X01-16GAUGE" value="M01ADN">
<attribute name="NAME"/>
</element>
<element name="PINGND" library="OMSI - ADN" package="1X01-16GAUGE" value="M01ADN"/>
<element name="RES-10K-UP" library="OMSI - ADN" package="S016M" value="RESISTOR-ARRAYS16-MEDIUM">
<attribute name="NAME"/>
</element>
<element name="BACK_LIGHT" library="SparkFun" package="LED-1206" value="">
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun" package="0805" value="330">
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun" package="0805" value="190">
<attribute name="VALUE"/>
</element>
<element name="U1" library="SparkFun" package="RELAY-S108T02" value="S108T02"/>
<element name="POWER4" library="SparkFun-Connectors" package="SCREWTERMINAL-5MM-2" value="M025MM"/>
<element name="R1" library="SparkFun-Passives" package="0805" value="10k">
<attribute name="VALUE"/>
</element>
<element name="U$1" library="OMSI - ADN" package="SO08" value="MOSFET_ARRAY_P-CH">
<attribute name="NAME"/>
</element>
<element name="1" library="SparkFun" package="LED-1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="2" library="SparkFun" package="LED-1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="OMSI - ADN" package="SO08" value="MOSFET_ARRAY_P-CH">
<attribute name="NAME"/>
</element>
<element name="3" library="SparkFun" package="LED-1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="4" library="SparkFun" package="LED-1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$3" library="OMSI - ADN" package="SO08" value="MOSFET_ARRAY_P-CH">
<attribute name="NAME"/>
</element>
<element name="5" library="SparkFun" package="LED-1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="6" library="SparkFun" package="LED-1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP3" library="SparkFun-Connectors" package="JST-4-PTH" value=""/>
<element name="5V1" library="OMSI - ADN" package="1X01-16GAUGE" value="M01ADN"/>
<element name="RES-150-DOWN" library="OMSI - ADN" package="S016M" value="RESISTOR-ARRAYS16-MEDIUM">
<attribute name="NAME"/>
</element>
<element name="U2" library="adafruit" package="ARDUINOR3-BPLACE" value="ARDUINOR3-BPLACE"/>
<element name="JP6" library="SparkFun-Connectors" package="JST-3-PTH" value=""/>
<element name="JP5" library="SparkFun-Connectors" package="JST-3-PTH" value=""/>
<element name="JP4" library="SparkFun-Connectors" package="JST-3-PTH" value=""/>
<element name="JP3X" library="SparkFun-Connectors" package="JST-3-PTH" value=""/>
<element name="JP2" library="SparkFun-Connectors" package="JST-3-PTH" value=""/>
<element name="JP1" library="SparkFun-Connectors" package="JST-3-PTH" value=""/>
<element name="U$4" library="OMSI - ADN" package="SO08" value="MOSFET_ARRAY_P-CH">
<attribute name="NAME"/>
</element>
<element name="U$5" library="OMSI - ADN" package="SO08" value="MOSFET_ARRAY_P-CH">
<attribute name="NAME"/>
</element>
<element name="U$7" library="OMSI - ADN" package="SO08" value="MOSFET_ARRAY_P-CH">
<attribute name="NAME"/>
</element>
<element name="POWER1" library="Bee_Counter" package="JUMPER_SJ" value=""/>
<element name="POWER2" library="Bee_Counter" package="JUMPER_SJ" value=""/>
<element name="POWER3" library="Bee_Counter" package="JUMPER_SJ" value=""/>
<element name="POWER5" library="Bee_Counter" package="JUMPER_SJ" value=""/>
<element name="POWER6" library="Bee_Counter" package="JUMPER_SJ" value=""/>
<element name="POWERX4" library="Bee_Counter" package="JUMPER_SJ" value=""/>
<element name="GND_OPTION" library="Bee_Counter" package="JUMPER_SJ" value=""/>
<element name="JP10" library="SparkFun-Connectors" package="JST-3-PTH" value=""/>
<element name="RES-10K-DOWN" library="OMSI - ADN" package="S016M" value="RESISTOR-ARRAYS16-MEDIUM">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="GND" pad="1"/>
<contactref element="FET1.1" pad="3"/>
<contactref element="R1" pad="1"/>
<contactref element="FET1.1" pad="1"/>
<contactref element="PINGND" pad="1"/>
<contactref element="RES-150-DOWN" pad="16"/>
<contactref element="U2" pad="GND"/>
<contactref element="GND_OPTION" pad="1"/>
<contactref element="U2" pad="GND1"/>
<contactref element="U2" pad="GND2"/>
<contactref element="JP10" pad="2"/>
<contactref element="RES-10K-DOWN" pad="16"/>
</signal>
<signal name="5V">
<contactref element="5V" pad="1"/>
<contactref element="RES-10K-UP" pad="16"/>
<contactref element="BACK_LIGHT" pad="A"/>
<contactref element="R3" pad="2"/>
<contactref element="U$1" pad="1"/>
<contactref element="U$1" pad="3"/>
<contactref element="U$2" pad="1"/>
<contactref element="U$2" pad="3"/>
<contactref element="U$3" pad="1"/>
<contactref element="U$3" pad="3"/>
<contactref element="5V1" pad="1"/>
<contactref element="U2" pad="5V"/>
<contactref element="U2" pad="5V"/>
<contactref element="U$4" pad="1"/>
<contactref element="U$4" pad="3"/>
<contactref element="U$5" pad="1"/>
<contactref element="U$5" pad="3"/>
<contactref element="U$7" pad="1"/>
<contactref element="U$7" pad="3"/>
<contactref element="POWER1" pad="2"/>
<contactref element="POWER2" pad="2"/>
<contactref element="POWER3" pad="2"/>
<contactref element="POWER5" pad="2"/>
<contactref element="POWER6" pad="2"/>
<contactref element="POWERX4" pad="2"/>
<contactref element="JP10" pad="1"/>
</signal>
<signal name="N$117">
</signal>
<signal name="N$1">
<contactref element="RES-10K-UP" pad="1"/>
<contactref element="U$1" pad="2"/>
<contactref element="U2" pad="D2"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="N$3">
<contactref element="RES-10K-UP" pad="2"/>
<contactref element="U$1" pad="4"/>
<contactref element="U2" pad="D3"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="RES-10K-UP" pad="3"/>
<contactref element="U$2" pad="2"/>
<contactref element="U2" pad="D4"/>
<contactref element="JP3X" pad="3"/>
</signal>
<signal name="N$6">
<contactref element="RES-10K-UP" pad="5"/>
<contactref element="U$3" pad="2"/>
<contactref element="U2" pad="D6"/>
<contactref element="JP5" pad="3"/>
</signal>
<signal name="CTL">
<contactref element="FET1.1" pad="4"/>
<contactref element="R1" pad="2"/>
<contactref element="U2" pad="D13"/>
</signal>
<signal name="N$20">
<contactref element="BACK_LIGHT" pad="C"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="COIL">
<contactref element="R4" pad="1"/>
<contactref element="U1" pad="4"/>
<contactref element="FET1.1" pad="6"/>
<contactref element="FET1.1" pad="5"/>
</signal>
<signal name="LOAD2">
<contactref element="U1" pad="2"/>
<contactref element="POWER4" pad="1"/>
</signal>
<signal name="LOAD1">
<contactref element="U1" pad="1"/>
<contactref element="POWER4" pad="2"/>
</signal>
<signal name="N$25">
<contactref element="R3" pad="1"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="N$28">
<contactref element="U$1" pad="7"/>
<contactref element="U$1" pad="8"/>
<contactref element="1" pad="A"/>
</signal>
<signal name="N$19">
<contactref element="2" pad="A"/>
<contactref element="U$1" pad="6"/>
<contactref element="U$1" pad="5"/>
</signal>
<signal name="N$30">
<contactref element="U$2" pad="4"/>
<contactref element="RES-10K-UP" pad="4"/>
<contactref element="U2" pad="D5"/>
<contactref element="JP4" pad="3"/>
</signal>
<signal name="N$31">
<contactref element="U$2" pad="7"/>
<contactref element="U$2" pad="8"/>
<contactref element="3" pad="A"/>
</signal>
<signal name="N$32">
<contactref element="4" pad="A"/>
<contactref element="U$2" pad="6"/>
<contactref element="U$2" pad="5"/>
</signal>
<signal name="N$34">
<contactref element="U$3" pad="4"/>
<contactref element="RES-10K-UP" pad="6"/>
<contactref element="U2" pad="D7"/>
<contactref element="JP6" pad="3"/>
</signal>
<signal name="N$35">
<contactref element="U$3" pad="7"/>
<contactref element="U$3" pad="8"/>
<contactref element="5" pad="A"/>
</signal>
<signal name="N$36">
<contactref element="6" pad="A"/>
<contactref element="U$3" pad="6"/>
<contactref element="U$3" pad="5"/>
</signal>
<signal name="N$7">
<contactref element="1" pad="C"/>
<contactref element="RES-150-DOWN" pad="15"/>
</signal>
<signal name="N$21">
<contactref element="2" pad="C"/>
<contactref element="RES-150-DOWN" pad="14"/>
</signal>
<signal name="N$22">
<contactref element="3" pad="C"/>
<contactref element="RES-150-DOWN" pad="13"/>
</signal>
<signal name="N$24">
<contactref element="4" pad="C"/>
<contactref element="RES-150-DOWN" pad="12"/>
</signal>
<signal name="N$26">
<contactref element="5" pad="C"/>
<contactref element="RES-150-DOWN" pad="11"/>
</signal>
<signal name="N$27">
<contactref element="6" pad="C"/>
<contactref element="RES-150-DOWN" pad="10"/>
</signal>
<signal name="VIN">
<contactref element="U2" pad="VIN"/>
</signal>
<signal name="3V">
<contactref element="U2" pad="3V"/>
</signal>
<signal name="N$8">
<contactref element="U$4" pad="2"/>
<contactref element="U2" pad="D8"/>
<contactref element="RES-10K-DOWN" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="U$4" pad="4"/>
<contactref element="U2" pad="D9"/>
<contactref element="RES-10K-DOWN" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="U$5" pad="2"/>
<contactref element="U2" pad="D10"/>
<contactref element="RES-10K-DOWN" pad="3"/>
</signal>
<signal name="N$14">
<contactref element="U$7" pad="2"/>
<contactref element="U2" pad="D12"/>
<contactref element="RES-10K-DOWN" pad="5"/>
</signal>
<signal name="P6">
<contactref element="U$4" pad="7"/>
<contactref element="U$4" pad="8"/>
<contactref element="JP6" pad="1"/>
<contactref element="POWER6" pad="1"/>
</signal>
<signal name="P5">
<contactref element="U$4" pad="6"/>
<contactref element="U$4" pad="5"/>
<contactref element="JP5" pad="1"/>
<contactref element="POWER5" pad="1"/>
</signal>
<signal name="N$23">
<contactref element="U$5" pad="4"/>
<contactref element="U2" pad="D11"/>
<contactref element="RES-10K-DOWN" pad="4"/>
</signal>
<signal name="P4">
<contactref element="U$5" pad="7"/>
<contactref element="U$5" pad="8"/>
<contactref element="JP4" pad="1"/>
<contactref element="POWERX4" pad="1"/>
</signal>
<signal name="P3">
<contactref element="U$5" pad="6"/>
<contactref element="U$5" pad="5"/>
<contactref element="JP3X" pad="1"/>
<contactref element="POWER3" pad="1"/>
</signal>
<signal name="N$37">
<contactref element="U$7" pad="4"/>
<contactref element="U2" pad="A0"/>
<contactref element="RES-10K-DOWN" pad="6"/>
</signal>
<signal name="P2">
<contactref element="U$7" pad="7"/>
<contactref element="U$7" pad="8"/>
<contactref element="JP2" pad="1"/>
<contactref element="POWER2" pad="1"/>
</signal>
<signal name="P1">
<contactref element="U$7" pad="6"/>
<contactref element="U$7" pad="5"/>
<contactref element="JP1" pad="1"/>
<contactref element="POWER1" pad="1"/>
</signal>
<signal name="SENSOR_GND">
<contactref element="FET1.1" pad="8"/>
<contactref element="FET1.1" pad="7"/>
<contactref element="JP1" pad="2"/>
<contactref element="JP2" pad="2"/>
<contactref element="JP3X" pad="2"/>
<contactref element="JP4" pad="2"/>
<contactref element="JP5" pad="2"/>
<contactref element="JP6" pad="2"/>
<contactref element="GND_OPTION" pad="2"/>
</signal>
<signal name="SENSOR_GND_PIN">
<contactref element="FET1.1" pad="2"/>
<contactref element="U2" pad="A1"/>
<contactref element="RES-10K-UP" pad="7"/>
</signal>
<signal name="N$15">
<contactref element="U2" pad="D0"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="N$16">
<contactref element="U2" pad="D1"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="U2" pad="A5"/>
<contactref element="JP3" pad="3"/>
</signal>
<signal name="N$18">
<contactref element="U2" pad="A4"/>
<contactref element="JP3" pad="4"/>
</signal>
<signal name="N$29">
<contactref element="U2" pad="A3"/>
<contactref element="JP10" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
