<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="13.335" x2="101.27" y2="13.335" width="0" layer="20"/>
<wire x1="101.27" y1="13.335" x2="101.27" y2="76.825" width="0" layer="20"/>
<wire x1="101.27" y1="76.825" x2="0" y2="76.825" width="0" layer="20"/>
<wire x1="0" y1="76.825" x2="0" y2="13.335" width="0" layer="20"/>
<text>SIN</text>
<text>SCLK</text>
<text>XLAT</text>
<text>BLANK</text>
<text>GND</text>
<text>5V</text>
<text>GCLK</text>
<text>SOUT</text>
<text>modular-muse.com</text>
<text>0</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>5</text>
<text>6</text>
<text>7</text>
<text>8</text>
<text>9</text>
<text>10</text>
<text>11</text>
<text>12</text>
<text>13</text>
<text>14</text>
<text>15</text>
<text>PWR1</text>
<text>PWR2</text>
<text>TLC5940</text>
<text>TLC5940</text>
<text>solenoid/DC driver</text>
<text>short me to</text>
<text>share pwr 1&amp;2</text>
</plain>
<libraries>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TO220V">
<description>&lt;b&gt;TO 220 Vertical&lt;/b&gt; Package works with various parts including N-Channel MOSFET SparkFun SKU: COM-10213</description>
</package>
<package name="DIODE-1N4001">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="POWER_JACK_PTH">
</package>
<package name="1X02_2.54_SCREWTERM">
</package>
<package name="1X08_PIN1_NO_SILK">
</package>
<package name="SCREWTERMINAL-5MM-2">
</package>
<package name="1X02_LONGPADS">
</package>
</packages>
</library>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DIL28-3">
<description>Standard 28-pin DIP package.&lt;br&gt;
IC needs to have legs bent before insertion.</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.4">
<description>1/4W Resistor, 0.4" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
<package name="CAP-PTH-SMALLEZ">
<description>This is the "EZ" version of the .1" spaced ceramic thru-hole cap.&lt;br&gt;
It has reduced top mask to make it harder to put the component on the wrong side of the board.</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CAP-PTH-LARGE">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="DIODE0" library="SparkFun-DiscreteSemi" package="DIODE-1N4001" value=""/>
<element name="R0" library="SparkFun-Resistors" package="AXIAL-0.3" value="10k">
<attribute name="PROD_ID" value="RES-9435"/>
</element>
<element name="DIODE1" library="SparkFun-DiscreteSemi" package="DIODE-1N4001" value=""/>
<element name="R1" library="SparkFun-Resistors" package="AXIAL-0.3" value="10k">
<attribute name="PROD_ID" value="RES-9435"/>
</element>
<element name="DIODE2" library="SparkFun-DiscreteSemi" package="DIODE-1N4001" value=""/>
<element name="R2" library="SparkFun-Resistors" package="AXIAL-0.3" value="10k">
<attribute name="PROD_ID" value="RES-9435"/>
</element>
<element name="U1" library="SparkFun-DigitalIC" package="DIL28-3" value="TLC5940-NT"/>
<element name="R3" library="SparkFun-Passives" package="AXIAL-0.4" value="10k"/>
<element name="R4" library="SparkFun-Passives" package="AXIAL-0.4" value="2.2k"/>
<element name="C1" library="SparkFun-Passives" package="CAP-PTH-SMALLEZ" value=""/>
<element name="DIODE3" library="SparkFun-DiscreteSemi" package="DIODE-1N4001" value=""/>
<element name="R5" library="SparkFun-Resistors" package="AXIAL-0.3" value="10k">
<attribute name="PROD_ID" value="RES-9435"/>
</element>
<element name="DIODE4" library="SparkFun-DiscreteSemi" package="DIODE-1N4001" value=""/>
<element name="R6" library="SparkFun-Resistors" package="AXIAL-0.3" value="10k">
<attribute name="PROD_ID" value="RES-9435"/>
</element>
<element name="DIODE5" library="SparkFun-DiscreteSemi" package="DIODE-1N4001" value=""/>
<element name="R7" library="SparkFun-Resistors" package="AXIAL-0.3" value="10k">
<attribute name="PROD_ID" value="RES-9435"/>
</element>
<element name="DIODE6" library="SparkFun-DiscreteSemi" package="DIODE-1N4001" value=""/>
<element name="R8" library="SparkFun-Resistors" package="AXIAL-0.3" value="10k">
<attribute name="PROD_ID" value="RES-9435"/>
</element>
<element name="DIODE7" library="SparkFun-DiscreteSemi" package="DIODE-1N4001" value=""/>
<element name="R9" library="SparkFun-Resistors" package="AXIAL-0.3" value="10k">
<attribute name="PROD_ID" value="RES-9435"/>
</element>
<element name="DIODE8" library="SparkFun-DiscreteSemi" package="DIODE-1N4001" value=""/>
<element name="R10" library="SparkFun-Resistors" package="AXIAL-0.3" value="10k">
<attribute name="PROD_ID" value="RES-9435"/>
</element>
<element name="DIODE9" library="SparkFun-DiscreteSemi" package="DIODE-1N4001" value=""/>
<element name="R11" library="SparkFun-Resistors" package="AXIAL-0.3" value="10k">
<attribute name="PROD_ID" value="RES-9435"/>
</element>
<element name="DIODE10" library="SparkFun-DiscreteSemi" package="DIODE-1N4001" value=""/>
<element name="R12" library="SparkFun-Resistors" package="AXIAL-0.3" value="10k">
<attribute name="PROD_ID" value="RES-9435"/>
</element>
<element name="DIODE11" library="SparkFun-DiscreteSemi" package="DIODE-1N4001" value=""/>
<element name="R13" library="SparkFun-Resistors" package="AXIAL-0.3" value="10k">
<attribute name="PROD_ID" value="RES-9435"/>
</element>
<element name="DIODE12" library="SparkFun-DiscreteSemi" package="DIODE-1N4001" value=""/>
<element name="R14" library="SparkFun-Resistors" package="AXIAL-0.3" value="10k">
<attribute name="PROD_ID" value="RES-9435"/>
</element>
<element name="DIODE13" library="SparkFun-DiscreteSemi" package="DIODE-1N4001" value=""/>
<element name="R15" library="SparkFun-Resistors" package="AXIAL-0.3" value="10k">
<attribute name="PROD_ID" value="RES-9435"/>
</element>
<element name="DIODE14" library="SparkFun-DiscreteSemi" package="DIODE-1N4001" value=""/>
<element name="R16" library="SparkFun-Resistors" package="AXIAL-0.3" value="10k">
<attribute name="PROD_ID" value="RES-9435"/>
</element>
<element name="DIODE15" library="SparkFun-DiscreteSemi" package="DIODE-1N4001" value=""/>
<element name="R17" library="SparkFun-Resistors" package="AXIAL-0.3" value="10k">
<attribute name="PROD_ID" value="RES-9435"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="POWER_JACK_PTH" value="POWER_JACKPTH">
<attribute name="PROD_ID" value="PRT-00119"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="CAP-PTH-LARGE" value=""/>
<element name="JP17" library="SparkFun-Connectors" package="1X02_2.54_SCREWTERM" value="M022.54MM_SCREWTERM"/>
<element name="JP1" library="SparkFun-Connectors" package="1X02_2.54_SCREWTERM" value="M022.54MM_SCREWTERM"/>
<element name="JP2" library="SparkFun-Connectors" package="1X02_2.54_SCREWTERM" value="M022.54MM_SCREWTERM"/>
<element name="JP3" library="SparkFun-Connectors" package="1X02_2.54_SCREWTERM" value="M022.54MM_SCREWTERM"/>
<element name="JP4" library="SparkFun-Connectors" package="1X02_2.54_SCREWTERM" value="M022.54MM_SCREWTERM"/>
<element name="JP5" library="SparkFun-Connectors" package="1X02_2.54_SCREWTERM" value="M022.54MM_SCREWTERM"/>
<element name="JP6" library="SparkFun-Connectors" package="1X02_2.54_SCREWTERM" value="M022.54MM_SCREWTERM"/>
<element name="JP7" library="SparkFun-Connectors" package="1X02_2.54_SCREWTERM" value="M022.54MM_SCREWTERM"/>
<element name="JP8" library="SparkFun-Connectors" package="1X02_2.54_SCREWTERM" value="M022.54MM_SCREWTERM"/>
<element name="JP9" library="SparkFun-Connectors" package="1X02_2.54_SCREWTERM" value="M022.54MM_SCREWTERM"/>
<element name="JP10" library="SparkFun-Connectors" package="1X02_2.54_SCREWTERM" value="M022.54MM_SCREWTERM"/>
<element name="JP11" library="SparkFun-Connectors" package="1X02_2.54_SCREWTERM" value="M022.54MM_SCREWTERM"/>
<element name="JP12" library="SparkFun-Connectors" package="1X02_2.54_SCREWTERM" value="M022.54MM_SCREWTERM"/>
<element name="JP13" library="SparkFun-Connectors" package="1X02_2.54_SCREWTERM" value="M022.54MM_SCREWTERM"/>
<element name="JP14" library="SparkFun-Connectors" package="1X02_2.54_SCREWTERM" value="M022.54MM_SCREWTERM"/>
<element name="JP15" library="SparkFun-Connectors" package="1X02_2.54_SCREWTERM" value="M022.54MM_SCREWTERM"/>
<element name="JP16" library="SparkFun-Connectors" package="1X08_PIN1_NO_SILK" value=""/>
<element name="JP18" library="SparkFun-Connectors" package="SCREWTERMINAL-5MM-2" value="M025MM">
<attribute name="STOREFRONT_ID" value="PRT-08432"/>
</element>
<element name="Q17" library="SparkFun-DiscreteSemi" package="TO220V" value="MOSFET-PCHANNELFQP27P06"/>
<element name="Q1" library="SparkFun-DiscreteSemi" package="TO220V" value="MOSFET-PCHANNELFQP27P06"/>
<element name="Q2" library="SparkFun-DiscreteSemi" package="TO220V" value="MOSFET-PCHANNELFQP27P06"/>
<element name="Q3" library="SparkFun-DiscreteSemi" package="TO220V" value="MOSFET-PCHANNELFQP27P06"/>
<element name="Q4" library="SparkFun-DiscreteSemi" package="TO220V" value="MOSFET-PCHANNELFQP27P06"/>
<element name="Q5" library="SparkFun-DiscreteSemi" package="TO220V" value="MOSFET-PCHANNELFQP27P06"/>
<element name="Q6" library="SparkFun-DiscreteSemi" package="TO220V" value="MOSFET-PCHANNELFQP27P06"/>
<element name="Q7" library="SparkFun-DiscreteSemi" package="TO220V" value="MOSFET-PCHANNELFQP27P06"/>
<element name="Q8" library="SparkFun-DiscreteSemi" package="TO220V" value="MOSFET-PCHANNELFQP27P06"/>
<element name="Q9" library="SparkFun-DiscreteSemi" package="TO220V" value="MOSFET-PCHANNELFQP27P06"/>
<element name="Q10" library="SparkFun-DiscreteSemi" package="TO220V" value="MOSFET-PCHANNELFQP27P06"/>
<element name="Q11" library="SparkFun-DiscreteSemi" package="TO220V" value="MOSFET-PCHANNELFQP27P06"/>
<element name="Q12" library="SparkFun-DiscreteSemi" package="TO220V" value="MOSFET-PCHANNELFQP27P06"/>
<element name="Q13" library="SparkFun-DiscreteSemi" package="TO220V" value="MOSFET-PCHANNELFQP27P06"/>
<element name="Q14" library="SparkFun-DiscreteSemi" package="TO220V" value="MOSFET-PCHANNELFQP27P06"/>
<element name="Q15" library="SparkFun-DiscreteSemi" package="TO220V" value="MOSFET-PCHANNELFQP27P06"/>
<element name="J2" library="SparkFun-Connectors" package="POWER_JACK_PTH" value="POWER_JACKPTH">
<attribute name="PROD_ID" value="PRT-00119"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="CAP-PTH-LARGE" value=""/>
<element name="JP19" library="SparkFun-Connectors" package="SCREWTERMINAL-5MM-2" value="M025MM">
<attribute name="STOREFRONT_ID" value="PRT-08432"/>
</element>
<element name="JP21" library="SparkFun-Connectors" package="1X02_LONGPADS" value="M02PTH3"/>
<element name="JP20" library="SparkFun-Connectors" package="1X08_PIN1_NO_SILK" value=""/>
</elements>
<signals>
<signal name="DRAIN0">
<contactref element="DIODE0" pad="C"/>
<contactref element="JP17" pad="P1"/>
<contactref element="Q17" pad="2"/>
</signal>
<signal name="GND">
<contactref element="C1" pad="2"/>
<contactref element="U1" pad="22"/>
<contactref element="U1" pad="27"/>
<contactref element="R4" pad="P$1"/>
<contactref element="J1" pad="GNDBREAK"/>
<contactref element="J1" pad="GND"/>
<contactref element="C2" pad="2"/>
<contactref element="JP18" pad="2"/>
<contactref element="DIODE0" pad="A"/>
<contactref element="JP17" pad="P2"/>
<contactref element="JP1" pad="P2"/>
<contactref element="DIODE1" pad="A"/>
<contactref element="DIODE2" pad="A"/>
<contactref element="JP2" pad="P2"/>
<contactref element="DIODE3" pad="A"/>
<contactref element="JP3" pad="P2"/>
<contactref element="JP4" pad="P2"/>
<contactref element="DIODE4" pad="A"/>
<contactref element="DIODE5" pad="A"/>
<contactref element="JP5" pad="P2"/>
<contactref element="DIODE6" pad="A"/>
<contactref element="JP6" pad="P2"/>
<contactref element="DIODE7" pad="A"/>
<contactref element="JP7" pad="P2"/>
<contactref element="DIODE8" pad="A"/>
<contactref element="JP8" pad="P2"/>
<contactref element="DIODE9" pad="A"/>
<contactref element="JP9" pad="P2"/>
<contactref element="JP10" pad="P2"/>
<contactref element="DIODE10" pad="A"/>
<contactref element="DIODE11" pad="A"/>
<contactref element="JP11" pad="P2"/>
<contactref element="JP12" pad="P2"/>
<contactref element="DIODE12" pad="A"/>
<contactref element="DIODE13" pad="A"/>
<contactref element="JP13" pad="P2"/>
<contactref element="DIODE14" pad="A"/>
<contactref element="JP14" pad="P2"/>
<contactref element="J2" pad="GNDBREAK"/>
<contactref element="J2" pad="GND"/>
<contactref element="C3" pad="2"/>
<contactref element="JP19" pad="2"/>
<contactref element="JP15" pad="P2"/>
<contactref element="DIODE15" pad="A"/>
<contactref element="JP20" pad="4"/>
<contactref element="JP16" pad="4"/>
</signal>
<signal name="N$2">
<contactref element="U1" pad="20"/>
<contactref element="R4" pad="P$2"/>
</signal>
<signal name="VCC">
<contactref element="U1" pad="21"/>
<contactref element="C1" pad="1"/>
<contactref element="R3" pad="P$1"/>
<contactref element="U1" pad="19"/>
<contactref element="JP20" pad="3"/>
<contactref element="JP16" pad="3"/>
</signal>
<signal name="O1">
<contactref element="U1" pad="1"/>
<contactref element="R1" pad="P$1"/>
<contactref element="Q1" pad="1"/>
</signal>
<signal name="O0">
<contactref element="U1" pad="28"/>
<contactref element="Q17" pad="1"/>
<contactref element="R0" pad="P$1"/>
</signal>
<signal name="O2">
<contactref element="U1" pad="2"/>
<contactref element="R2" pad="P$1"/>
<contactref element="Q2" pad="1"/>
</signal>
<signal name="O3">
<contactref element="U1" pad="3"/>
<contactref element="R5" pad="P$1"/>
<contactref element="Q3" pad="1"/>
</signal>
<signal name="O4">
<contactref element="U1" pad="4"/>
<contactref element="R6" pad="P$1"/>
<contactref element="Q4" pad="1"/>
</signal>
<signal name="O5">
<contactref element="U1" pad="5"/>
<contactref element="R7" pad="P$1"/>
<contactref element="Q5" pad="1"/>
</signal>
<signal name="O6">
<contactref element="U1" pad="6"/>
<contactref element="R8" pad="P$1"/>
<contactref element="Q6" pad="1"/>
</signal>
<signal name="O7">
<contactref element="U1" pad="7"/>
<contactref element="R9" pad="P$1"/>
<contactref element="Q7" pad="1"/>
</signal>
<signal name="O8">
<contactref element="U1" pad="8"/>
<contactref element="R10" pad="P$1"/>
<contactref element="Q8" pad="1"/>
</signal>
<signal name="O9">
<contactref element="U1" pad="9"/>
<contactref element="R11" pad="P$1"/>
<contactref element="Q9" pad="1"/>
</signal>
<signal name="O10">
<contactref element="U1" pad="10"/>
<contactref element="R12" pad="P$1"/>
<contactref element="Q10" pad="1"/>
</signal>
<signal name="O11">
<contactref element="U1" pad="11"/>
<contactref element="R13" pad="P$1"/>
<contactref element="Q11" pad="1"/>
</signal>
<signal name="O12">
<contactref element="U1" pad="12"/>
<contactref element="R14" pad="P$1"/>
<contactref element="Q12" pad="1"/>
</signal>
<signal name="O13">
<contactref element="U1" pad="13"/>
<contactref element="R15" pad="P$1"/>
<contactref element="Q13" pad="1"/>
</signal>
<signal name="O14">
<contactref element="U1" pad="14"/>
<contactref element="R16" pad="P$1"/>
<contactref element="Q14" pad="1"/>
</signal>
<signal name="O15">
<contactref element="U1" pad="15"/>
<contactref element="R17" pad="P$1"/>
<contactref element="Q15" pad="1"/>
</signal>
<signal name="DRAIN1">
<contactref element="JP1" pad="P1"/>
<contactref element="DIODE1" pad="C"/>
<contactref element="Q1" pad="2"/>
</signal>
<signal name="DRAIN2">
<contactref element="JP2" pad="P1"/>
<contactref element="DIODE2" pad="C"/>
<contactref element="Q2" pad="2"/>
</signal>
<signal name="DRAIN3">
<contactref element="JP3" pad="P1"/>
<contactref element="DIODE3" pad="C"/>
<contactref element="Q3" pad="2"/>
</signal>
<signal name="DRAIN4">
<contactref element="JP4" pad="P1"/>
<contactref element="DIODE4" pad="C"/>
<contactref element="Q4" pad="2"/>
</signal>
<signal name="DRAIN6">
<contactref element="JP6" pad="P1"/>
<contactref element="DIODE6" pad="C"/>
<contactref element="Q6" pad="2"/>
</signal>
<signal name="DRAIN7">
<contactref element="JP7" pad="P1"/>
<contactref element="DIODE7" pad="C"/>
<contactref element="Q7" pad="2"/>
</signal>
<signal name="DRAIN8">
<contactref element="JP8" pad="P1"/>
<contactref element="DIODE8" pad="C"/>
<contactref element="Q8" pad="2"/>
</signal>
<signal name="DRAIN9">
<contactref element="JP9" pad="P1"/>
<contactref element="DIODE9" pad="C"/>
<contactref element="Q9" pad="2"/>
</signal>
<signal name="DRAIN10">
<contactref element="JP10" pad="P1"/>
<contactref element="DIODE10" pad="C"/>
<contactref element="Q10" pad="2"/>
</signal>
<signal name="DRAIN11">
<contactref element="JP11" pad="P1"/>
<contactref element="DIODE11" pad="C"/>
<contactref element="Q11" pad="2"/>
</signal>
<signal name="DRAIN12">
<contactref element="JP12" pad="P1"/>
<contactref element="DIODE12" pad="C"/>
<contactref element="Q12" pad="2"/>
</signal>
<signal name="DRAIN13">
<contactref element="DIODE13" pad="C"/>
<contactref element="JP13" pad="P1"/>
<contactref element="Q13" pad="2"/>
</signal>
<signal name="DRAIN14">
<contactref element="JP14" pad="P1"/>
<contactref element="DIODE14" pad="C"/>
<contactref element="Q14" pad="2"/>
</signal>
<signal name="DRAIN15">
<contactref element="JP15" pad="P1"/>
<contactref element="DIODE15" pad="C"/>
<contactref element="Q15" pad="2"/>
</signal>
<signal name="SIN">
<contactref element="U1" pad="26"/>
<contactref element="JP20" pad="8"/>
<contactref element="JP16" pad="8"/>
</signal>
<signal name="SCLK">
<contactref element="U1" pad="25"/>
<contactref element="JP16" pad="7"/>
<contactref element="JP20" pad="7"/>
</signal>
<signal name="XLAT">
<contactref element="U1" pad="24"/>
<contactref element="JP16" pad="6"/>
<contactref element="JP20" pad="6"/>
</signal>
<signal name="BLANK">
<contactref element="U1" pad="23"/>
<contactref element="R3" pad="P$2"/>
<contactref element="JP20" pad="5"/>
<contactref element="JP16" pad="5"/>
</signal>
<signal name="GSCLK">
<contactref element="U1" pad="18"/>
<contactref element="JP20" pad="2"/>
<contactref element="JP16" pad="2"/>
</signal>
<signal name="SOUT">
<contactref element="U1" pad="17"/>
<contactref element="JP16" pad="1"/>
<contactref element="JP20" pad="1"/>
</signal>
<signal name="DRAIN5">
<contactref element="JP5" pad="P1"/>
<contactref element="DIODE5" pad="C"/>
<contactref element="Q5" pad="2"/>
</signal>
<signal name="POWER2">
<contactref element="J2" pad="PWR"/>
<contactref element="C3" pad="1"/>
<contactref element="JP19" pad="1"/>
<contactref element="Q13" pad="3"/>
<contactref element="R16" pad="P$2"/>
<contactref element="Q14" pad="3"/>
<contactref element="R17" pad="P$2"/>
<contactref element="Q15" pad="3"/>
<contactref element="R10" pad="P$2"/>
<contactref element="Q8" pad="3"/>
<contactref element="R11" pad="P$2"/>
<contactref element="Q9" pad="3"/>
<contactref element="R12" pad="P$2"/>
<contactref element="Q10" pad="3"/>
<contactref element="R13" pad="P$2"/>
<contactref element="Q11" pad="3"/>
<contactref element="R14" pad="P$2"/>
<contactref element="Q12" pad="3"/>
<contactref element="R15" pad="P$2"/>
<contactref element="JP21" pad="1"/>
</signal>
<signal name="POWER1">
<contactref element="J1" pad="PWR"/>
<contactref element="C2" pad="1"/>
<contactref element="JP18" pad="1"/>
<contactref element="Q17" pad="3"/>
<contactref element="R0" pad="P$2"/>
<contactref element="R1" pad="P$2"/>
<contactref element="R2" pad="P$2"/>
<contactref element="R5" pad="P$2"/>
<contactref element="R6" pad="P$2"/>
<contactref element="R7" pad="P$2"/>
<contactref element="R8" pad="P$2"/>
<contactref element="R9" pad="P$2"/>
<contactref element="Q1" pad="3"/>
<contactref element="Q2" pad="3"/>
<contactref element="Q3" pad="3"/>
<contactref element="Q4" pad="3"/>
<contactref element="Q5" pad="3"/>
<contactref element="Q6" pad="3"/>
<contactref element="Q7" pad="3"/>
<contactref element="JP21" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
