<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.0">
<drawing>
<board>
<plain>
<circle x="17.78" y="17.78" radius="14.986" width="0.254" layer="20"/>
<text>1</text>
<text>2</text>
<text>3</text>
<text>6</text>
<text>5</text>
<text>4</text>
<text>VDD</text>
<text>6</text>
<text>5</text>
<text>4</text>
<text>1</text>
<text>2</text>
<text>GND</text>
</plain>
<libraries>
<library name="saberlib">
<packages>
<package name="0603">
</package>
<package name="Q5B">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X4">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R2" library="saberlib" package="0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="saberlib" package="0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IN" library="SparkFun-Connectors" package="2X4" value="M04X2">
<attribute name="NAME"/>
</element>
<element name="OUT" library="SparkFun-Connectors" package="2X4" value="M04X2">
<attribute name="NAME"/>
</element>
<element name="R3" library="saberlib" package="0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="saberlib" package="0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="saberlib" package="0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="saberlib" package="0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="saberlib" package="0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="saberlib" package="0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="saberlib" package="0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="saberlib" package="0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="saberlib" package="0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="saberlib" package="0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="saberlib" package="Q5B" value="CSD18509Q5B">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="saberlib" package="Q5B" value="CSD18509Q5B">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q3" library="saberlib" package="Q5B" value="CSD18509Q5B">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q4" library="saberlib" package="Q5B" value="CSD18509Q5B">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q5" library="saberlib" package="Q5B" value="CSD18509Q5B">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q6" library="saberlib" package="Q5B" value="CSD18509Q5B">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$2">
<contactref element="R2" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="Q1" pad="P$4"/>
</signal>
<signal name="GND">
<contactref element="R2" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="R7" pad="1"/>
<contactref element="R9" pad="1"/>
<contactref element="R11" pad="1"/>
<contactref element="IN" pad="8"/>
<contactref element="OUT" pad="7"/>
<contactref element="Q1" pad="P$2"/>
<contactref element="Q1" pad="P$3"/>
<contactref element="Q1" pad="P$1"/>
<contactref element="Q2" pad="P$2"/>
<contactref element="Q2" pad="P$3"/>
<contactref element="Q2" pad="P$1"/>
<contactref element="Q3" pad="P$2"/>
<contactref element="Q3" pad="P$3"/>
<contactref element="Q3" pad="P$1"/>
<contactref element="Q4" pad="P$2"/>
<contactref element="Q4" pad="P$3"/>
<contactref element="Q4" pad="P$1"/>
<contactref element="Q5" pad="P$2"/>
<contactref element="Q5" pad="P$3"/>
<contactref element="Q5" pad="P$1"/>
<contactref element="Q6" pad="P$2"/>
<contactref element="Q6" pad="P$3"/>
<contactref element="Q6" pad="P$1"/>
</signal>
<signal name="IN1">
<contactref element="R1" pad="2"/>
<contactref element="IN" pad="1"/>
</signal>
<signal name="OUT1">
<contactref element="OUT" pad="1"/>
<contactref element="Q1" pad="P$8"/>
<contactref element="Q1" pad="P$7"/>
<contactref element="Q1" pad="P$5"/>
<contactref element="Q1" pad="P$6"/>
<contactref element="Q1" pad="P$9"/>
</signal>
<signal name="IN2">
<contactref element="IN" pad="3"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="IN3">
<contactref element="IN" pad="5"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="IN6">
<contactref element="IN" pad="2"/>
<contactref element="R12" pad="2"/>
</signal>
<signal name="IN5">
<contactref element="IN" pad="4"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="IN4">
<contactref element="IN" pad="6"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="OUT2">
<contactref element="OUT" pad="3"/>
<contactref element="Q2" pad="P$8"/>
<contactref element="Q2" pad="P$7"/>
<contactref element="Q2" pad="P$5"/>
<contactref element="Q2" pad="P$6"/>
<contactref element="Q2" pad="P$9"/>
</signal>
<signal name="OUT3">
<contactref element="OUT" pad="5"/>
<contactref element="Q3" pad="P$8"/>
<contactref element="Q3" pad="P$7"/>
<contactref element="Q3" pad="P$5"/>
<contactref element="Q3" pad="P$6"/>
<contactref element="Q3" pad="P$9"/>
</signal>
<signal name="OUT4">
<contactref element="OUT" pad="6"/>
<contactref element="Q4" pad="P$8"/>
<contactref element="Q4" pad="P$7"/>
<contactref element="Q4" pad="P$5"/>
<contactref element="Q4" pad="P$6"/>
<contactref element="Q4" pad="P$9"/>
</signal>
<signal name="OUT5">
<contactref element="OUT" pad="4"/>
<contactref element="Q5" pad="P$8"/>
<contactref element="Q5" pad="P$7"/>
<contactref element="Q5" pad="P$5"/>
<contactref element="Q5" pad="P$6"/>
<contactref element="Q5" pad="P$9"/>
</signal>
<signal name="OUT6">
<contactref element="OUT" pad="2"/>
<contactref element="Q6" pad="P$8"/>
<contactref element="Q6" pad="P$7"/>
<contactref element="Q6" pad="P$5"/>
<contactref element="Q6" pad="P$6"/>
<contactref element="Q6" pad="P$9"/>
</signal>
<signal name="VCC">
<contactref element="OUT" pad="8"/>
<contactref element="IN" pad="7"/>
</signal>
<signal name="N$1">
<contactref element="R3" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="Q2" pad="P$4"/>
</signal>
<signal name="N$3">
<contactref element="R5" pad="2"/>
<contactref element="R6" pad="1"/>
<contactref element="Q3" pad="P$4"/>
</signal>
<signal name="N$4">
<contactref element="R7" pad="2"/>
<contactref element="R8" pad="1"/>
<contactref element="Q4" pad="P$4"/>
</signal>
<signal name="N$5">
<contactref element="R9" pad="2"/>
<contactref element="R10" pad="1"/>
<contactref element="Q5" pad="P$4"/>
</signal>
<signal name="N$6">
<contactref element="R11" pad="2"/>
<contactref element="R12" pad="1"/>
<contactref element="Q6" pad="P$4"/>
</signal>
<signal name="N$7">
</signal>
</signals>
</board>
</drawing>
</eagle>
