<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="10.465" y2="0" width="0" layer="20"/>
<wire x1="10.465" y1="0" x2="10.465" y2="38.09" width="0" layer="20"/>
<wire x1="10.465" y1="38.09" x2="0" y2="38.09" width="0" layer="20"/>
<wire x1="0" y1="38.09" x2="0" y2="0" width="0" layer="20"/>
<text>AutoISP85 v1.0 µTh 2014</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X3">
</package>
</packages>
</library>
<library name="Atmel_By_element14_Batch_1-00">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 27/07/2012 14:02:49</description>
<packages>
<package name="DIP254P762X533-8">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="SparkFun-Connectors" package="2X3" value="MCU">
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="2X3" value="BOARD">
<attribute name="VALUE"/>
</element>
<element name="U1" library="Atmel_By_element14_Batch_1-00" package="DIP254P762X533-8" value="ATTINY85">
<attribute name="PACKAGE" value="PDIP-8"/>
<attribute name="OC_NEWARK" value="58M3796"/>
<attribute name="MPN" value="ATTINY85-20PU"/>
<attribute name="SUPPLIER" value="Atmel"/>
<attribute name="OC_FARNELL" value="1455162"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="Atmel_By_element14_Batch_1-00" package="DIP254P762X533-8" value="BOARD">
<attribute name="PACKAGE" value="PDIP-8"/>
<attribute name="OC_NEWARK" value="58M3796"/>
<attribute name="MPN" value="ATTINY85-20PU"/>
<attribute name="SUPPLIER" value="Atmel"/>
<attribute name="OC_FARNELL" value="1455162"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="U1" pad="1"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="N$2">
<contactref element="U1" pad="8"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="4"/>
<contactref element="J1" pad="6"/>
</signal>
<signal name="N$4">
<contactref element="J1" pad="4"/>
<contactref element="U1" pad="5"/>
</signal>
<signal name="N$5">
<contactref element="U1" pad="6"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="J1" pad="3"/>
<contactref element="U1" pad="7"/>
</signal>
<signal name="N$7">
<contactref element="U2" pad="1"/>
<contactref element="J2" pad="5"/>
</signal>
<signal name="N$8">
<contactref element="U2" pad="8"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="U2" pad="4"/>
<contactref element="J2" pad="6"/>
</signal>
<signal name="N$10">
<contactref element="J2" pad="4"/>
<contactref element="U2" pad="5"/>
</signal>
<signal name="N$11">
<contactref element="U2" pad="6"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="J2" pad="3"/>
<contactref element="U2" pad="7"/>
</signal>
<signal name="N$13">
<contactref element="U2" pad="2"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="U1" pad="3"/>
<contactref element="U2" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
