<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.3.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="86.03" y2="0" width="0" layer="20"/>
<wire x1="86.03" y1="0" x2="86.03" y2="27.93" width="0" layer="20"/>
<wire x1="86.03" y1="27.93" x2="0" y2="27.93" width="0" layer="20"/>
<wire x1="0" y1="27.93" x2="0" y2="0" width="0" layer="20"/>
<text>PWR</text>
<text>GND</text>
<text>1</text>
<text>1</text>
<text>RGB LED
Strip Driver</text>
<text>Shane
Kent '15</text>
</plain>
<libraries>
<library name="car_led_driver_lib">
<packages>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="TO220">
<description>&lt;b&gt;TO 220 horizontal&lt;/b&gt;</description>
</package>
<package name="HOLE">
</package>
<package name="SL_4PIN">
<description>4-Pin Molex SL Through-Hole Connector</description>
</package>
<package name="0207/10">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 10 mm</description>
</package>
<package name="SL_5PIN">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="." library="car_led_driver_lib" package="DIL08" value="ATTINY85"/>
<element name="BLUE" library="car_led_driver_lib" package="TO220" value="STP16"/>
<element name="GND" library="car_led_driver_lib" package="HOLE" value="HOLEA"/>
<element name="GREEN" library="car_led_driver_lib" package="TO220" value="STP16"/>
<element name="LEDSTRIP" library="car_led_driver_lib" package="SL_4PIN" value="SL_4PIN"/>
<element name="LM7805" library="car_led_driver_lib" package="TO220" value="LM7805A"/>
<element name="PWR" library="car_led_driver_lib" package="HOLE" value="HOLEA"/>
<element name="," library="car_led_driver_lib" package="0207/10" value="10K OHM"/>
<element name="RED" library="car_led_driver_lib" package="TO220" value="STP16"/>
<element name="POT" library="car_led_driver_lib" package="SL_5PIN" value="SL_5PINA"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="." pad="1"/>
<contactref element="," pad="1"/>
</signal>
<signal name="N$2">
<contactref element="," pad="2"/>
<contactref element="." pad="8"/>
<contactref element="LM7805" pad="3"/>
<contactref element="POT" pad="P$3"/>
</signal>
<signal name="N$4">
<contactref element="LM7805" pad="1"/>
<contactref element="LEDSTRIP" pad="P$4"/>
<contactref element="POT" pad="P$2"/>
</signal>
<signal name="N$3">
<contactref element="BLUE" pad="3"/>
<contactref element="RED" pad="3"/>
<contactref element="GREEN" pad="3"/>
<contactref element="GND" pad="P$1"/>
<contactref element="." pad="4"/>
<contactref element="LM7805" pad="2"/>
<contactref element="POT" pad="P$5"/>
</signal>
<signal name="N$6">
<contactref element="GREEN" pad="2"/>
<contactref element="LEDSTRIP" pad="P$3"/>
</signal>
<signal name="N$7">
<contactref element="RED" pad="2"/>
<contactref element="LEDSTRIP" pad="P$2"/>
</signal>
<signal name="N$8">
<contactref element="BLUE" pad="2"/>
<contactref element="LEDSTRIP" pad="P$1"/>
</signal>
<signal name="N$9">
<contactref element="RED" pad="1"/>
<contactref element="." pad="5"/>
</signal>
<signal name="N$10">
<contactref element="GREEN" pad="1"/>
<contactref element="." pad="6"/>
</signal>
<signal name="N$5">
<contactref element="BLUE" pad="1"/>
<contactref element="." pad="3"/>
</signal>
<signal name="N$11">
<contactref element="POT" pad="P$1"/>
<contactref element="PWR" pad="P$1"/>
</signal>
<signal name="N$12">
<contactref element="." pad="2"/>
<contactref element="POT" pad="P$4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
