<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<circle x="40.64" y="41.91" radius="43.18" width="0.4064" layer="20"/>
<text>reset</text>
<text>PwrLed</text>
<text>Help</text>
<text>Batt</text>
<text>ON</text>
<text>GND</text>
<text>3v</text>
<text>A5</text>
<text>5v</text>
<text>A6</text>
<text>gnd</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>-</text>
<text>-</text>
<text>+</text>
<text>+</text>
<text>-</text>
<text>+</text>
<text>-</text>
<text>20w led</text>
<text>20w led</text>
<text>GND</text>
<text>inner</text>
<text>Niccolo
 Casas</text>
<text>Anouk
 Wipprecht</text>
<text>Daniel Schatzmayr</text>
<text>Metal!</text>
<text>v0</text>
</plain>
<libraries>
<library name="matt-Teensy">
<packages>
<package name="TEENSY_3.0_BASIC">
</package>
</packages>
</library>
<library name="buckpuck">
<packages>
<package name="BUCKPUCK">
</package>
<package name="32VBOOST_WD">
</package>
<package name="NOUKLOGO3IN">
</package>
<package name="NOUKLOGO300MIL_COPPER">
</package>
</packages>
</library>
<library name="linear">
<description>&lt;b&gt;Linear Devices&lt;/b&gt;&lt;p&gt;
Operational amplifiers,  comparators, voltage regulators, ADCs, DACs, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO220V">
<description>&lt;b&gt;TO 200 vertical&lt;/b&gt;</description>
</package>
<package name="SOT223">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SCREWTERMINAL-3.5MM-2">
</package>
<package name="1X03_LONGPADS">
</package>
</packages>
</library>
<library name="SparkFun">
<packages>
<package name="AXIAL-0.3">
</package>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
<package name="LED5MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, round</description>
</package>
</packages>
</library>
<library name="LilyPad-Wearables">
<packages>
<package name="SIMPLE_HOLE">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0402-CAP">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="0603-CAP">
</package>
</packages>
</library>
<library name="Edison">
<packages>
<package name="DF40-XC-(X.X)-70DS-0.4V(51)">
</package>
</packages>
</library>
<library name="mpinnermaxstream">
<description>&lt;b&gt;MaxSream&lt;/b&gt; XBee Products&lt;p&gt;
http://www.maxstream.net</description>
<packages>
<package name="XBEE-PRO">
<description>&lt;b&gt;XBEE Pro&lt;/b&gt;&lt;p&gt;
Source: http://www.maxstream.net/products/xbee/datasheet_XBee_OEM_RF-Modules.pdf</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="TEENSY_3.0" library="matt-Teensy" package="TEENSY_3.0_BASIC" value="TEENSY_3.0_BASIC"/>
<element name="LED0" library="buckpuck" package="BUCKPUCK" value=""/>
<element name="5V_REG" library="linear" package="TO220V" value="7805TV">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="HPLED0" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-2" value="M023.5MM">
<attribute name="NAME"/>
</element>
<element name="BATTERY_PLUG" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-2" value="M023.5MM">
<attribute name="NAME"/>
</element>
<element name="XB1" library="mpinnermaxstream" package="XBEE-PRO" value="XBEE-PRO">
<attribute name="OC_NEWARK" value="42M2667"/>
<attribute name="MPN" value="XBP24-AWI-001"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1337916"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun" package="AXIAL-0.3" value="470"/>
<element name="Q2" library="SparkFun" package="SOT23" value="2N3904">
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun" package="AXIAL-0.3" value="220"/>
<element name="H1" library="LilyPad-Wearables" package="SIMPLE_HOLE" value="SEW_HOLE"/>
<element name="GND" library="LilyPad-Wearables" package="SIMPLE_HOLE" value="SEW_HOLE"/>
<element name="H3" library="LilyPad-Wearables" package="SIMPLE_HOLE" value="SEW_HOLE"/>
<element name="H4" library="LilyPad-Wearables" package="SIMPLE_HOLE" value="SEW_HOLE"/>
<element name="LED1" library="buckpuck" package="BUCKPUCK" value=""/>
<element name="HPL1" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-2" value="M023.5MM">
<attribute name="NAME"/>
</element>
<element name="R4" library="SparkFun" package="AXIAL-0.3" value="470"/>
<element name="Q1" library="SparkFun" package="SOT23" value="2N3904">
<attribute name="VALUE"/>
</element>
<element name="PWR_LED" library="SparkFun" package="LED5MM" value="">
<attribute name="VALUE"/>
</element>
<element name="R6" library="SparkFun" package="AXIAL-0.3" value="220"/>
<element name="POWER_SWITCH" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-2" value="M023.5MM">
<attribute name="NAME"/>
</element>
<element name="R5" library="SparkFun" package="AXIAL-0.3" value="220"/>
<element name="R3" library="SparkFun" package="AXIAL-0.3" value="220"/>
<element name="POWER_LED" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-2" value="M023.5MM">
<attribute name="NAME"/>
</element>
<element name="U$1" library="buckpuck" package="32VBOOST_WD" value="32VBOOSTWIDE"/>
<element name="3VREG" library="linear" package="SOT223" value="MCP1703DB">
<attribute name="NAME"/>
</element>
<element name="RESET" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-2" value="M023.5MM">
<attribute name="NAME"/>
</element>
<element name="HELP_BTN" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-2" value="M023.5MM">
<attribute name="NAME"/>
</element>
<element name="H5" library="LilyPad-Wearables" package="SIMPLE_HOLE" value="SEW_HOLE"/>
<element name="H6" library="LilyPad-Wearables" package="SIMPLE_HOLE" value="SEW_HOLE"/>
<element name="5V_A6" library="SparkFun-Connectors" package="1X03_LONGPADS" value="">
<attribute name="VALUE"/>
</element>
<element name="GND_3V_A5" library="SparkFun-Connectors" package="1X03_LONGPADS" value="">
<attribute name="VALUE"/>
</element>
<element name="U$2" library="buckpuck" package="NOUKLOGO3IN" value=""/>
<element name="U$3" library="buckpuck" package="NOUKLOGO300MIL_COPPER" value=""/>
<element name="C1" library="SparkFun-Capacitors" package="0402-CAP" value="0.1uF">
<attribute name="PROD_ID" value="CAP-00810"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0603-CAP" value="4.7uF">
<attribute name="PROD_ID" value="CAP-08280"/>
</element>
<element name="U1" library="Edison" package="DF40-XC-(X.X)-70DS-0.4V(51)" value="EDISON_CONNECTOR_FULLSOCKET"/>
</elements>
<signals>
<signal name="AGND">
<contactref element="TEENSY_3.0" pad="AGND"/>
</signal>
<signal name="VBAT">
<contactref element="TEENSY_3.0" pad="VBAT"/>
</signal>
<signal name="GND">
<contactref element="LED0" pad="P$6"/>
<contactref element="TEENSY_3.0" pad="GND"/>
<contactref element="TEENSY_3.0" pad="GND1"/>
<contactref element="5V_REG" pad="2"/>
<contactref element="XB1" pad="10"/>
<contactref element="Q2" pad="2"/>
<contactref element="GND" pad="P$1"/>
<contactref element="H3" pad="P$1"/>
<contactref element="H4" pad="P$1"/>
<contactref element="H1" pad="P$1"/>
<contactref element="LED1" pad="P$6"/>
<contactref element="Q1" pad="2"/>
<contactref element="PWR_LED" pad="K"/>
<contactref element="LED1" pad="P$2"/>
<contactref element="HPL1" pad="1"/>
<contactref element="LED0" pad="P$2"/>
<contactref element="HPLED0" pad="1"/>
<contactref element="U$1" pad="P$4"/>
<contactref element="U$1" pad="P$1"/>
<contactref element="BATTERY_PLUG" pad="1"/>
<contactref element="3VREG" pad="2"/>
<contactref element="RESET" pad="1"/>
<contactref element="HELP_BTN" pad="1"/>
<contactref element="H5" pad="P$1"/>
<contactref element="H6" pad="P$1"/>
<contactref element="5V_A6" pad="1"/>
<contactref element="GND_3V_A5" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="POWER_LED" pad="1"/>
<contactref element="U1" pad="1"/>
<contactref element="U1" pad="5"/>
<contactref element="U1" pad="9"/>
<contactref element="U1" pad="11"/>
<contactref element="U1" pad="13"/>
<contactref element="U1" pad="15"/>
</signal>
<signal name="32VDC">
<contactref element="LED0" pad="P$5"/>
<contactref element="LED1" pad="P$5"/>
<contactref element="U$1" pad="P$3"/>
</signal>
<signal name="5VDC">
<contactref element="TEENSY_3.0" pad="VIN"/>
<contactref element="5V_REG" pad="3"/>
<contactref element="R2" pad="P$1"/>
<contactref element="R5" pad="P$1"/>
<contactref element="R6" pad="P$2"/>
<contactref element="R3" pad="P$2"/>
<contactref element="3VREG" pad="1"/>
<contactref element="5V_A6" pad="2"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="LED0" pad="P$1"/>
<contactref element="HPLED0" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="TEENSY_3.0" pad="10"/>
<contactref element="XB1" pad="3"/>
</signal>
<signal name="N$9">
<contactref element="XB1" pad="2"/>
<contactref element="TEENSY_3.0" pad="9"/>
</signal>
<signal name="LEDCTR1">
<contactref element="R4" pad="P$2"/>
<contactref element="TEENSY_3.0" pad="23/A9"/>
<contactref element="U1" pad="33"/>
</signal>
<signal name="N$1">
<contactref element="R1" pad="P$1"/>
<contactref element="Q2" pad="1"/>
</signal>
<signal name="LEDCTR0">
<contactref element="R1" pad="P$2"/>
<contactref element="TEENSY_3.0" pad="22/A8"/>
<contactref element="U1" pad="35"/>
</signal>
<signal name="N$5">
<contactref element="LED1" pad="P$1"/>
<contactref element="HPL1" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="R4" pad="P$1"/>
<contactref element="Q1" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="LED1" pad="P$3"/>
<contactref element="R5" pad="P$2"/>
<contactref element="Q1" pad="3"/>
</signal>
<signal name="N$15">
<contactref element="R6" pad="P$1"/>
<contactref element="PWR_LED" pad="A"/>
</signal>
<signal name="11.1VDC">
<contactref element="5V_REG" pad="1"/>
<contactref element="POWER_SWITCH" pad="2"/>
<contactref element="U$1" pad="P$2"/>
</signal>
<signal name="N$11">
<contactref element="LED0" pad="P$3"/>
<contactref element="R2" pad="P$2"/>
<contactref element="Q2" pad="3"/>
</signal>
<signal name="N$2">
<contactref element="R3" pad="P$1"/>
<contactref element="POWER_LED" pad="2"/>
</signal>
<signal name="11VDC_BATT">
<contactref element="BATTERY_PLUG" pad="2"/>
<contactref element="POWER_SWITCH" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="TEENSY_3.0" pad="PGM"/>
<contactref element="RESET" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="TEENSY_3.0" pad="19/A5"/>
<contactref element="GND_3V_A5" pad="3"/>
</signal>
<signal name="3.3VDC">
<contactref element="GND_3V_A5" pad="2"/>
<contactref element="XB1" pad="1"/>
<contactref element="3VREG" pad="3"/>
<contactref element="C1" pad="2"/>
<contactref element="U1" pad="6"/>
<contactref element="U1" pad="4"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="5V_A6" pad="3"/>
<contactref element="TEENSY_3.0" pad="20/A6"/>
</signal>
<signal name="T3.3">
<contactref element="TEENSY_3.0" pad="3.3V1"/>
<contactref element="TEENSY_3.0" pad="3.3V"/>
</signal>
<signal name="N$4">
<contactref element="HELP_BTN" pad="2"/>
<contactref element="TEENSY_3.0" pad="17/A3"/>
</signal>
<signal name="N$7">
<contactref element="U1" pad="37"/>
</signal>
<signal name="N$16">
<contactref element="U1" pad="39"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
