<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.0.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="25.4" y2="0" width="0" layer="20"/>
<wire x1="25.4" y1="0" x2="25.4" y2="12.7" width="0" layer="20"/>
<wire x1="25.4" y1="12.7" x2="0" y2="12.7" width="0" layer="20"/>
<wire x1="0" y1="12.7" x2="0" y2="0" width="0" layer="20"/>
<text>BLINKY0Z</text>
<text>GND</text>
<text>+12V</text>
<text>+</text>
<text>B</text>
<text>R</text>
<text>G</text>
</plain>
<libraries>
<library name="Microchip_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 30/07/2012 11:22:31</description>
<packages>
<package name="SOT95P300X145-3N">
</package>
</packages>
</library>
<library name="NXP_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 30/07/2012 14:27:46</description>
<packages>
<package name="SOT95P230X110-3N">
</package>
</packages>
</library>
<library name="Jeff - Discrete">
<packages>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="C0603K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 0603 reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 1608</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02">
</package>
<package name="1X04">
</package>
<package name="2X3-NS">
</package>
</packages>
</library>
<library name="Jeff - Parts">
<packages>
<package name="SOIC8">
<description>&lt;b&gt;Small Outline IC&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J_PHOTO" library="SparkFun-Connectors" package="1X02" value="M02PTH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J_POWER" library="SparkFun-Connectors" package="1X02" value="M02PTH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="Microchip_By_element14_Batch_1" package="SOT95P300X145-3N" value="MCP1703T-3302E/CB">
<attribute name="PACKAGE" value="SOT-3"/>
<attribute name="OC_NEWARK" value="40M0637"/>
<attribute name="MPN" value="MCP1703T-3302E/CB"/>
<attribute name="SUPPLIER" value="Microchip"/>
<attribute name="OC_FARNELL" value="1439518"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="NXP_By_element14_Batch_1" package="SOT95P230X110-3N" value="2N7002BK">
<attribute name="PACKAGE" value="SOT-23-3"/>
<attribute name="OC_NEWARK" value="28T0305"/>
<attribute name="MPN" value="2N7002BK"/>
<attribute name="SUPPLIER" value="NXP"/>
<attribute name="OC_FARNELL" value="1859847"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U3" library="NXP_By_element14_Batch_1" package="SOT95P230X110-3N" value="2N7002BK">
<attribute name="PACKAGE" value="SOT-23-3"/>
<attribute name="OC_NEWARK" value="28T0305"/>
<attribute name="MPN" value="2N7002BK"/>
<attribute name="SUPPLIER" value="NXP"/>
<attribute name="OC_FARNELL" value="1859847"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U4" library="NXP_By_element14_Batch_1" package="SOT95P230X110-3N" value="2N7002BK">
<attribute name="PACKAGE" value="SOT-23-3"/>
<attribute name="OC_NEWARK" value="28T0305"/>
<attribute name="MPN" value="2N7002BK"/>
<attribute name="SUPPLIER" value="NXP"/>
<attribute name="OC_FARNELL" value="1859847"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="Jeff - Discrete" package="R0603" value="49.9">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="Jeff - Discrete" package="R0603" value="49.9">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="Jeff - Discrete" package="R0603" value="49.9">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="Jeff - Discrete" package="R0603" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="Jeff - Discrete" package="R0603" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="Jeff - Discrete" package="R0603" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="Jeff - Discrete" package="C0603K" value="1-10uF Ceramic">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="Jeff - Discrete" package="C0603K" value="0.1uF Ceramic">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="Jeff - Discrete" package="R0603" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="Jeff - Parts" package="SOIC8" value="MSP430G2210">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J_PRGM" library="SparkFun-Connectors" package="2X3-NS" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="U3" pad="1"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="RED_CNTL">
<contactref element="R5" pad="2"/>
<contactref element="R2" pad="1"/>
<contactref element="U1" pad="4"/>
</signal>
<signal name="BLUE_CNTL">
<contactref element="R6" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="N$5">
<contactref element="R1" pad="2"/>
<contactref element="U4" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="R2" pad="2"/>
<contactref element="U2" pad="1"/>
</signal>
<signal name="GREEN">
<contactref element="JP2" pad="4"/>
<contactref element="U3" pad="3"/>
</signal>
<signal name="RED">
<contactref element="JP2" pad="3"/>
<contactref element="U2" pad="3"/>
</signal>
<signal name="BLUE">
<contactref element="JP2" pad="2"/>
<contactref element="U4" pad="3"/>
</signal>
<signal name="GND">
<contactref element="R6" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="U$1" pad="1"/>
<contactref element="J_POWER" pad="1"/>
<contactref element="C3" pad="2"/>
<contactref element="R7" pad="1"/>
<contactref element="U1" pad="8"/>
<contactref element="J_PRGM" pad="5"/>
<contactref element="U4" pad="2"/>
<contactref element="U2" pad="2"/>
<contactref element="U3" pad="2"/>
</signal>
<signal name="+3V3">
<contactref element="U$1" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="J_PHOTO" pad="2"/>
<contactref element="U1" pad="1"/>
<contactref element="J_PRGM" pad="2"/>
</signal>
<signal name="+12V">
<contactref element="U$1" pad="3"/>
<contactref element="C1" pad="1"/>
<contactref element="J_POWER" pad="2"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="GREEN_CNTL">
<contactref element="R3" pad="1"/>
<contactref element="R4" pad="2"/>
<contactref element="U1" pad="5"/>
</signal>
<signal name="PHOTOCELL_VOLTAGE">
<contactref element="J_PHOTO" pad="1"/>
<contactref element="R7" pad="2"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="U1" pad="7"/>
<contactref element="J_PRGM" pad="3"/>
</signal>
<signal name="N$3">
<contactref element="J_PRGM" pad="4"/>
<contactref element="U1" pad="6"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
