<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<board>
<plain>
<wire x1="6.35" y1="0" x2="6.35" y2="25.4" width="0" layer="20"/>
<wire x1="6.35" y1="25.4" x2="76.2" y2="25.4" width="0" layer="20"/>
<wire x1="76.2" y1="25.4" x2="76.2" y2="0" width="0" layer="20"/>
<wire x1="76.2" y1="0" x2="6.35" y2="0" width="0" layer="20"/>
<text>OSHW</text>
<text>ATtiny84 LED+EL</text>
<text>DigitalMisery.com</text>
<text>ISP</text>
<text>FTDI</text>
<text>RST</text>
<text>RX</text>
<text>TX</text>
<text>VCC</text>
<text>CTS</text>
<text>GND</text>
<text>A3</text>
<text>D1</text>
<text>D0</text>
<text>A0</text>
<text>VCC</text>
<text>GND</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>VOLTAGE</text>
<text>HIGH</text>
<text>HIGH</text>
<text>VOLTAGE</text>
</plain>
<libraries>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DIL14">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="AVRISP">
</package>
<package name="LED5MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, round</description>
</package>
</packages>
</library>
<library name="optocoupler">
<description>&lt;b&gt;Opto Couplers&lt;/b&gt;&lt;p&gt;
Siemens, Hewlett-Packard, Texas Instuments, Sharp, Motorola&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL06">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="my_triac">
<description>&lt;b&gt;Thyristors, Triacs, Trigger Diodes&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO220AB">
<description>&lt;B&gt;TO220 AB&lt;/B&gt;&lt;p&gt;
3-lead molded horzintal</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.4">
<description>1/4W Resistor, 0.4" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CAP-PTH-SMALL">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X06_LONGPADS">
</package>
<package name="SCREWTERMINAL-5MM-2">
</package>
</packages>
</library>
<library name="ohw-logo">
<packages>
<package name="OSHW_FILLX150_NOTEXT">
</package>
</packages>
</library>
<library name="jlpcb-144">
<description>Generated from &lt;b&gt;jlpcb-144.sch&lt;/b&gt;&lt;p&gt;
by exp-project-lbr.ulp</description>
<packages>
<package name="JEELABS_BATTCOM_20MM_PTH">
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TO-92">
<description>&lt;b&gt;TO 92&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="SparkFun-DigitalIC" package="DIL14" value="ATTINY84-20PU">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ISP1" library="adafruit" package="AVRISP" value="AVRISP-6"/>
<element name="U2" library="optocoupler" package="DIL06" value="MOC3043M">
<attribute name="OC_NEWARK" value="72K8900"/>
<attribute name="MPN" value="MOC3043-M"/>
<attribute name="MF" value="FAIRCHILD SEMICONDUCTOR"/>
<attribute name="OC_FARNELL" value="1021371"/>
<attribute name="NAME"/>
</element>
<element name="U3" library="my_triac" package="TO220AB" value="BTA06">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="1" library="adafruit" package="LED5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="2" library="adafruit" package="LED5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="3" library="adafruit" package="LED5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Passives" package="AXIAL-0.4" value="10k">
<attribute name="NAME"/>
</element>
<element name="R2" library="SparkFun-Passives" package="AXIAL-0.4" value="100">
<attribute name="NAME"/>
</element>
<element name="R3" library="SparkFun-Passives" package="AXIAL-0.4" value="100">
<attribute name="NAME"/>
</element>
<element name="R4" library="SparkFun-Passives" package="AXIAL-0.4" value="100">
<attribute name="NAME"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="CAP-PTH-SMALL" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="CAP-PTH-SMALL" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="SCREWTERMINAL-5MM-2" value="">
<attribute name="NAME"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="SCREWTERMINAL-5MM-2" value="">
<attribute name="NAME"/>
</element>
<element name="R5" library="SparkFun-Passives" package="AXIAL-0.4" value="180">
<attribute name="NAME"/>
</element>
<element name="R6" library="SparkFun-Passives" package="AXIAL-0.4" value="330">
<attribute name="NAME"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X06_LONGPADS" value="">
<attribute name="VALUE"/>
</element>
<element name="R7" library="SparkFun-Passives" package="AXIAL-0.4" value="330">
<attribute name="NAME"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="1X06_LONGPADS" value="">
<attribute name="VALUE"/>
</element>
<element name="BAT1" library="jlpcb-144" package="JEELABS_BATTCOM_20MM_PTH" value="3.0V"/>
<element name="Q1" library="SparkFun-DiscreteSemi" package="TO-92" value="MOSFET-NCHANNELPTH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="SparkFun-DiscreteSemi" package="TO-92" value="MOSFET-NCHANNELPTH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q3" library="SparkFun-DiscreteSemi" package="TO-92" value="MOSFET-NCHANNELPTH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="SparkFun-Passives" package="AXIAL-0.4" value="10k">
<attribute name="NAME"/>
</element>
<element name="R9" library="SparkFun-Passives" package="AXIAL-0.4" value="10k">
<attribute name="NAME"/>
</element>
<element name="R10" library="SparkFun-Passives" package="AXIAL-0.4" value="10k">
<attribute name="NAME"/>
</element>
<element name="U$1" library="ohw-logo" package="OSHW_FILLX150_NOTEXT" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="C1" pad="1"/>
<contactref element="U1" pad="14"/>
<contactref element="JP1" pad="5"/>
<contactref element="JP1" pad="6"/>
<contactref element="ISP1" pad="6"/>
<contactref element="BAT1" pad="2"/>
<contactref element="JP2" pad="6"/>
<contactref element="Q1" pad="3"/>
<contactref element="Q2" pad="3"/>
<contactref element="Q3" pad="3"/>
<contactref element="R8" pad="P$1"/>
<contactref element="R9" pad="P$1"/>
<contactref element="R10" pad="P$1"/>
</signal>
<signal name="VCC">
<contactref element="ISP1" pad="2"/>
<contactref element="U1" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="R1" pad="P$2"/>
<contactref element="JP1" pad="4"/>
<contactref element="R5" pad="P$2"/>
<contactref element="BAT1" pad="1"/>
<contactref element="JP2" pad="5"/>
<contactref element="R4" pad="P$1"/>
<contactref element="R3" pad="P$1"/>
<contactref element="R2" pad="P$1"/>
<contactref element="ISP1" pad="2"/>
</signal>
<signal name="RST">
<contactref element="U1" pad="4"/>
<contactref element="R1" pad="P$1"/>
<contactref element="C2" pad="1"/>
<contactref element="ISP1" pad="5"/>
</signal>
<signal name="D1">
<contactref element="U1" pad="3"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="D0">
<contactref element="U1" pad="2"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="D4/MOSI">
<contactref element="ISP1" pad="4"/>
<contactref element="U1" pad="7"/>
<contactref element="Q3" pad="2"/>
<contactref element="R10" pad="P$2"/>
</signal>
<signal name="D9/A1/TXO">
<contactref element="U1" pad="12"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="D8/A4/RXI">
<contactref element="U1" pad="11"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="D10/A0">
<contactref element="U1" pad="13"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="D7/A3">
<contactref element="U1" pad="10"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="D5/MISO">
<contactref element="U1" pad="8"/>
<contactref element="ISP1" pad="1"/>
<contactref element="U2" pad="2"/>
</signal>
<signal name="D6/SCK">
<contactref element="U1" pad="9"/>
<contactref element="ISP1" pad="3"/>
</signal>
<signal name="N$1">
<contactref element="JP1" pad="1"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="U2" pad="1"/>
<contactref element="R5" pad="P$1"/>
</signal>
<signal name="AC1">
<contactref element="U3" pad="2"/>
<contactref element="R6" pad="P$1"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="R6" pad="P$2"/>
<contactref element="U2" pad="6"/>
</signal>
<signal name="AC3">
<contactref element="U3" pad="1"/>
<contactref element="R7" pad="P$1"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="D2">
<contactref element="U1" pad="5"/>
<contactref element="Q1" pad="2"/>
<contactref element="R8" pad="P$2"/>
</signal>
<signal name="D3">
<contactref element="U1" pad="6"/>
<contactref element="Q2" pad="2"/>
<contactref element="R9" pad="P$2"/>
</signal>
<signal name="N$3">
<contactref element="1" pad="K"/>
<contactref element="Q1" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="2" pad="K"/>
<contactref element="Q2" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="3" pad="K"/>
<contactref element="Q3" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="R2" pad="P$2"/>
<contactref element="1" pad="A"/>
</signal>
<signal name="N$14">
<contactref element="R4" pad="P$2"/>
<contactref element="3" pad="A"/>
</signal>
<signal name="N$12">
<contactref element="R3" pad="P$2"/>
<contactref element="2" pad="A"/>
</signal>
<signal name="AC2">
<contactref element="J1" pad="2"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="R7" pad="P$2"/>
<contactref element="U3" pad="3"/>
<contactref element="U2" pad="4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
