<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="7.62" y1="29.21" x2="7.62" y2="0" width="0.4064" layer="20"/>
<wire x1="7.62" y1="0" x2="43.18" y2="0" width="0.4064" layer="20"/>
<wire x1="43.18" y1="0" x2="43.18" y2="29.21" width="0.4064" layer="20"/>
<wire x1="43.18" y1="29.21" x2="7.62" y2="29.21" width="0.4064" layer="20"/>
<text>getmicros</text>
<text>by IH</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="1X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="AVRISP">
</package>
<package name="0207/12">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 12 mm</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X05">
</package>
<package name="1X02">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CPOL-RADIAL-10UF-25V">
</package>
</packages>
</library>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DIP08">
<description>&lt;b&gt;Dual In Line&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="adafruit" package="1X03" value=""/>
<element name="JP2" library="adafruit" package="1X03" value=""/>
<element name="JP3" library="SparkFun-Connectors" package="1X05" value=""/>
<element name="JP4" library="SparkFun-Connectors" package="1X05" value=""/>
<element name="C1" library="SparkFun-Capacitors" package="CPOL-RADIAL-10UF-25V" value="10uF"/>
<element name="ISP1" library="adafruit" package="AVRISP" value="AVRISP-6"/>
<element name="U$2" library="SparkFun-DigitalIC" package="DIP08" value="ATTINY"/>
<element name="JP5" library="SparkFun-Connectors" package="1X02" value=""/>
<element name="R2" library="adafruit" package="0207/12" value="10k"/>
</elements>
<signals>
<signal name="N$3">
<contactref element="JP2" pad="1"/>
<contactref element="ISP1" pad="5"/>
<contactref element="U$2" pad="1"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="JP1" pad="3"/>
<contactref element="ISP1" pad="4"/>
<contactref element="U$2" pad="5"/>
</signal>
<signal name="N$2">
<contactref element="JP1" pad="2"/>
<contactref element="ISP1" pad="1"/>
<contactref element="U$2" pad="6"/>
</signal>
<signal name="N$4">
<contactref element="JP1" pad="1"/>
<contactref element="ISP1" pad="3"/>
<contactref element="U$2" pad="7"/>
</signal>
<signal name="N$5">
<contactref element="JP2" pad="2"/>
<contactref element="U$2" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="JP2" pad="3"/>
<contactref element="U$2" pad="3"/>
</signal>
<signal name="N$7">
<contactref element="JP4" pad="1"/>
<contactref element="JP4" pad="2"/>
<contactref element="JP4" pad="3"/>
<contactref element="JP4" pad="4"/>
<contactref element="JP4" pad="5"/>
<contactref element="C1" pad="2"/>
<contactref element="ISP1" pad="6"/>
<contactref element="U$2" pad="4"/>
<contactref element="JP5" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="JP3" pad="5"/>
<contactref element="JP3" pad="4"/>
<contactref element="JP3" pad="3"/>
<contactref element="JP3" pad="2"/>
<contactref element="JP3" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="ISP1" pad="2"/>
<contactref element="U$2" pad="8"/>
<contactref element="JP5" pad="1"/>
<contactref element="R2" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
