<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.0.0">
<drawing>
<board>
<plain>
<wire x1="0.0254" y1="6.8326" x2="0.0254" y2="0" width="0.2032" layer="20"/>
<wire x1="0.0254" y1="0" x2="24.7142" y2="-0.0254" width="0.2032" layer="20"/>
<wire x1="24.7142" y1="-0.0254" x2="24.7142" y2="6.8326" width="0.2032" layer="20"/>
<wire x1="24.7142" y1="6.8326" x2="0.0254" y2="6.8326" width="0.2032" layer="20"/>
<text>Valid combinations:</text>
<text>168V / 3.3V Reg / 8MHz</text>
<text>168 / 5V Reg / 16MHz</text>
<text>168 / 5V Reg / 20MHz</text>
<text>Mark back accordingly</text>
<text>+</text>
<text>+</text>
<text>Vin:3.5-20v - Vout=3.3V - I = 150mA</text>
<text>chip@mcclellands.org 8/1/14</text>
</plain>
<libraries>
<library name="SparkFun">
<packages>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
<package name="EIA3216">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02_LOCK">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="COUT" library="SparkFun" package="EIA3216" value="2.2uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MIC5205" library="SparkFun" package="SOT23-5" value="MIC5205">
<attribute name="NAME"/>
</element>
<element name="CIN" library="SparkFun" package="EIA3216" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="VIN" library="SparkFun-Connectors" package="1X02_LOCK" value="M02LOCK">
<attribute name="NAME"/>
</element>
<element name="CBYP" library="SparkFun-Capacitors" package="0805" value="470pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="VOUT" library="SparkFun-Connectors" package="1X02_LOCK" value="M02LOCK">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="COUT" pad="C"/>
<contactref element="MIC5205" pad="2"/>
<contactref element="CIN" pad="C"/>
<contactref element="VIN" pad="2"/>
<contactref element="CBYP" pad="2"/>
<contactref element="VOUT" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="MIC5205" pad="5"/>
<contactref element="COUT" pad="A"/>
<contactref element="VOUT" pad="1"/>
</signal>
<signal name="VIN">
<contactref element="VIN" pad="1"/>
<contactref element="MIC5205" pad="1"/>
<contactref element="MIC5205" pad="3"/>
<contactref element="CIN" pad="A"/>
</signal>
<signal name="N$8">
</signal>
<signal name="N$9">
</signal>
<signal name="N$10">
</signal>
<signal name="N$11">
</signal>
<signal name="N$12">
</signal>
<signal name="N$13">
</signal>
<signal name="N$1">
</signal>
<signal name="N$2">
<contactref element="MIC5205" pad="4"/>
<contactref element="CBYP" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
