<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="49.53" y2="0" width="0.254" layer="20"/>
<wire x1="49.53" y1="0" x2="49.53" y2="66.04" width="0.254" layer="20"/>
<wire x1="49.53" y1="66.04" x2="0" y2="66.04" width="0.254" layer="20"/>
<wire x1="0" y1="66.04" x2="0" y2="0" width="0.254" layer="20"/>
<text>330uF</text>
<text>v02</text>
<text>v02</text>
</plain>
<libraries>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CAP-PTH-SMALLEZ">
<description>This is the "EZ" version of the .1" spaced ceramic thru-hole cap.&lt;br&gt;
It has reduced top mask to make it harder to put the component on the wrong side of the board.</description>
</package>
<package name="AXIAL-5MM">
</package>
<package name="CPOL-RADIAL-100UF-25V">
</package>
<package name="AXIAL-0.6">
<description>1W Resistor, 0.6" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
<package name="AXIAL-0.4">
<description>1/4W Resistor, 0.4" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
<package name="AXIAL-0.3">
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DIODE-1N4148">
</package>
<package name="TO-92-AMMO">
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CREATIVE_COMMONS">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X3">
</package>
<package name="1X02">
</package>
<package name="1X03_PP_HOLES_ONLY">
</package>
</packages>
</library>
<library name="SparkFun-RF">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find things that send or receive RF- GPS, cellular modules, Bluetooth, WiFi, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="XBEE-SILK">
</package>
</packages>
</library>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DIL28-3">
<description>Standard 28-pin DIP package.&lt;br&gt;
IC needs to have legs bent before insertion.</description>
</package>
</packages>
</library>
<library name="SparkFun-PowerIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find drivers, regulators, and amplifiers.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TO220-ADJ">
</package>
<package name="DIP-08">
</package>
<package name="TO-92">
<description>&lt;b&gt;TO 92&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="RHT03_DHT-22_AM2302">
<description>&lt;h1&gt;RHT03 / DHT-22 / AM2302 library&lt;/h1&gt;
&lt;p&gt;
Library with devices (schematic symbol and packages) for the RHT03 / DHT-22 / AM2302 digital relative humidity and tempearture sensor.&lt;br /&gt;
Warning: Package does not include tKeepout areas so that the part may optionally be placed on a riser with components underneath.  Please keep the package outline and bent-pin space in mind.
&lt;/p&gt;</description>
<packages>
<package name="RHT03_DHT-22">
<description>&lt;h1&gt;RHT03 / DHT-22&lt;/h1&gt;
&lt;p&gt;
Package for the RHT03 / DHT-22 relative humidity and temperature sensor.
&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-FreqCtrl">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find crystals and oscillators and other things that go "tick".&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="HC49US">
<description>&lt;B&gt;CRYSTAL&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives-DK">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.4">
<description>1/4W Resistor, 0.4" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
</packages>
</library>
<library name="diode">
<description>&lt;b&gt;Diodes&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola : www.onsemi.com
&lt;li&gt;Fairchild : www.fairchildsemi.com
&lt;li&gt;Philips : www.semiconductors.com
&lt;li&gt;Vishay : www.vishay.de
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DO35-7">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 2 mm, horizontal, grid 7.62 mm</description>
</package>
<package name="DO41-10">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 2.54 mm, horizontal, grid 10.16 mm</description>
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="STAND-OFF">
<description>&lt;b&gt;Stand Off&lt;/b&gt;&lt;p&gt;
This is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components. SKU : PRT-00447</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Passives" package="AXIAL-5MM" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="SparkFun-Passives" package="AXIAL-5MM" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Passives" package="AXIAL-5MM" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="SparkFun-Passives" package="AXIAL-5MM" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="SparkFun-Passives" package="CPOL-RADIAL-100UF-25V" value="100uF"/>
<element name="C5" library="SparkFun-Passives" package="CPOL-RADIAL-100UF-25V" value="100uF"/>
<element name="C6" library="SparkFun-Passives" package="CPOL-RADIAL-100UF-25V" value="100uF"/>
<element name="C7" library="SparkFun-Passives" package="CPOL-RADIAL-100UF-25V" value="330uF"/>
<element name="C8" library="SparkFun-Passives" package="CAP-PTH-SMALLEZ" value="160pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="SparkFun-Passives" package="AXIAL-5MM" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="SparkFun-DiscreteSemi" package="DIODE-1N4148" value="1N5189">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FRAME1" library="SparkFun-Aesthetics" package="CREATIVE_COMMONS" value="DANIEL KURIN - SWIFTLET TECHNOLOGY">
<attribute name="VERSION" value="v02"/>
<attribute name="DESIGNER" value="DANIEL KURIN - SWIFTLET TECHNOLOGY LLC"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="2X3" value="AVR_SPI_PRG_6PTH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="1X02" value="M02PTH">
<attribute name="USE" value="Battery"/>
</element>
<element name="JP3" library="SparkFun-Connectors" package="1X03_PP_HOLES_ONLY" value="">
<attribute name="USE" value="LEDs"/>
</element>
<element name="JP4" library="SparkFun-Connectors" package="1X02" value="M02PTH">
<attribute name="USE" value="Solar Panel"/>
</element>
<element name="R1" library="SparkFun-Passives" package="AXIAL-0.4" value="180R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="SparkFun-Passives" package="AXIAL-0.3" value="150K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="SparkFun-Passives" package="AXIAL-0.3" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="SparkFun-Passives" package="AXIAL-0.3" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Passives" package="AXIAL-0.6" value="0R47">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Passives" package="AXIAL-0.3" value="11R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun-Passives" package="AXIAL-0.3" value="30K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="SparkFun-Passives" package="AXIAL-0.3" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="SparkFun-Passives" package="AXIAL-0.3" value="1M3">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="SparkFun-Passives" package="AXIAL-0.3" value="150K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="SparkFun-Passives" package="AXIAL-0.3" value="1M3">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U6" library="SparkFun-RF" package="XBEE-SILK" value="XBEE-2B2"/>
<element name="U1" library="SparkFun-DigitalIC" package="DIL28-3" value="ATMEGA328P_PDIP">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="SparkFun-PowerIC" package="TO220-ADJ" value="V_REG_317SINK"/>
<element name="U3" library="SparkFun-PowerIC" package="DIP-08" value="MC34063DIP">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="U4" library="RHT03_DHT-22_AM2302" package="RHT03_DHT-22" value="DHT-22">
<attribute name="PROD_ID" value="SEN-10167"/>
</element>
<element name="U5" library="SparkFun-PowerIC" package="TO-92" value="MCP1700-3302E/TO">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Y1" library="SparkFun-FreqCtrl" package="HC49US" value="ATS16B"/>
<element name="L1" library="SparkFun-Passives-DK" package="AXIAL-0.4" value="22uH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="diode" package="DO35-7" value="1N4148DO35-7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="diode" package="DO41-10" value="1N4004">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="SparkFun-DiscreteSemi" package="TO-92-AMMO" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="SparkFun-Electromechanical" package="STAND-OFF" value=""/>
<element name="U$2" library="SparkFun-Electromechanical" package="STAND-OFF" value=""/>
</elements>
<signals>
<signal name="$N32">
<contactref element="JP4" pad="1"/>
<contactref element="R6" pad="P$1"/>
<contactref element="C6" pad="2"/>
<contactref element="U3" pad="4"/>
<contactref element="U3" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="JP2" pad="2"/>
<contactref element="U5" pad="1"/>
<contactref element="C5" pad="2"/>
<contactref element="U1" pad="8"/>
<contactref element="U1" pad="22"/>
<contactref element="C1" pad="P$2"/>
<contactref element="R8" pad="P$1"/>
<contactref element="C9" pad="P$2"/>
<contactref element="R10" pad="P$1"/>
<contactref element="C10" pad="P$2"/>
<contactref element="C2" pad="P$2"/>
<contactref element="U4" pad="GND"/>
<contactref element="C4" pad="2"/>
<contactref element="C3" pad="P$2"/>
<contactref element="U6" pad="10"/>
<contactref element="JP1" pad="6"/>
<contactref element="JP3" pad="3"/>
</signal>
<signal name="N$1">
<contactref element="JP4" pad="2"/>
<contactref element="U2" pad="IN"/>
<contactref element="R7" pad="P$2"/>
</signal>
<signal name="BAT">
<contactref element="U3" pad="6"/>
<contactref element="C6" pad="1"/>
<contactref element="R2" pad="P$1"/>
<contactref element="JP2" pad="1"/>
<contactref element="U5" pad="2"/>
<contactref element="R9" pad="P$2"/>
<contactref element="D3" pad="C"/>
</signal>
<signal name="N$4">
<contactref element="R2" pad="P$2"/>
<contactref element="U3" pad="7"/>
<contactref element="R1" pad="P$1"/>
<contactref element="L1" pad="P$1"/>
</signal>
<signal name="N$5">
<contactref element="R1" pad="P$2"/>
<contactref element="U3" pad="8"/>
</signal>
<signal name="N$6">
<contactref element="D1" pad="A"/>
<contactref element="U3" pad="1"/>
<contactref element="L1" pad="P$2"/>
</signal>
<signal name="N$7">
<contactref element="U3" pad="5"/>
<contactref element="R6" pad="P$2"/>
<contactref element="R5" pad="P$1"/>
</signal>
<signal name="N$8">
<contactref element="U3" pad="3"/>
<contactref element="C8" pad="1"/>
</signal>
<signal name="3.3V">
<contactref element="U5" pad="3"/>
<contactref element="C5" pad="1"/>
<contactref element="U1" pad="20"/>
<contactref element="U1" pad="7"/>
<contactref element="R11" pad="P$1"/>
<contactref element="C1" pad="P$1"/>
<contactref element="C2" pad="P$1"/>
<contactref element="U4" pad="VDD"/>
<contactref element="C4" pad="1"/>
<contactref element="C3" pad="P$1"/>
<contactref element="U6" pad="1"/>
<contactref element="JP1" pad="2"/>
<contactref element="R12" pad="P$2"/>
</signal>
<signal name="N$3">
<contactref element="R11" pad="P$2"/>
<contactref element="U1" pad="1"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="N$9">
<contactref element="Y1" pad="2"/>
<contactref element="U1" pad="9"/>
</signal>
<signal name="N$10">
<contactref element="U1" pad="10"/>
<contactref element="Y1" pad="1"/>
</signal>
<signal name="SOLAR_AD">
<contactref element="R8" pad="P$2"/>
<contactref element="C9" pad="P$1"/>
<contactref element="U1" pad="24"/>
<contactref element="R7" pad="P$1"/>
</signal>
<signal name="BAT_AD">
<contactref element="R10" pad="P$2"/>
<contactref element="R9" pad="P$1"/>
<contactref element="C10" pad="P$1"/>
<contactref element="U1" pad="23"/>
</signal>
<signal name="5V">
<contactref element="D1" pad="C"/>
<contactref element="C7" pad="1"/>
<contactref element="R5" pad="P$2"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="DHT22">
<contactref element="U4" pad="DATA"/>
<contactref element="U1" pad="11"/>
</signal>
<signal name="N$11">
<contactref element="U1" pad="2"/>
<contactref element="U6" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="U1" pad="3"/>
<contactref element="U6" pad="3"/>
</signal>
<signal name="N$13">
<contactref element="U1" pad="18"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="U1" pad="19"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="N$15">
<contactref element="JP1" pad="4"/>
<contactref element="U1" pad="17"/>
</signal>
<signal name="LED_CTRL">
<contactref element="JP3" pad="2"/>
<contactref element="U1" pad="12"/>
</signal>
<signal name="XB_RESET">
<contactref element="U1" pad="4"/>
<contactref element="U6" pad="5"/>
<contactref element="R12" pad="P$1"/>
</signal>
<signal name="XB_SLEEP_RQ">
<contactref element="U6" pad="9"/>
<contactref element="U1" pad="5"/>
</signal>
<signal name="XB_ON">
<contactref element="U6" pad="13"/>
<contactref element="U1" pad="6"/>
</signal>
<signal name="N$2">
<contactref element="U2" pad="OUT"/>
<contactref element="D2" pad="A"/>
<contactref element="R3" pad="P$1"/>
</signal>
<signal name="N$23">
<contactref element="D2" pad="C"/>
<contactref element="Q1" pad="2"/>
</signal>
<signal name="N$56">
<contactref element="R3" pad="P$2"/>
<contactref element="D3" pad="A"/>
<contactref element="Q1" pad="3"/>
</signal>
<signal name="N$58">
<contactref element="Q1" pad="1"/>
<contactref element="U2" pad="ADJ"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
