<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="2" y1="-1" x2="47.24" y2="-1" width="0" layer="20"/>
<wire x1="47.24" y1="-1" x2="47.24" y2="12.5" width="0" layer="20"/>
<wire x1="47.24" y1="12.5" x2="2" y2="12.5" width="0" layer="20"/>
<wire x1="2" y1="12.5" x2="2" y2="-1" width="0" layer="20"/>
<text>+</text>
<text>-</text>
<text>ATM</text>
<text>+</text>
<text>-</text>
<text>VIN</text>
<text>FIRE BUTTON</text>
<text>TRIM</text>
</plain>
<libraries>
<library name="steve">
<packages>
<package name="NAOSRAPTOR">
</package>
<package name="SCREWBLOCK">
</package>
<package name="TO263">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
</package>
</packages>
</library>
<library name="diode">
<description>&lt;b&gt;Diodes&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola : www.onsemi.com
&lt;li&gt;Fairchild : www.fairchildsemi.com
&lt;li&gt;Philips : www.semiconductors.com
&lt;li&gt;Vishay : www.vishay.de
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23">
<description>&lt;B&gt;DIODE&lt;/B&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="NR" library="steve" package="NAOSRAPTOR" value="NAOSRAPTOR"/>
<element name="FIRE" library="steve" package="SCREWBLOCK" value="SCREWBLOCK"/>
<element name="ATM" library="steve" package="SCREWBLOCK" value="SCREWBLOCK"/>
<element name="VIN" library="steve" package="SCREWBLOCK" value="SCREWBLOCK"/>
<element name="TRIM" library="steve" package="SCREWBLOCK" value="SCREWBLOCK"/>
<element name="Q1" library="steve" package="TO263" value="FDD4685">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="1206" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="1206" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="diode" package="SOT23" value="5V6">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="steve" package="TO263" value="FDD4685">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="ATM" pad="P$2"/>
<contactref element="NR" pad="P10"/>
<contactref element="NR" pad="P3"/>
<contactref element="VIN" pad="P$2"/>
<contactref element="FIRE" pad="P$2"/>
<contactref element="Q2" pad="G"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="R1" pad="2"/>
<contactref element="Q2" pad="S"/>
<contactref element="Q1" pad="S"/>
</signal>
<signal name="ATM">
<contactref element="ATM" pad="P$1"/>
<contactref element="NR" pad="P1"/>
</signal>
<signal name="FIRE">
<contactref element="FIRE" pad="P$1"/>
<contactref element="R1" pad="1"/>
<contactref element="Q1" pad="G"/>
</signal>
<signal name="VIN">
<contactref element="VIN" pad="P$1"/>
<contactref element="Q2" pad="D"/>
</signal>
<signal name="ON">
<contactref element="NR" pad="P5"/>
<contactref element="D1" pad="1"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="TRIM+">
<contactref element="NR" pad="P2"/>
<contactref element="TRIM" pad="P$2"/>
</signal>
<signal name="TRIM-">
<contactref element="NR" pad="P9"/>
<contactref element="TRIM" pad="P$1"/>
</signal>
<signal name="PWR">
<contactref element="Q1" pad="D"/>
<contactref element="NR" pad="P6"/>
<contactref element="D1" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
