<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="31.674" y2="0" width="0" layer="20"/>
<wire x1="31.674" y1="0" x2="31.674" y2="63.49" width="0" layer="20"/>
<wire x1="31.674" y1="63.49" x2="0" y2="63.49" width="0" layer="20"/>
<wire x1="0" y1="63.49" x2="0" y2="0" width="0" layer="20"/>
<text>VCC</text>
<text>GND</text>
<text>X-</text>
<text>X+</text>
<text>FMARK</text>
<text>RS</text>
<text>NRD</text>
<text>SDO</text>
<text>D0</text>
<text>D2</text>
<text>D4</text>
<text>D6</text>
<text>D8</text>
<text>D10</text>
<text>D12</text>
<text>D14</text>
<text>D16</text>
<text>NRST</text>
<text>IM2</text>
<text>IM0</text>
<text>LEDK</text>
<text>LEDA</text>
<text>IM1</text>
<text>IM3</text>
<text>D17</text>
<text>D15</text>
<text>D13</text>
<text>D11</text>
<text>D9</text>
<text>D7</text>
<text>D5</text>
<text>D3</text>
<text>D1</text>
<text>SDI</text>
<text>NWR
SCL</text>
<text>NCS</text>
<text>Y+</text>
<text>Y-</text>
<text>TFTProtoBreakout
Rev1
F. Lee
12/29/14</text>
<text>H</text>
<text>H</text>
<text>H</text>
<text>H</text>
<text>L</text>
<text>L</text>
<text>L</text>
<text>L</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X20">
</package>
<package name="1X16">
</package>
<package name="1X02">
</package>
<package name="1X03">
</package>
<package name="1X09">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-RES">
</package>
</packages>
</library>
<library name="freddyLibr">
<packages>
<package name="PCM12SMTR">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="SparkFun-Connectors" package="1X20" value="M20"/>
<element name="JP2" library="SparkFun-Connectors" package="1X20" value="M20"/>
<element name="JP3" library="SparkFun-Connectors" package="1X16" value="M16PTH"/>
<element name="JP4" library="SparkFun-Connectors" package="1X02" value="M02PTH"/>
<element name="JP5" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="VALUE"/>
</element>
<element name="JP6" library="SparkFun-Connectors" package="1X09" value="M09"/>
<element name="R1" library="SparkFun-Resistors" package="0603-RES" value="1K">
<attribute name="PROD_ID" value="RES-07856"/>
<attribute name="NAME"/>
</element>
<element name="SW1" library="freddyLibr" package="PCM12SMTR" value="PCM12SMTR">
<attribute name="NAME"/>
</element>
<element name="SW2" library="freddyLibr" package="PCM12SMTR" value="PCM12SMTR">
<attribute name="NAME"/>
</element>
<element name="SW3" library="freddyLibr" package="PCM12SMTR" value="PCM12SMTR">
<attribute name="NAME"/>
</element>
<element name="SW4" library="freddyLibr" package="PCM12SMTR" value="PCM12SMTR">
<attribute name="NAME"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP7" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="X-">
<contactref element="JP1" pad="19"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="X+">
<contactref element="JP1" pad="18"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="FMARK">
<contactref element="JP3" pad="3"/>
<contactref element="JP1" pad="17"/>
</signal>
<signal name="RS">
<contactref element="JP1" pad="16"/>
<contactref element="JP3" pad="4"/>
</signal>
<signal name="NRD">
<contactref element="JP3" pad="5"/>
<contactref element="JP1" pad="15"/>
</signal>
<signal name="SDO">
<contactref element="JP1" pad="14"/>
<contactref element="JP3" pad="6"/>
</signal>
<signal name="D0">
<contactref element="JP3" pad="7"/>
<contactref element="JP1" pad="13"/>
</signal>
<signal name="D2">
<contactref element="JP1" pad="12"/>
<contactref element="JP3" pad="8"/>
</signal>
<signal name="D4">
<contactref element="JP3" pad="9"/>
<contactref element="JP1" pad="11"/>
</signal>
<signal name="D6">
<contactref element="JP3" pad="10"/>
<contactref element="JP1" pad="10"/>
</signal>
<signal name="D8">
<contactref element="JP3" pad="11"/>
<contactref element="JP1" pad="9"/>
</signal>
<signal name="D10">
<contactref element="JP3" pad="12"/>
<contactref element="JP1" pad="8"/>
</signal>
<signal name="D12">
<contactref element="JP1" pad="7"/>
<contactref element="JP3" pad="13"/>
</signal>
<signal name="D14">
<contactref element="JP3" pad="14"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="D16">
<contactref element="JP1" pad="5"/>
<contactref element="JP3" pad="15"/>
</signal>
<signal name="NRST">
<contactref element="JP3" pad="16"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="Y-">
<contactref element="JP2" pad="19"/>
<contactref element="JP4" pad="1"/>
</signal>
<signal name="Y+">
<contactref element="JP2" pad="18"/>
<contactref element="JP4" pad="2"/>
</signal>
<signal name="NCS">
<contactref element="JP5" pad="1"/>
<contactref element="JP2" pad="16"/>
</signal>
<signal name="NWR_SCL">
<contactref element="JP5" pad="2"/>
<contactref element="JP2" pad="15"/>
</signal>
<signal name="SDI">
<contactref element="JP5" pad="3"/>
<contactref element="JP2" pad="14"/>
</signal>
<signal name="D1">
<contactref element="JP6" pad="1"/>
<contactref element="JP2" pad="12"/>
</signal>
<signal name="D3">
<contactref element="JP6" pad="2"/>
<contactref element="JP2" pad="11"/>
</signal>
<signal name="D5">
<contactref element="JP2" pad="10"/>
<contactref element="JP6" pad="3"/>
</signal>
<signal name="D7">
<contactref element="JP6" pad="4"/>
<contactref element="JP2" pad="9"/>
</signal>
<signal name="D9">
<contactref element="JP2" pad="8"/>
<contactref element="JP6" pad="5"/>
</signal>
<signal name="D11">
<contactref element="JP6" pad="6"/>
<contactref element="JP2" pad="7"/>
</signal>
<signal name="D13">
<contactref element="JP2" pad="6"/>
<contactref element="JP6" pad="7"/>
</signal>
<signal name="IM3">
<contactref element="JP2" pad="3"/>
<contactref element="SW4" pad="2"/>
</signal>
<signal name="GND">
<contactref element="JP2" pad="20"/>
<contactref element="JP2" pad="17"/>
<contactref element="JP2" pad="13"/>
<contactref element="R1" pad="2"/>
<contactref element="SW1" pad="1"/>
<contactref element="SW2" pad="1"/>
<contactref element="SW3" pad="1"/>
<contactref element="SW4" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="JP7" pad="1"/>
</signal>
<signal name="LEDK">
<contactref element="JP1" pad="1"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="IM0">
<contactref element="JP1" pad="2"/>
<contactref element="SW1" pad="2"/>
</signal>
<signal name="IM2">
<contactref element="JP1" pad="3"/>
<contactref element="SW3" pad="2"/>
</signal>
<signal name="IM1">
<contactref element="JP2" pad="2"/>
<contactref element="SW2" pad="2"/>
</signal>
<signal name="D17">
<contactref element="JP2" pad="4"/>
<contactref element="JP6" pad="9"/>
</signal>
<signal name="D15">
<contactref element="JP6" pad="8"/>
<contactref element="JP2" pad="5"/>
</signal>
<signal name="VCC">
<contactref element="SW1" pad="3"/>
<contactref element="SW2" pad="3"/>
<contactref element="SW3" pad="3"/>
<contactref element="SW4" pad="3"/>
<contactref element="JP2" pad="1"/>
<contactref element="JP1" pad="20"/>
<contactref element="C1" pad="1"/>
<contactref element="JP7" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
