<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="30.48" y2="0" width="0" layer="20"/>
<wire x1="30.48" y1="0" x2="30.48" y2="15.24" width="0" layer="20"/>
<wire x1="30.48" y1="15.24" x2="0" y2="15.24" width="0" layer="20"/>
<wire x1="0" y1="15.24" x2="0" y2="0" width="0" layer="20"/>
<text>D1</text>
<text>D3</text>
<text>D4</text>
<text>D5</text>
<text>D7</text>
<text>D8</text>
<text>D6</text>
<text>D2</text>
<text>VCC</text>
<text>GND</text>
<text>DIN</text>
<text>CLK</text>
</plain>
<libraries>
<library name="playground">
<packages>
<package name="DIL12">
<description>12 pin dual in-line package, 0.3"x0.1" pin spacing.  Edited from DIL14-KIT in SparkFun-DigitalIC.lbr.</description>
</package>
</packages>
</library>
<library name="ChipsParts">
<packages>
<package name="TSSOP-14(TI)">
<description>TSSOP-14, TI PW package, From TI SM74LV164a datasheet</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X01">
</package>
</packages>
</library>
<library name="NewFrame">
<packages>
<package name="FR-LTR-ON-PCB">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="playground" package="DIL12" value="HP_DISPLAY">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="playground" package="DIL12" value="HP_DISPLAY">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="ChipsParts" package="TSSOP-14(TI)" value="SN74LV164APW">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0805" value=""/>
<element name="R2" library="SparkFun-Resistors" package="0805" value=""/>
<element name="R3" library="SparkFun-Resistors" package="0805" value=""/>
<element name="R4" library="SparkFun-Resistors" package="0805" value=""/>
<element name="R5" library="SparkFun-Resistors" package="0805" value=""/>
<element name="R6" library="SparkFun-Resistors" package="0805" value=""/>
<element name="R7" library="SparkFun-Resistors" package="0805" value=""/>
<element name="R8" library="SparkFun-Resistors" package="0805" value="56"/>
<element name="C1" library="SparkFun-Capacitors" package="0805" value="10uF"/>
<element name="JP1" library="SparkFun-Connectors" package="1X01" value="M01PTH">
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="1X01" value="M01PTH">
<attribute name="VALUE"/>
</element>
<element name="JP3" library="SparkFun-Connectors" package="1X01" value="M01PTH">
<attribute name="VALUE"/>
</element>
<element name="JP4" library="SparkFun-Connectors" package="1X01" value="M01PTH">
<attribute name="VALUE"/>
</element>
<element name="JP5" library="SparkFun-Connectors" package="1X01" value="M01PTH">
<attribute name="VALUE"/>
</element>
<element name="JP6" library="SparkFun-Connectors" package="1X01" value="M01PTH">
<attribute name="VALUE"/>
</element>
<element name="JP7" library="SparkFun-Connectors" package="1X01" value="M01PTH">
<attribute name="VALUE"/>
</element>
<element name="JP8" library="SparkFun-Connectors" package="1X01" value="M01PTH">
<attribute name="VALUE"/>
</element>
<element name="JP9" library="SparkFun-Connectors" package="1X01" value="M01PTH">
<attribute name="VALUE"/>
</element>
<element name="JP10" library="SparkFun-Connectors" package="1X01" value="M01PTH">
<attribute name="VALUE"/>
</element>
<element name="JP11" library="SparkFun-Connectors" package="1X01" value="M01PTH">
<attribute name="VALUE"/>
</element>
<element name="JP12" library="SparkFun-Connectors" package="1X01" value="M01PTH">
<attribute name="VALUE"/>
</element>
<element name="FRAME1" library="NewFrame" package="FR-LTR-ON-PCB" value="FRAME_LTR_CU_MARK">
<attribute name="CNAME" value="C.Schnarel"/>
<attribute name="DATECODE" value="13OCT2014"/>
<attribute name="DESIGNER" value="C.Schnarel"/>
<attribute name="CREVISION" value="Rev 2"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="R1" pad="1"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="N$2">
<contactref element="R2" pad="1"/>
<contactref element="U1" pad="4"/>
</signal>
<signal name="N$3">
<contactref element="R3" pad="1"/>
<contactref element="U1" pad="5"/>
</signal>
<signal name="N$4">
<contactref element="R4" pad="1"/>
<contactref element="U1" pad="6"/>
</signal>
<signal name="N$5">
<contactref element="R5" pad="1"/>
<contactref element="U1" pad="10"/>
</signal>
<signal name="N$6">
<contactref element="U1" pad="11"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="R7" pad="1"/>
<contactref element="U1" pad="12"/>
</signal>
<signal name="N$8">
<contactref element="R8" pad="1"/>
<contactref element="U1" pad="13"/>
</signal>
<signal name="VCC">
<contactref element="U1" pad="9"/>
<contactref element="U1" pad="14"/>
<contactref element="U1" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="JP9" pad="1"/>
</signal>
<signal name="GND">
<contactref element="U1" pad="7"/>
<contactref element="C1" pad="2"/>
<contactref element="JP12" pad="1"/>
</signal>
<signal name="CLK">
<contactref element="U1" pad="8"/>
<contactref element="JP11" pad="1"/>
</signal>
<signal name="SEGA">
<contactref element="U$1" pad="12"/>
<contactref element="U$2" pad="12"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="SEGB">
<contactref element="U$1" pad="11"/>
<contactref element="U$2" pad="11"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="SEGC">
<contactref element="U$1" pad="3"/>
<contactref element="U$2" pad="3"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="SEGD">
<contactref element="U$2" pad="8"/>
<contactref element="U$1" pad="8"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="SEGE">
<contactref element="U$2" pad="2"/>
<contactref element="U$1" pad="2"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="SEGF">
<contactref element="U$2" pad="9"/>
<contactref element="U$1" pad="9"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="SEGG">
<contactref element="U$2" pad="7"/>
<contactref element="U$1" pad="7"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="SEGDP">
<contactref element="U$2" pad="5"/>
<contactref element="U$1" pad="5"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="DIG1">
<contactref element="U$1" pad="1"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="DIG2">
<contactref element="U$1" pad="10"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="DIG3">
<contactref element="U$1" pad="4"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="DIG4">
<contactref element="U$1" pad="6"/>
<contactref element="JP4" pad="1"/>
</signal>
<signal name="DIG5">
<contactref element="U$2" pad="1"/>
<contactref element="JP5" pad="1"/>
</signal>
<signal name="DIG6">
<contactref element="U$2" pad="10"/>
<contactref element="JP6" pad="1"/>
</signal>
<signal name="DIG7">
<contactref element="U$2" pad="4"/>
<contactref element="JP7" pad="1"/>
</signal>
<signal name="DIG8">
<contactref element="U$2" pad="6"/>
<contactref element="JP8" pad="1"/>
</signal>
<signal name="DIN">
<contactref element="U1" pad="2"/>
<contactref element="JP10" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
