<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<text>OUT</text>
<text>5V</text>
<text>GND</text>
<text>PWM</text>
<text>GND</text>
<text>VCC</text>
<text>+</text>
<text>-</text>
<text>12V</text>
<text>5V</text>
<text>+</text>
<text>+</text>
<text>-</text>
<text>-</text>
<text>LED</text>
<text>+</text>
<text>-</text>
<wire x1="0.028465625" y1="27.639725" x2="0" y2="-0.254" width="0.254" layer="20"/>
<wire x1="0" y1="-0.254" x2="53.213" y2="-0.254" width="0.254" layer="20"/>
<wire x1="53.213" y1="-0.254" x2="53.241465625" y2="27.639725" width="0.254" layer="20"/>
<wire x1="53.241465625" y1="27.639725" x2="0.028465625" y2="27.639725" width="0.254" layer="20"/>
<text>HEATSINK</text>
<text>hummerdikk 2014</text>
<text>Led strip driver
with 
high speed optocoupled input</text>
<text>IN_A</text>
<text>OUT_A</text>
<hole x="12.192" y="2.032" drill="3.2"/>
<hole x="2.54" y="25.4" drill="3.2"/>
<hole x="39.37" y="25.4" drill="3.2"/>
<hole x="39.37" y="2.032" drill="3.2"/>
</plain>
<libraries>
<library name="on-semiconductor">
<description>&lt;b&gt;ON Semiconductor&lt;/b&gt;&lt;p&gt;
&lt;a href="http://onsemi.com"&gt; Home page &lt;/a&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL8">
<description>&lt;B&gt;Dual In Line&lt;/B&gt;&lt;p&gt;
package type P</description>
</package>
</packages>
</library>
<library name="microchip">
<description>&lt;b&gt;Microchip PIC Microcontrollers and other Devices&lt;/b&gt;&lt;p&gt;
Based on the following sources :
&lt;ul&gt;
&lt;li&gt;Microchip Data Book, 1993
&lt;li&gt;THE EMERGING WORLD STANDARD, 1995/1996
&lt;li&gt;Microchip, Technical Library CD-ROM, June 1998
&lt;li&gt;www.microchip.com
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL8">
<description>&lt;B&gt;Dual In Line&lt;/B&gt;&lt;p&gt;
package type P</description>
</package>
</packages>
</library>
<library name="transistor-power">
<description>&lt;b&gt;Power Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO220BV">
<description>&lt;b&gt;Molded Package&lt;/b&gt;&lt;p&gt;
grid 2.54 mm</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="0207/10">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 10 mm</description>
</package>
<package name="0207/5V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 5 mm</description>
</package>
<package name="C025-024X044">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 2.4 x 4.4 mm</description>
</package>
<package name="E5-6">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5.08 mm, diameter 6 mm</description>
</package>
<package name="DO41-10">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 2.54 mm, horizontal, grid 10.16 mm</description>
</package>
<package name="0414V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0414, grid 5 mm</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="MOLEX-1X2">
</package>
</packages>
</library>
<library name="SparkFunConnectorHummerdikk2">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SCREWTERMINAL-5MM-2">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="MC34151" library="on-semiconductor" package="DIL8" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="6N137" library="microchip" package="DIL8" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MOSFET" library="transistor-power" package="TO220BV" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="adafruit" package="0207/10" value="330">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="adafruit" package="C025-024X044" value="100 nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="adafruit" package="C025-024X044" value="100 nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="adafruit" package="DO41-10" value="1N5819">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="adafruit" package="DO41-10" value="1N5819">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="E$2" library="SparkFun-Connectors" package="MOLEX-1X2" value=""/>
<element name="12V_CON" library="SparkFunConnectorHummerdikk2" package="SCREWTERMINAL-5MM-2" value=""/>
<element name="5V_CON" library="SparkFunConnectorHummerdikk2" package="SCREWTERMINAL-5MM-2" value=""/>
<element name="LED_OUT_CONNECTOR" library="SparkFunConnectorHummerdikk2" package="SCREWTERMINAL-5MM-2" value=""/>
<element name="C3" library="adafruit" package="E5-6" value="10 uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="adafruit" package="0207/5V" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="adafruit" package="0414V" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="adafruit" package="C025-024X044" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="S$1">
<contactref element="6N137" pad="2"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="5V">
<contactref element="6N137" pad="8"/>
<contactref element="C1" pad="1"/>
<contactref element="6N137" pad="7"/>
<contactref element="5V_CON" pad="1"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="GND">
<contactref element="6N137" pad="5"/>
<contactref element="C1" pad="2"/>
<contactref element="MC34151" pad="3"/>
<contactref element="D2" pad="A"/>
<contactref element="5V_CON" pad="2"/>
<contactref element="12V_CON" pad="2"/>
<contactref element="MOSFET" pad="S"/>
<contactref element="MC34151" pad="4"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="S$4">
<contactref element="MC34151" pad="2"/>
<contactref element="6N137" pad="6"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="12V">
<contactref element="MC34151" pad="6"/>
<contactref element="C2" pad="1"/>
<contactref element="D1" pad="C"/>
<contactref element="12V_CON" pad="1"/>
<contactref element="LED_OUT_CONNECTOR" pad="1"/>
<contactref element="C3" pad="+"/>
</signal>
<signal name="S$3">
<contactref element="D2" pad="C"/>
<contactref element="D1" pad="A"/>
<contactref element="MC34151" pad="7"/>
<contactref element="R3" pad="2"/>
<contactref element="C4" pad="2"/>
</signal>
<signal name="S$11">
<contactref element="R1" pad="1"/>
<contactref element="E$2" pad="1"/>
</signal>
<signal name="S$12">
<contactref element="6N137" pad="3"/>
<contactref element="E$2" pad="2"/>
</signal>
<signal name="S$2">
<contactref element="MOSFET" pad="D"/>
<contactref element="LED_OUT_CONNECTOR" pad="2"/>
<contactref element="C3" pad="-"/>
</signal>
<signal name="S$5">
<contactref element="MOSFET" pad="G"/>
<contactref element="R3" pad="1"/>
<contactref element="C4" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
