<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="16.51" x2="0" y2="2.54" width="0" layer="20"/>
<wire x1="0" y1="2.54" x2="2.54" y2="0" width="0" layer="20" curve="90"/>
<wire x1="2.54" y1="0" x2="16.8275" y2="0" width="0" layer="20"/>
<wire x1="16.8275" y1="0" x2="19.05" y2="2.2225" width="0" layer="20" curve="90"/>
<wire x1="19.05" y1="2.2225" x2="19.05" y2="16.8275" width="0" layer="20"/>
<wire x1="19.05" y1="16.8275" x2="16.8275" y2="19.05" width="0" layer="20" curve="90"/>
<wire x1="16.8275" y1="19.05" x2="2.54" y2="19.05" width="0" layer="20"/>
<wire x1="2.54" y1="19.05" x2="0" y2="16.51" width="0" layer="20" curve="90"/>
<text>RST</text>
<text>GND</text>
<text>0</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>VCC</text>
<text>Barbary</text>
<text>Enterprises</text>
<text>Pixie</text>
<text>85</text>
<text>ATtiny85</text>
</plain>
<libraries>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DIP08">
<description>&lt;b&gt;Dual In Line&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X04">
</package>
</packages>
</library>
<library name="barbary_enterprises">
<packages>
<package name="2X3-NS">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="SparkFun-DigitalIC" package="DIP08" value="TINY45-20-DIP">
<attribute name="PROD_ID" value="IC-09439"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="VALUE"/>
</element>
<element name="J1" library="barbary_enterprises" package="2X3-NS" value="AVR_SPI_PRG_6LABELED"/>
</elements>
<signals>
<signal name="GND">
<contactref element="U1" pad="4"/>
<contactref element="JP1" pad="1"/>
<contactref element="J1" pad="6"/>
</signal>
<signal name="VCC">
<contactref element="U1" pad="8"/>
<contactref element="JP2" pad="4"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="0">
<contactref element="U1" pad="5"/>
<contactref element="J1" pad="4"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="1">
<contactref element="U1" pad="6"/>
<contactref element="JP2" pad="2"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="2">
<contactref element="U1" pad="7"/>
<contactref element="J1" pad="3"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="3">
<contactref element="U1" pad="2"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="4">
<contactref element="U1" pad="3"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="RST">
<contactref element="U1" pad="1"/>
<contactref element="JP1" pad="4"/>
<contactref element="J1" pad="5"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
