<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.0">
<drawing>
<board>
<plain>
<wire x1="1.27" y1="0" x2="49.53" y2="0" width="0" layer="20"/>
<hole x="31.115" y="12.7" drill="3.6"/>
<hole x="15.24" y="26.67" drill="3.6"/>
<hole x="46.99" y="26.67" drill="3.6"/>
<text>PWM1</text>
<wire x1="1.27" y1="29.21" x2="49.53" y2="29.21" width="0" layer="20"/>
<wire x1="49.53" y1="29.21" x2="49.53" y2="0" width="0" layer="20"/>
<wire x1="1.27" y1="29.21" x2="1.27" y2="0" width="0" layer="20"/>
<text>+</text>
<text>+</text>
<text>+</text>
<text>-</text>
<text>-</text>
<text>-</text>
</plain>
<libraries>
<library name="SparkFun">
<packages>
<package name="PANASONIC_E">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package E&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="resistor">
<packages>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="led">
<packages>
<package name="CHIP-LED0805">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB R99A&lt;br&gt;
Source: http://www.osram.convergy.de/ ... lb_r99a.pdf</description>
</package>
</packages>
</library>
<library name="transistor-power">
<packages>
<package name="TO220BV">
<description>&lt;b&gt;Molded Package&lt;/b&gt;&lt;p&gt;
grid 2.54 mm</description>
</package>
</packages>
</library>
<library name="con-amp">
<packages>
<package name="10X02MTA">
<description>&lt;b&gt;AMP MTA connector&lt;/b&gt;&lt;p&gt;
Source: http://ecommas.tycoelectronics.com .. ENG_CD_640456_W.pdf</description>
</package>
</packages>
</library>
<library name="con-weidmueller-sl35">
<packages>
<package name="180G-2">
<description>&lt;b&gt;WEIDMUELLER CLAMP CONNECTOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="linear">
<description>&lt;b&gt;Linear Devices&lt;/b&gt;&lt;p&gt;
Operational amplifiers,  comparators, voltage regulators, ADCs, DACs, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT89">
<description>&lt;b&gt;SOT98&lt;/b&gt; PK (R-PDSO-G3)&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/ua78l05.pdf</description>
</package>
</packages>
</library>
<library name="custom_esorensen">
<packages>
<package name="SOIC8">
</package>
</packages>
</library>
<library name="eric_sorensen">
<packages>
<package name="1715250000">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="MOLEX-1X2">
</package>
<package name="MOLEX-1X4">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="Q6" library="transistor-power" package="TO220BV" value="AOT240L">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q7" library="transistor-power" package="TO220BV" value="AOT240L">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R69" library="resistor" package="R0603" value="22R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R70" library="resistor" package="R0603" value="22R">
<attribute name="VALUE"/>
</element>
<element name="C60" library="SparkFun" package="PANASONIC_E" value="100uF">
<attribute name="NAME"/>
</element>
<element name="R71" library="resistor" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R72" library="resistor" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X10" library="con-weidmueller-sl35" package="180G-2" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="J9" library="con-amp" package="10X02MTA" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R67" library="resistor" package="R0603" value="5.6K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R68" library="resistor" package="R0603" value="5.6K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED7" library="led" package="CHIP-LED0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED8" library="led" package="CHIP-LED0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C62" library="resistor" package="C0603" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C66" library="resistor" package="C0603" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC14" library="custom_esorensen" package="SOIC8" value="TC4427">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC11" library="linear" package="SOT89" value="78L12F">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$5" library="eric_sorensen" package="1715250000" value="5MMCONN"/>
<element name="U$6" library="eric_sorensen" package="1715250000" value="5MMCONN"/>
<element name="R90" library="resistor" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R91" library="resistor" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X13" library="con-weidmueller-sl35" package="180G-2" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="X15" library="con-weidmueller-sl35" package="180G-2" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="U$10" library="eric_sorensen" package="1715250000" value="5MMCONN"/>
<element name="J11" library="con-amp" package="10X02MTA" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="MOLEX-1X2" value="M02POLAR"/>
<element name="JP2" library="SparkFun-Connectors" package="MOLEX-1X4" value=""/>
<element name="JP3" library="SparkFun-Connectors" package="MOLEX-1X4" value=""/>
<element name="JP4" library="SparkFun-Connectors" package="MOLEX-1X4" value=""/>
<element name="JP5" library="SparkFun-Connectors" package="MOLEX-1X4" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="Q7" pad="S"/>
<contactref element="Q6" pad="S"/>
<contactref element="C60" pad="-"/>
<contactref element="R71" pad="1"/>
<contactref element="R72" pad="1"/>
<contactref element="C66" pad="2"/>
<contactref element="IC14" pad="3"/>
<contactref element="C62" pad="2"/>
<contactref element="IC11" pad="2"/>
<contactref element="IC11" pad="2@1"/>
<contactref element="U$5" pad="P$2"/>
<contactref element="R90" pad="2"/>
<contactref element="R91" pad="2"/>
<contactref element="X13" pad="2"/>
</signal>
<signal name="P2.7">
<contactref element="R72" pad="2"/>
<contactref element="IC14" pad="4"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="PWM1">
<contactref element="R71" pad="2"/>
<contactref element="IC14" pad="2"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$92">
<contactref element="Q6" pad="D"/>
<contactref element="X10" pad="1"/>
<contactref element="J9" pad="1"/>
<contactref element="LED7" pad="C"/>
<contactref element="U$10" pad="P$1"/>
</signal>
<signal name="N$94">
<contactref element="Q7" pad="D"/>
<contactref element="LED8" pad="C"/>
<contactref element="U$6" pad="P$1"/>
<contactref element="X15" pad="1"/>
<contactref element="J11" pad="1"/>
</signal>
<signal name="MOSFET_DRIVE">
<contactref element="C60" pad="+"/>
<contactref element="X10" pad="2"/>
<contactref element="J9" pad="2"/>
<contactref element="R67" pad="1"/>
<contactref element="R68" pad="1"/>
<contactref element="IC11" pad="3"/>
<contactref element="U$5" pad="P$1"/>
<contactref element="U$6" pad="P$2"/>
<contactref element="X13" pad="1"/>
<contactref element="X15" pad="2"/>
<contactref element="U$10" pad="P$2"/>
<contactref element="J11" pad="2"/>
</signal>
<signal name="N$105">
<contactref element="R67" pad="2"/>
<contactref element="LED7" pad="A"/>
</signal>
<signal name="N$112">
<contactref element="R68" pad="2"/>
<contactref element="LED8" pad="A"/>
</signal>
<signal name="12VREG">
<contactref element="C62" pad="1"/>
<contactref element="C66" pad="1"/>
<contactref element="IC14" pad="6"/>
<contactref element="IC11" pad="1"/>
</signal>
<signal name="PWM1_FET">
<contactref element="R69" pad="2"/>
<contactref element="Q6" pad="G"/>
<contactref element="R90" pad="1"/>
</signal>
<signal name="GPIO_FET">
<contactref element="R70" pad="2"/>
<contactref element="Q7" pad="G"/>
<contactref element="R91" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="R69" pad="1"/>
<contactref element="IC14" pad="7"/>
</signal>
<signal name="N$19">
<contactref element="IC14" pad="5"/>
<contactref element="R70" pad="1"/>
</signal>
<signal name="PIN1">
<contactref element="JP2" pad="1"/>
<contactref element="JP3" pad="1"/>
<contactref element="JP4" pad="1"/>
<contactref element="JP5" pad="1"/>
</signal>
<signal name="PIN2">
<contactref element="JP2" pad="2"/>
<contactref element="JP3" pad="2"/>
<contactref element="JP4" pad="2"/>
<contactref element="JP5" pad="2"/>
</signal>
<signal name="PIN3">
<contactref element="JP4" pad="3"/>
<contactref element="JP3" pad="3"/>
<contactref element="JP2" pad="3"/>
<contactref element="JP5" pad="3"/>
</signal>
<signal name="PIN4">
<contactref element="JP2" pad="4"/>
<contactref element="JP3" pad="4"/>
<contactref element="JP4" pad="4"/>
<contactref element="JP5" pad="4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
