<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="-0.508" y1="0" x2="16.688" y2="0" width="0" layer="20"/>
<wire x1="16.688" y1="0" x2="16.688" y2="8.372" width="0" layer="20"/>
<wire x1="16.688" y1="8.372" x2="-0.508" y2="8.372" width="0" layer="20"/>
<wire x1="-0.508" y1="8.372" x2="-0.508" y2="0" width="0" layer="20"/>
<text>COM</text>
<text>OUT</text>
<text>4 BIT R2R </text>
</plain>
<libraries>
<library name="resistor-array">
<description>&lt;b&gt;SMD Resistor Arrays&lt;/b&gt;&lt;p&gt;
CTS, Rohm, etc&lt;p&gt;
&lt;p&gt;THIS LIBRARY IS PROVIDED AS IS AND WITHOUT WARRANTY OF ANY KIND, EXPRESSED OR IMPLIED.&lt;br&gt;
USE AT YOUR OWN RISK!&lt;p&gt;
&lt;author&gt;Copyright (C) 2008, Bob Starr&lt;br&gt; http://www.bobstarr.net&lt;br&gt;&lt;/author&gt;</description>
<packages>
<package name="742-8">
<description>CTS 742 Series&lt;p&gt;
8 Terminations, 4 Resistors</description>
</package>
</packages>
</library>
<library name="dp_devices">
<description>Dangerous Prototypes Standard PCB sizes
http://dangerousprototypes.com</description>
<packages>
<package name="M1X6">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R" library="resistor-array" package="742-8" value="R">
<attribute name="VALUE"/>
</element>
<element name="RN1" library="resistor-array" package="742-8" value="2R">
<attribute name="VALUE"/>
</element>
<element name="J2" library="dp_devices" package="M1X6" value="CON_HEADER_1X06-PTH"/>
</elements>
<signals>
<signal name="N$91">
<contactref element="R" pad="5"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="N$92">
<contactref element="R" pad="4"/>
<contactref element="R" pad="3"/>
<contactref element="RN1" pad="4"/>
</signal>
<signal name="N$93">
<contactref element="R" pad="6"/>
<contactref element="R" pad="7"/>
<contactref element="RN1" pad="3"/>
</signal>
<signal name="N$94">
<contactref element="R" pad="2"/>
<contactref element="R" pad="1"/>
<contactref element="RN1" pad="2"/>
</signal>
<signal name="N$95">
<contactref element="R" pad="8"/>
<contactref element="RN1" pad="1"/>
<contactref element="J2" pad="6"/>
</signal>
<signal name="N$1">
<contactref element="RN1" pad="5"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="RN1" pad="6"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="N$3">
<contactref element="RN1" pad="7"/>
<contactref element="J2" pad="4"/>
</signal>
<signal name="N$4">
<contactref element="RN1" pad="8"/>
<contactref element="J2" pad="5"/>
</signal>
<signal name="N$5">
</signal>
<signal name="N$6">
</signal>
</signals>
</board>
</drawing>
</eagle>
