<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="0" y1="39.918615625" x2="0" y2="0.71841875" width="0" layer="20"/>
<wire x1="0" y1="0.71841875" x2="0.71841875" y2="0" width="0" layer="20" curve="90"/>
<wire x1="0.71841875" y1="0" x2="14.62571875" y2="0" width="0" layer="20"/>
<wire x1="14.62571875" y1="0" x2="15.164" y2="0.53828125" width="0" layer="20" curve="90"/>
<wire x1="15.164" y1="0.53828125" x2="15.164" y2="39.9707375" width="0" layer="20"/>
<wire x1="15.164" y1="39.9707375" x2="14.5047375" y2="40.63" width="0" layer="20" curve="90"/>
<wire x1="14.5047375" y1="40.63" x2="0.711384375" y2="40.63" width="0" layer="20"/>
<wire x1="0.711384375" y1="40.63" x2="0" y2="39.918615625" width="0" layer="20" curve="90"/>
<text>GND</text>
<text>+5V</text>
<text>CTL</text>
<text>AOA Indexer Display</text>
<text>aeropunk.com</text>
<text>4/24/2013</text>
</plain>
<libraries>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CREATIVE_COMMONS">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X03_NO_SILK">
</package>
</packages>
</library>
<library name="Aeropunk">
<packages>
<package name="WS2812">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="FRAME1" library="SparkFun-Aesthetics" package="CREATIVE_COMMONS" value="FRAME-LETTER"/>
<element name="LED1" library="Aeropunk" package="WS2812" value="WS2812">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="Aeropunk" package="WS2812" value="WS2812">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED3" library="Aeropunk" package="WS2812" value="WS2812">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X03_NO_SILK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Passives" package="0805" value="150"/>
<element name="C1" library="SparkFun-Passives" package="0805" value="0.1uF"/>
<element name="R3" library="SparkFun-Passives" package="0805" value="150"/>
<element name="C3" library="SparkFun-Passives" package="0805" value="0.1uF"/>
<element name="R2" library="SparkFun-Passives" package="0805" value="150">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Passives" package="0805" value="0.1uF"/>
</elements>
<signals>
<signal name="CTL">
<contactref element="LED1" pad="2"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="VCC">
<contactref element="LED1" pad="5"/>
<contactref element="JP1" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="LED3" pad="5"/>
<contactref element="R2" pad="1"/>
<contactref element="LED2" pad="5"/>
</signal>
<signal name="GND">
<contactref element="LED1" pad="6"/>
<contactref element="LED2" pad="6"/>
<contactref element="LED3" pad="6"/>
<contactref element="JP1" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="LED2" pad="2"/>
<contactref element="LED1" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="LED2" pad="1"/>
<contactref element="LED3" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="R1" pad="2"/>
<contactref element="LED1" pad="3"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="R3" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="LED3" pad="3"/>
</signal>
<signal name="N$5">
<contactref element="R2" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="LED2" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
