<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<board>
<plain>
<wire x1="29.21" y1="15.24" x2="44.7675" y2="15.24" width="0" layer="20"/>
<wire x1="44.7675" y1="15.24" x2="44.7675" y2="27.295" width="0" layer="20"/>
<wire x1="44.7675" y1="27.295" x2="29.21" y2="27.295" width="0" layer="20"/>
<wire x1="29.21" y1="27.295" x2="29.21" y2="15.24" width="0" layer="20"/>
</plain>
<libraries>
<library name="transistor-small-signal">
<description>&lt;b&gt;Small Signal Transistors&lt;/b&gt;&lt;p&gt;
Packages from :&lt;br&gt;
www.infineon.com; &lt;br&gt;
www.semiconductors.com;&lt;br&gt;
www.irf.com&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="B1,27">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X06">
</package>
<package name="1X02_LOCK">
</package>
<package name="1206">
</package>
<package name="1X01">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="Q1" library="transistor-small-signal" package="SOT23" value="BSS123">
<attribute name="VALUE"/>
</element>
<element name="Q3" library="transistor-small-signal" package="SOT23" value="BSS123">
<attribute name="VALUE"/>
</element>
<element name="Q5" library="transistor-small-signal" package="SOT23" value="BSS123">
<attribute name="VALUE"/>
</element>
<element name="Q7" library="transistor-small-signal" package="SOT23" value="BSS123">
<attribute name="VALUE"/>
</element>
<element name="TP1" library="testpad" package="B1,27" value="TPB1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP2" library="testpad" package="B1,27" value="TPB1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP3" library="testpad" package="B1,27" value="TPB1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP4" library="testpad" package="B1,27" value="TPB1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun" package="1X06" value="">
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun" package="1X02_LOCK" value="">
<attribute name="VALUE"/>
</element>
<element name="JP3" library="SparkFun" package="1X02_LOCK" value="">
<attribute name="VALUE"/>
</element>
<element name="Q2" library="transistor-small-signal" package="SOT23" value="BSS123">
<attribute name="VALUE"/>
</element>
<element name="TP5" library="testpad" package="B1,27" value="TPB1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="PPM" library="testpad" package="B1,27" value="TPB1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q4" library="transistor-small-signal" package="SOT23" value="BSS123">
<attribute name="VALUE"/>
</element>
<element name="TP7" library="testpad" package="B1,27" value="TPB1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun" package="1206" value=""/>
<element name="R2" library="SparkFun" package="1206" value=""/>
<element name="R3" library="SparkFun" package="1206" value=""/>
<element name="R4" library="SparkFun" package="1206" value=""/>
<element name="R5" library="SparkFun" package="1206" value=""/>
<element name="R6" library="SparkFun" package="1206" value=""/>
<element name="TP6" library="testpad" package="B1,27" value="TPB1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP9" library="testpad" package="B1,27" value="TPB1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP10" library="testpad" package="B1,27" value="TPB1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP11" library="testpad" package="B1,27" value="TPB1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP12" library="testpad" package="B1,27" value="TPB1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP13" library="testpad" package="B1,27" value="TPB1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="JP4" library="SparkFun" package="1X01" value="M01PTH">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$6">
<contactref element="Q3" pad="1"/>
<contactref element="JP2" pad="4"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="Q5" pad="1"/>
<contactref element="JP2" pad="5"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="Q7" pad="1"/>
<contactref element="JP2" pad="6"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="Q1" pad="1"/>
<contactref element="JP2" pad="3"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="JP2" pad="1"/>
<contactref element="PPM" pad="TP"/>
</signal>
<signal name="N$12">
<contactref element="JP2" pad="2"/>
<contactref element="Q2" pad="1"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="TP1" pad="TP"/>
<contactref element="Q2" pad="3"/>
<contactref element="TP6" pad="TP"/>
</signal>
<signal name="N$3">
<contactref element="TP2" pad="TP"/>
<contactref element="Q1" pad="3"/>
<contactref element="TP9" pad="TP"/>
</signal>
<signal name="N$4">
<contactref element="TP3" pad="TP"/>
<contactref element="Q3" pad="3"/>
<contactref element="TP10" pad="TP"/>
</signal>
<signal name="N$5">
<contactref element="TP4" pad="TP"/>
<contactref element="Q5" pad="3"/>
<contactref element="TP11" pad="TP"/>
</signal>
<signal name="N$13">
<contactref element="TP5" pad="TP"/>
<contactref element="Q7" pad="3"/>
<contactref element="TP12" pad="TP"/>
</signal>
<signal name="N$14">
<contactref element="Q4" pad="3"/>
<contactref element="TP7" pad="TP"/>
<contactref element="TP13" pad="TP"/>
</signal>
<signal name="N$15">
<contactref element="Q4" pad="1"/>
<contactref element="R6" pad="2"/>
<contactref element="JP4" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="JP3" pad="2"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="GND">
<contactref element="Q1" pad="2"/>
<contactref element="Q3" pad="2"/>
<contactref element="Q5" pad="2"/>
<contactref element="Q7" pad="2"/>
<contactref element="JP3" pad="1"/>
<contactref element="JP1" pad="1"/>
<contactref element="Q2" pad="2"/>
<contactref element="Q4" pad="2"/>
<contactref element="R6" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$1">
</signal>
</signals>
</board>
</drawing>
</eagle>
