<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<hole x="27.432" y="6.35" drill="3.2"/>
<hole x="27.432" y="17.78" drill="3.2"/>
<wire x1="0" y1="1.27" x2="1.27" y2="0" width="0" layer="20"/>
<wire x1="1.27" y1="0" x2="43.18" y2="0" width="0" layer="20"/>
<wire x1="43.18" y1="0" x2="44.45" y2="1.27" width="0" layer="20"/>
<wire x1="44.45" y1="1.27" x2="44.45" y2="25.4" width="0" layer="20"/>
<wire x1="44.45" y1="25.4" x2="43.18" y2="26.67" width="0" layer="20"/>
<wire x1="43.18" y1="26.67" x2="1.27" y2="26.67" width="0" layer="20"/>
<wire x1="1.27" y1="26.67" x2="0" y2="25.4" width="0" layer="20"/>
<wire x1="0" y1="25.4" x2="0" y2="1.27" width="0" layer="20"/>
<text>Steve Rich</text>
<text>AntiBubbler v0.1</text>
<text>Speed Control</text>
<text>Use Slow Blow
3A/250V
5x20mm Fuse</text>
</plain>
<libraries>
<library name="national-semiconductor">
<description>&lt;b&gt;National Semiconductor&lt;/b&gt;&lt;p&gt;
http://www.national.com&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="T05D">
<description>&lt;b&gt;TO-220&lt;/b&gt;&lt;p&gt;
5 lead, National Semiconductor T05D</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="POWER_JACK_SMD">
</package>
<package name="SCREWTERMINAL-3.5MM-3">
</package>
<package name="SCREWTERMINAL-5MM-2">
</package>
</packages>
</library>
<library name="fuse">
<description>&lt;b&gt;Fuses and Fuse Holders&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SHK20L">
<description>&lt;b&gt;FUSE HOLDER&lt;/b&gt;&lt;p&gt; 5 x 20 mm, SH contact, SHH1 Schukat / E1073 Buerklin</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="national-semiconductor" package="T05D" value="LM2596T">
<attribute name="OC_NEWARK" value="65K5910"/>
<attribute name="MPN" value="LM2596T-ADJ/LF02"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="9494162"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="POWER_JACK_SMD" value="5.5x2.1mm Barrel">
<attribute name="SF_ID" value="PRT-12748"/>
<attribute name="PROD_ID" value="CONN-08106"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-3" value="">
<attribute name="PROD_ID" value="CONN-08288"/>
<attribute name="VALUE"/>
</element>
<element name="JP3" library="SparkFun-Connectors" package="SCREWTERMINAL-5MM-2" value="">
<attribute name="STOREFRONT_ID" value="PRT-08432"/>
<attribute name="VALUE"/>
</element>
<element name="F1" library="fuse" package="SHK20L" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="5VIN">
<contactref element="JP1" pad="VIN0"/>
<contactref element="F1" pad="1A"/>
</signal>
<signal name="5VOUT">
<contactref element="IC1" pad="1"/>
<contactref element="IC1" pad="5"/>
<contactref element="JP2" pad="1"/>
<contactref element="F1" pad="2A"/>
</signal>
<signal name="GND">
<contactref element="JP1" pad="P$4"/>
<contactref element="IC1" pad="3"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="3V">
<contactref element="IC1" pad="2"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="N$5">
<contactref element="JP2" pad="2"/>
<contactref element="JP3" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
