<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="31.439946875" y1="12.95" x2="6.09004375" y2="12.95" width="0" layer="20"/>
<wire x1="6.09004375" y1="12.95" x2="0" y2="6.75995625" width="0" layer="20" curve="90"/>
<wire x1="0" y1="6.75995625" x2="0" y2="6.272" width="0" layer="20"/>
<wire x1="0" y1="6.272" x2="6.272" y2="0" width="0" layer="20" curve="90"/>
<wire x1="6.272" y1="0" x2="32.567828125" y2="0" width="0" layer="20"/>
<wire x1="31.45" y1="12.95" x2="34.85" y2="12.95" width="0" layer="20"/>
<wire x1="34.85" y1="12.95" x2="36" y2="11.8" width="0" layer="20" curve="-90"/>
<wire x1="36" y1="11.8" x2="36" y2="1" width="0" layer="20"/>
<wire x1="36" y1="1" x2="35" y2="0" width="0" layer="20" curve="-90"/>
<wire x1="35" y1="0" x2="32.6" y2="0" width="0" layer="20"/>
<text>Please feed me a battery and put me back!</text>
<text>I chirp and blink like a Firefly</text>
</plain>
<libraries>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="BATTCON_20MM_4LEGS">
</package>
</packages>
</library>
<library name="atmel">
<description>&lt;b&gt;AVR Devices&lt;/b&gt;&lt;p&gt;
Configurable logic, microcontrollers, nonvolatile memories&lt;p&gt;
Based on the following sources:&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;www.atmel.com
&lt;li&gt;CD-ROM : Configurable Logic Microcontroller Nonvolatile Memory
&lt;li&gt;CadSoft download site, www.cadsoft.de or www.cadsoftusa.com , file at90smcu_v400.zip
&lt;li&gt;avr.lbr
&lt;/ul&gt;
&lt;author&gt;Revised by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="8S2">
<description>&lt;b&gt;8S2&lt;/b&gt; 8-lead, 0.208 Body&lt;p&gt;
Plastic Small Outline Package (EIAJ)&lt;br&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/2535S.pdf</description>
</package>
</packages>
</library>
<library name="_adafruit">
<packages>
<package name="CHIP-LED0603">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB Q993&lt;br&gt;
Source: http://www.osram.convergy.de/ ... Lb_q993.pdf</description>
</package>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X3_LOCK">
</package>
<package name="1X01NS-KIT">
</package>
</packages>
</library>
<library name="_roger">
<description>&lt;h1&gt;Roger's Parts&lt;/h1&gt;</description>
<packages>
<package name="BUZZER-9MM">
<description>&lt;b&gt;9mm x 9mm Piezo Buzzer&lt;/b&gt;
&lt;p&gt;
4KHz frequency
&lt;/p&gt;
&lt;p&gt;
Mouser part 81-PKMCS0909E4000-R1
&lt;br/&gt;
MFR part PKMCS0909E4000-R1
&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-S">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="CR-2032" library="SparkFun-Electromechanical" package="BATTCON_20MM_4LEGS" value="3v Lithium Battery">
<attribute name="PROD_ID" value="BATT-10373"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="atmel" package="8S2" value="TINY13-20SU">
<attribute name="OC_NEWARK" value="96K6522"/>
<attribute name="MPN" value="ATTINY13-20SU"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="9171568"/>
</element>
<element name="LED1" library="_adafruit" package="CHIP-LED0603" value="BRIGHT"/>
<element name="R1" library="_adafruit" package="R0603" value="1M">
<attribute name="NAME"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="2X3_LOCK" value="AVR_SPI_PRG_62X3_LOCK"/>
<element name="JP2" library="SparkFun-Connectors" package="1X01NS-KIT" value="M01NOSILK-KIT"/>
<element name="JP3" library="SparkFun-Connectors" package="1X01NS-KIT" value="M01NOSILK-KIT"/>
<element name="SG1" library="_roger" package="BUZZER-9MM" value="BUZZERSMT"/>
<element name="R2" library="_adafruit" package="R1206" value="1300">
<attribute name="NAME"/>
</element>
<element name="U$1" library="SparkFun-Aesthetics" package="OSHW-LOGO-S" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="IC1" pad="4"/>
<contactref element="LED1" pad="C"/>
<contactref element="R1" pad="2"/>
<contactref element="JP1" pad="6"/>
<contactref element="R2" pad="2"/>
<contactref element="CR-2032" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="IC1" pad="8"/>
<contactref element="JP1" pad="2"/>
<contactref element="CR-2032" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="IC1" pad="3"/>
<contactref element="LED1" pad="A"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="IC1" pad="1"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="N$3">
<contactref element="IC1" pad="7"/>
<contactref element="JP3" pad="1"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="IC1" pad="6"/>
<contactref element="JP1" pad="1"/>
<contactref element="SG1" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="JP1" pad="4"/>
<contactref element="IC1" pad="5"/>
</signal>
<signal name="N$6">
<contactref element="IC1" pad="2"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="SG1" pad="2"/>
<contactref element="R2" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
