<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.2">
<drawing>
<board>
<plain>
<wire x1="55.88" y1="44.196" x2="80.264" y2="44.196" width="0" layer="20"/>
<wire x1="80.264" y1="44.196" x2="81.788" y2="42.672" width="0" layer="20"/>
<wire x1="81.788" y1="42.672" x2="81.788" y2="24.384" width="0" layer="20"/>
<wire x1="81.788" y1="24.384" x2="80.264" y2="22.86" width="0" layer="20"/>
<wire x1="80.264" y1="22.86" x2="55.88" y2="22.86" width="0" layer="20"/>
<wire x1="55.88" y1="22.86" x2="54.356" y2="24.384" width="0" layer="20"/>
<wire x1="54.356" y1="24.384" x2="54.356" y2="42.672" width="0" layer="20"/>
<wire x1="54.356" y1="42.672" x2="55.88" y2="44.196" width="0" layer="20"/>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>5</text>
<text>6</text>
<text>7</text>
<text>8</text>
<text>9</text>
<text>10</text>
<text>11</text>
<text>12</text>
<text>13</text>
<text>14</text>
<text>15</text>
<text>16</text>
<text>17</text>
<text>18</text>
<text>19</text>
<text>20</text>
<text>5V</text>
<text>ATtiny87</text>
<text>breakout</text>
</plain>
<libraries>
<library name="attiny87_167_automotive">
<description>&lt;b&gt;Atmel ATtiny87/167 Automotive: 8-bit AVR microcontroller with 8/16 kB in-system programmable flash and LIN controller&lt;/b&gt;
&lt;p&gt;&lt;b&gt;Based on Automotive Datasheet 07/09 - Doublecheck before using!&lt;/b&gt;&lt;/p&gt;</description>
<packages>
<package name="TSSOP20">
<description>&lt;b&gt;Thin Shrink Small Outline Plastic 20&lt;/b&gt;&lt;p&gt;
MAX3223-MAX3243.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X10_LOCK">
</package>
<package name="2X3_LOCK">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="attiny87_167_automotive" package="TSSOP20" value="ATTINY87"/>
<element name="JP1" library="SparkFun-Connectors" package="1X10_LOCK" value="M10LOCK"/>
<element name="JP2" library="SparkFun-Connectors" package="1X10_LOCK" value="M10LOCK"/>
<element name="J1" library="SparkFun-Connectors" package="2X3_LOCK" value="ICSP">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="P5">
<contactref element="IC1" pad="5"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="P6">
<contactref element="IC1" pad="6"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="P15">
<contactref element="IC1" pad="15"/>
<contactref element="JP2" pad="5"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="P16">
<contactref element="IC1" pad="16"/>
<contactref element="JP2" pad="6"/>
<contactref element="J1" pad="6"/>
</signal>
<signal name="P11">
<contactref element="IC1" pad="11"/>
<contactref element="JP2" pad="1"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="P12">
<contactref element="IC1" pad="12"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="P13">
<contactref element="IC1" pad="13"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="P14">
<contactref element="IC1" pad="14"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="P17">
<contactref element="IC1" pad="17"/>
<contactref element="JP2" pad="7"/>
</signal>
<signal name="P18">
<contactref element="IC1" pad="18"/>
<contactref element="JP2" pad="8"/>
</signal>
<signal name="P19">
<contactref element="IC1" pad="19"/>
<contactref element="JP2" pad="9"/>
</signal>
<signal name="P20">
<contactref element="IC1" pad="20"/>
<contactref element="JP2" pad="10"/>
</signal>
<signal name="P10">
<contactref element="IC1" pad="10"/>
<contactref element="JP1" pad="10"/>
</signal>
<signal name="P9">
<contactref element="IC1" pad="9"/>
<contactref element="JP1" pad="9"/>
</signal>
<signal name="P8">
<contactref element="IC1" pad="8"/>
<contactref element="JP1" pad="8"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="P7">
<contactref element="IC1" pad="7"/>
<contactref element="JP1" pad="7"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="P4">
<contactref element="IC1" pad="4"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="P3">
<contactref element="IC1" pad="3"/>
<contactref element="JP1" pad="3"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="P2">
<contactref element="IC1" pad="2"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="P1">
<contactref element="IC1" pad="1"/>
<contactref element="JP1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
