<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="24.11" y2="0" width="0" layer="20"/>
<wire x1="24.11" y1="0" x2="24.11" y2="12.37" width="0" layer="20"/>
<wire x1="24.11" y1="12.37" x2="0" y2="12.37" width="0" layer="20"/>
<wire x1="0" y1="12.37" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="switch-omron">
<description>&lt;b&gt;Omron Switches&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="B3F-10XX">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X04_LONGPADS">
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="DUOLED-C-5MM">
<description>&lt;B&gt;DUO LED&lt;/B&gt;&lt;P&gt;
2 colors (red/green, red/yellow), 5 mm, round, common Cathode&lt;BR&gt;
&lt;I&gt;www.ligitek.com&lt;/I&gt; or other producers.</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="S1" library="switch-omron" package="B3F-10XX" value="">
<attribute name="OC_NEWARK" value="36M3542"/>
<attribute name="MPN" value="B3F-1000"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="176432"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X04_LONGPADS" value="remote"/>
<element name="LD1" library="led" package="DUOLED-C-5MM" value=""/>
<element name="R1" library="SparkFun-Passives" package="AXIAL-0.3" value="330"/>
<element name="R2" library="SparkFun-Passives" package="AXIAL-0.3" value="330"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="LD1" pad="AR"/>
<contactref element="R1" pad="P$2"/>
</signal>
<signal name="N$2">
<contactref element="LD1" pad="AX"/>
<contactref element="R2" pad="P$2"/>
</signal>
<signal name="N$3">
<contactref element="S1" pad="1"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="N$4">
<contactref element="R1" pad="P$1"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="N$5">
<contactref element="R2" pad="P$1"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="JP1" pad="1"/>
<contactref element="S1" pad="3"/>
</signal>
<signal name="N$6">
<contactref element="S1" pad="2"/>
<contactref element="LD1" pad="C"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
