<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="-0.762" y1="11.176" x2="-0.762" y2="62.484" width="0.254" layer="20"/>
<wire x1="-0.762" y1="62.484" x2="7.62" y2="62.484" width="0.254" layer="20"/>
<wire x1="7.62" y1="62.484" x2="7.62" y2="66.802" width="0.254" layer="20"/>
<wire x1="7.62" y1="66.802" x2="39.878" y2="66.802" width="0.254" layer="20"/>
<wire x1="39.878" y1="66.802" x2="39.878" y2="48.26" width="0.254" layer="20"/>
<wire x1="39.878" y1="48.26" x2="13.97" y2="48.26" width="0.254" layer="20"/>
<wire x1="13.97" y1="48.26" x2="13.97" y2="30.988" width="0.254" layer="20"/>
<wire x1="13.97" y1="30.988" x2="38.354" y2="30.988" width="0.254" layer="20"/>
<wire x1="38.354" y1="30.988" x2="38.354" y2="8.128" width="0.254" layer="20"/>
<wire x1="38.354" y1="8.128" x2="7.62" y2="8.128" width="0.254" layer="20"/>
<wire x1="7.62" y1="8.128" x2="7.62" y2="11.176" width="0.254" layer="20"/>
<wire x1="7.62" y1="11.176" x2="-0.762" y2="11.176" width="0.254" layer="20"/>
<text>PlantAware</text>
<text>System Controller Module 1.0</text>
</plain>
<libraries>
<library name="ChipsParts">
<packages>
<package name="RFM69W">
<description>Radio module based on the RFM69 chip from HopeRF</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="U.FL">
</package>
</packages>
</library>
<library name="SparkFun-Boards">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find boards and modules: Arduino footprints, breadboards, non-RF modules, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X20-SHROUDED">
</package>
</packages>
</library>
<library name="crystal">
<packages>
<package name="TC38H">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="CR1220-THM">
</package>
</packages>
</library>
<library name="PlantAware">
<packages>
<package name="SO8">
<description>&lt;b&gt;SMALL OUTLINE INTEGRATED CIRCUIT&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="dp_devices">
<description>Dangerous Prototypes Standard PCB sizes
http://dangerousprototypes.com</description>
<packages>
<package name="C1206">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="ChipsParts" package="RFM69W" value="RFM69W"/>
<element name="J1" library="SparkFun-Connectors" package="U.FL" value="U.FL">
<attribute name="PROD_ID" value="CONN-09193"/>
</element>
<element name="PICONN" library="SparkFun-Boards" package="2X20-SHROUDED" value="RASPBERRYPI-B+-GPIO"/>
<element name="32.768KHZ" library="crystal" package="TC38H" value="32.768"/>
<element name="CR1220" library="adafruit" package="CR1220-THM" value="CR1220"/>
<element name="DS1307" library="PlantAware" package="SO8" value="DS1307"/>
<element name="R3" library="SparkFun-Passives" package="0805" value="2.2K"/>
<element name="R4" library="SparkFun-Passives" package="0805" value="2.2K"/>
<element name="C1" library="dp_devices" package="C1206" value="0.1 uF"/>
</elements>
<signals>
<signal name="GND">
<contactref element="PICONN" pad="29"/>
<contactref element="PICONN" pad="33"/>
<contactref element="C1" pad="2"/>
<contactref element="DS1307" pad="4"/>
<contactref element="CR1220" pad="-"/>
<contactref element="U1" pad="9"/>
<contactref element="U1" pad="11"/>
<contactref element="J1" pad="P$2"/>
<contactref element="J1" pad="P$1"/>
<contactref element="PICONN" pad="40"/>
</signal>
<signal name="N$8">
</signal>
<signal name="VCC">
<contactref element="DS1307" pad="8"/>
<contactref element="R3" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="PICONN" pad="1"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="CR1220" pad="+2"/>
<contactref element="DS1307" pad="3"/>
</signal>
<signal name="N$2">
<contactref element="DS1307" pad="1"/>
<contactref element="32.768KHZ" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="DS1307" pad="2"/>
<contactref element="32.768KHZ" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="U1" pad="13"/>
<contactref element="PICONN" pad="22"/>
</signal>
<signal name="N$4">
<contactref element="PICONN" pad="20"/>
<contactref element="U1" pad="14"/>
</signal>
<signal name="N$6">
<contactref element="PICONN" pad="23"/>
<contactref element="U1" pad="15"/>
</signal>
<signal name="N$7">
<contactref element="U1" pad="12"/>
<contactref element="PICONN" pad="24"/>
</signal>
<signal name="N$10">
<contactref element="J1" pad="P$3"/>
<contactref element="U1" pad="10"/>
</signal>
<signal name="N$11">
<contactref element="PICONN" pad="21"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="SDL">
<contactref element="R4" pad="2"/>
<contactref element="PICONN" pad="6"/>
<contactref element="DS1307" pad="6"/>
</signal>
<signal name="SDA">
<contactref element="DS1307" pad="5"/>
<contactref element="PICONN" pad="4"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="3.3V">
<contactref element="U1" pad="8"/>
<contactref element="PICONN" pad="2"/>
</signal>
<signal name="3.3V2">
<contactref element="PICONN" pad="18"/>
</signal>
<signal name="5V">
<contactref element="PICONN" pad="3"/>
</signal>
<signal name="GND2">
<contactref element="PICONN" pad="5"/>
</signal>
<signal name="GND3">
<contactref element="PICONN" pad="10"/>
</signal>
<signal name="GND4">
<contactref element="PICONN" pad="13"/>
</signal>
<signal name="N$12">
<contactref element="PICONN" pad="19"/>
</signal>
<signal name="GND5">
<contactref element="PICONN" pad="26"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
