<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="10.25" y2="0" width="0" layer="20"/>
<wire x1="10.25" y1="0" x2="10.25" y2="10.25" width="0" layer="20"/>
<wire x1="10.25" y1="10.25" x2="0" y2="10.25" width="0" layer="20"/>
<wire x1="0" y1="10.25" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SO08">
<description>&lt;p&gt;8-pin SOIC package&lt;/p&gt;</description>
</package>
<package name="DIP08">
<description>&lt;b&gt;Dual In Line&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="SparkFun-DigitalIC" package="SO08" value="ATTINY13SOIC"/>
<element name="U2" library="SparkFun-DigitalIC" package="DIP08" value="TINY45-20-DIP">
<attribute name="PROD_ID" value="IC-09439"/>
</element>
</elements>
<signals>
<signal name="VCC">
<contactref element="U$1" pad="8"/>
<contactref element="U2" pad="8"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="4"/>
<contactref element="U2" pad="4"/>
</signal>
<signal name="N$1">
<contactref element="U2" pad="5"/>
<contactref element="U$1" pad="5"/>
</signal>
<signal name="N$2">
<contactref element="U$1" pad="6"/>
<contactref element="U2" pad="6"/>
</signal>
<signal name="N$3">
<contactref element="U2" pad="7"/>
<contactref element="U$1" pad="7"/>
</signal>
<signal name="N$4">
<contactref element="U$1" pad="2"/>
<contactref element="U2" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="U2" pad="3"/>
<contactref element="U$1" pad="3"/>
</signal>
<signal name="N$6">
<contactref element="U$1" pad="1"/>
<contactref element="U2" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
