<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="101.58" y1="0" x2="101.58" y2="32.69" width="0" layer="20"/>
<wire x1="101.58" y1="32.69" x2="0" y2="32.69" width="0" layer="20"/>
<wire x1="0" y1="32.69" x2="0" y2="0" width="0" layer="20"/>
<wire x1="60.96" y1="11.43" x2="72.39" y2="11.43" width="0.0254" layer="20"/>
<wire x1="72.39" y1="11.43" x2="72.39" y2="12.7" width="0.0254" layer="20"/>
<wire x1="72.39" y1="12.7" x2="60.96" y2="12.7" width="0.0254" layer="20"/>
<wire x1="60.96" y1="12.7" x2="60.96" y2="11.43" width="0.0254" layer="20"/>
<wire x1="72.39" y1="10.795" x2="72.39" y2="3.81" width="0.0254" layer="20"/>
<wire x1="72.39" y1="3.81" x2="73.66" y2="3.81" width="0.0254" layer="20"/>
<wire x1="73.66" y1="3.81" x2="73.66" y2="10.795" width="0.0254" layer="20"/>
<wire x1="73.66" y1="10.795" x2="72.39" y2="10.795" width="0.0254" layer="20"/>
<wire x1="0" y1="0" x2="101.6" y2="0" width="0" layer="20"/>
<text>(C) 2015 http://www.pasadenaghosthunters.org/</text>
<text>(C) 2015 http://www.pasadenaghosthunters.org/</text>
</plain>
<libraries>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
<package name="SO016">
</package>
<package name="SSOP28DB">
<description>&lt;b&gt;Small Shrink Outline Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="0jeffk512">
<description>Jeff's Parts</description>
<packages>
<package name="CSTCE">
<description>Murata Resonator</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-RES">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-CAP">
</package>
<package name="EIA3216">
</package>
<package name="NIC_10X10.5_CAP">
</package>
</packages>
</library>
<library name="SparkFun-FreqCtrl">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find crystals and oscillators and other things that go "tick".&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SO08">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt; Fits JEDEC packages (narrow SOIC-8)</description>
</package>
</packages>
</library>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CRYSTAL-32KHZ-SMD">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="CR1220-SMD">
</package>
<package name="EG1213">
</package>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="MICRO-SD-SOCKET-PP">
</package>
<package name="USB-MINIB">
<description>&lt;b&gt;USB Series Mini-B Surface Mounted&lt;/b&gt;</description>
</package>
<package name="BC9VPC">
</package>
<package name="1X04">
</package>
<package name="JST-5-PTH-VERT">
</package>
</packages>
</library>
<library name="SparkFun-PowerIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find drivers, regulators, and amplifiers.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-0603">
</package>
<package name="WS2812B">
<description>&lt;b&gt;Intelligent control LED with integrated light source&lt;/b&gt;&lt;p&gt;
WS2812B&lt;br&gt;
source: http://www.world-semi.com/uploads/soft/130904/1_1500205981.pdf</description>
</package>
</packages>
</library>
<library name="burr-brown">
<description>&lt;b&gt;Burr-Brown Components&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT223">
<description>&lt;b&gt;Smal Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Sensors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find sensors- accelerometers, gyros, compasses, magnetometers, light sensors, imagers, temp sensors, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SHT1X">
<description>&lt;b&gt;SHT1x&lt;/b&gt;
Sensirion Humdity Sensor</description>
</package>
</packages>
</library>
<library name="_DENNIS">
<description>Dennis Personal collection of parts.
http://www.atmel.com/images/doc2549.pdf</description>
<packages>
<package name="SOIC-8">
<description>SOIP-8 or SOP-8 150mil package</description>
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SMA-DIODE">
<description>&lt;B&gt;Diode&lt;/B&gt;&lt;p&gt;
Basic SMA packaged diode. Good for reverse polarization protection. Common part #: MBRA140</description>
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-M">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="SparkFun-DigitalIC" package="TQFP32-08" value="ATMEGA328P_TQFP">
<attribute name="PROD_ID" value="IC-09069"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X1" library="0jeffk512" package="CSTCE" value="16Mhz">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0603-RES" value="10K">
<attribute name="PROD_ID" value="RES-00824"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="0603-CAP" value="0.1uF">
<attribute name="PROD_ID" value="CAP-00810"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0603-RES" value="10K">
<attribute name="PROD_ID" value="RES-00824"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0603-RES" value="10K">
<attribute name="PROD_ID" value="RES-07856"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="SparkFun-FreqCtrl" package="SO08" value="DS1307SO8">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="0603-RES" value="4.7K">
<attribute name="PROD_ID" value="RES-07857"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="0603-RES" value="4.7K">
<attribute name="PROD_ID" value="RES-07857"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="SparkFun" package="CRYSTAL-32KHZ-SMD" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BATT1" library="adafruit" package="CR1220-SMD" value="BATT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="SparkFun-Connectors" package="MICRO-SD-SOCKET-PP" value="USD-SOCKETNEW">
<attribute name="PROD_ID" value="CONN-07820"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U3" library="SparkFun-DigitalIC" package="SO016" value="HEX_CONVERTER">
<attribute name="PROD_ID" value="IC-09604"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0603-CAP" value="0.1uF">
<attribute name="PROD_ID" value="CAP-00810"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="0603-CAP" value="0.1uF">
<attribute name="PROD_ID" value="CAP-00810"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="0603-CAP" value="0.1uF">
<attribute name="PROD_ID" value="CAP-00810"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="SparkFun-Capacitors" package="0603-CAP" value="0.1uF">
<attribute name="PROD_ID" value="CAP-00810"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="SparkFun-PowerIC" package="SOT23-5" value="5V">
<attribute name="PROD_ID" value="VREG-00823"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$3" library="SparkFun-PowerIC" package="SOT23-5" value="3.3V/150mA">
<attribute name="PROD_ID" value="VREG-00822"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="SparkFun-Capacitors" package="EIA3216" value="10uF">
<attribute name="PROD_ID" value="CAP-00811"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="SparkFun-Capacitors" package="EIA3216" value="10uF">
<attribute name="PROD_ID" value="CAP-00811"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$4" library="SparkFun-Connectors" package="USB-MINIB" value="USB-MINIB-5PIN">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U4" library="SparkFun-DigitalIC" package="SSOP28DB" value="FT232RL-BASICSSOP">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="SparkFun-LED" package="LED-0603" value="RED">
<attribute name="PROD_ID" value="DIO-00819"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="SparkFun-LED" package="LED-0603" value="GREEN">
<attribute name="PROD_ID" value="DIO-00821"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="SparkFun-Resistors" package="0603-RES" value="330">
<attribute name="PROD_ID" value="RES-00818"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="SparkFun-Resistors" package="0603-RES" value="330">
<attribute name="PROD_ID" value="RES-00818"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BAT1" library="SparkFun-Connectors" package="BC9VPC" value="">
<attribute name="PROD_ID" value="BATT-10855"/>
</element>
<element name="S1" library="adafruit" package="EG1213" value="EG1213">
<attribute name="NAME"/>
</element>
<element name="C8" library="SparkFun-Capacitors" package="NIC_10X10.5_CAP" value="220uf">
<attribute name="PROD_ID" value="CAP-08362"/>
</element>
<element name="C9" library="SparkFun-Capacitors" package="0603-CAP" value="0.1uF">
<attribute name="PROD_ID" value="CAP-00810"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="SparkFun-LED" package="WS2812B" value="">
<attribute name="PROD_ID" value="DIO-12503"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D4" library="SparkFun-LED" package="WS2812B" value="">
<attribute name="PROD_ID" value="DIO-12503"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D5" library="SparkFun-LED" package="WS2812B" value="">
<attribute name="PROD_ID" value="DIO-12503"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D6" library="SparkFun-LED" package="WS2812B" value="">
<attribute name="PROD_ID" value="DIO-12503"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D7" library="SparkFun-LED" package="WS2812B" value="">
<attribute name="PROD_ID" value="DIO-12503"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="SparkFun-Resistors" package="0603-RES" value="10K">
<attribute name="PROD_ID" value="RES-00824"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="burr-brown" package="SOT223" value="REG1118">
<attribute name="OC_NEWARK" value="14M2185"/>
<attribute name="MPN" value="REG1118-2.85/2K5G4"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="SparkFun-Capacitors" package="0603-CAP" value="470pF">
<attribute name="PROD_ID" value="CAP-07884"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="SparkFun-Capacitors" package="0603-CAP" value="470pF">
<attribute name="PROD_ID" value="CAP-07884"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="SparkFun-Resistors" package="0603-RES" value="10K">
<attribute name="PROD_ID" value="RES-00824"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="JST-5-PTH-VERT" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$5" library="SparkFun-Sensors" package="SHT1X" value="SHT1XSMD">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C12" library="SparkFun-Capacitors" package="0603-CAP" value="0.1uF">
<attribute name="PROD_ID" value="CAP-00810"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="SparkFun-Resistors" package="0603-RES" value="4.7K">
<attribute name="PROD_ID" value="RES-07857"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="SparkFun-Resistors" package="0603-RES" value="4.7K">
<attribute name="PROD_ID" value="RES-07857"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="SparkFun-Resistors" package="0603-RES" value="330">
<attribute name="PROD_ID" value="RES-00818"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="SparkFun-Resistors" package="0603-RES" value="330">
<attribute name="PROD_ID" value="RES-00818"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC3" library="_DENNIS" package="SOIC-8" value="DS18B20Z">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="Q2" library="adafruit" package="SOT23" value="BSH103"/>
<element name="D8" library="SparkFun-DiscreteSemi" package="SMA-DIODE" value="MBRA140T3G"/>
<element name="LOGO1" library="SparkFun-Aesthetics" package="OSHW-LOGO-M" value="OSHW-LOGOM"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="X1" pad="3"/>
<contactref element="U1" pad="7"/>
</signal>
<signal name="N$2">
<contactref element="U1" pad="8"/>
<contactref element="X1" pad="1"/>
</signal>
<signal name="GND">
<contactref element="X1" pad="2"/>
<contactref element="U1" pad="21"/>
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="5"/>
<contactref element="C1" pad="2"/>
<contactref element="R3" pad="1"/>
<contactref element="U$1" pad="4"/>
<contactref element="BATT1" pad="-"/>
<contactref element="U2" pad="6"/>
<contactref element="U2" pad="GND3"/>
<contactref element="U2" pad="CD1"/>
<contactref element="U2" pad="GND1"/>
<contactref element="U2" pad="CD2"/>
<contactref element="U3" pad="8"/>
<contactref element="C3" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C5" pad="1"/>
<contactref element="U$3" pad="2"/>
<contactref element="U$2" pad="2"/>
<contactref element="C6" pad="C"/>
<contactref element="C7" pad="C"/>
<contactref element="U$4" pad="MTN3"/>
<contactref element="U$4" pad="MTN1"/>
<contactref element="U$4" pad="MTN4"/>
<contactref element="U$4" pad="MTN2"/>
<contactref element="U$4" pad="GND"/>
<contactref element="U4" pad="25"/>
<contactref element="U4" pad="7"/>
<contactref element="U4" pad="18"/>
<contactref element="U4" pad="21"/>
<contactref element="BAT1" pad="V-"/>
<contactref element="C8" pad="-"/>
<contactref element="C9" pad="2"/>
<contactref element="U4" pad="26"/>
<contactref element="D3" pad="3"/>
<contactref element="D7" pad="3"/>
<contactref element="D6" pad="3"/>
<contactref element="D4" pad="3"/>
<contactref element="R8" pad="2"/>
<contactref element="D5" pad="3"/>
<contactref element="IC1" pad="2"/>
<contactref element="IC1" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="JP1" pad="2"/>
<contactref element="JP2" pad="5"/>
<contactref element="U$5" pad="1"/>
<contactref element="U$5" pad="1"/>
<contactref element="C12" pad="1"/>
<contactref element="IC3" pad="5"/>
<contactref element="IC3" pad="5"/>
</signal>
<signal name="VCC">
<contactref element="U1" pad="6"/>
<contactref element="U1" pad="4"/>
<contactref element="U1" pad="18"/>
<contactref element="R1" pad="2"/>
<contactref element="U$1" pad="8"/>
<contactref element="R5" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="U$3" pad="3"/>
<contactref element="U$3" pad="1"/>
<contactref element="U$2" pad="5"/>
<contactref element="U$4" pad="VBUS"/>
<contactref element="U4" pad="20"/>
<contactref element="R6" pad="1"/>
<contactref element="R7" pad="1"/>
<contactref element="U4" pad="4"/>
<contactref element="R9" pad="2"/>
<contactref element="JP1" pad="1"/>
<contactref element="IC3" pad="3"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="29"/>
<contactref element="R1" pad="1"/>
<contactref element="C4" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="U1" pad="20"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="BATTERYLEVEL">
<contactref element="R2" pad="1"/>
<contactref element="U1" pad="22"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="RAW">
<contactref element="U$2" pad="3"/>
<contactref element="U$2" pad="1"/>
<contactref element="C6" pad="A"/>
<contactref element="IC1" pad="3"/>
<contactref element="JP2" pad="1"/>
<contactref element="Q2" pad="2"/>
<contactref element="D8" pad="C"/>
</signal>
<signal name="SCK">
<contactref element="U1" pad="17"/>
<contactref element="U3" pad="7"/>
</signal>
<signal name="MISO">
<contactref element="U1" pad="16"/>
<contactref element="U2" pad="7"/>
</signal>
<signal name="MOSI">
<contactref element="U1" pad="15"/>
<contactref element="U3" pad="5"/>
</signal>
<signal name="CS">
<contactref element="U1" pad="14"/>
<contactref element="U3" pad="3"/>
</signal>
<signal name="X_SENSE">
<contactref element="U1" pad="23"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="Y_SENSE">
<contactref element="U1" pad="24"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="Z_SENSE">
<contactref element="U1" pad="25"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="SDA">
<contactref element="U1" pad="27"/>
<contactref element="U$1" pad="5"/>
<contactref element="R5" pad="1"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="SCL">
<contactref element="U1" pad="28"/>
<contactref element="U$1" pad="6"/>
<contactref element="R4" pad="1"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="N$10">
<contactref element="Q1" pad="X2"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="U$1" pad="2"/>
<contactref element="Q1" pad="X1"/>
</signal>
<signal name="N$12">
<contactref element="BATT1" pad="+$1"/>
<contactref element="BATT1" pad="+$2"/>
<contactref element="U$1" pad="3"/>
</signal>
<signal name="3.3V">
<contactref element="U2" pad="4"/>
<contactref element="C2" pad="1"/>
<contactref element="U3" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="U$3" pad="5"/>
<contactref element="C7" pad="A"/>
<contactref element="U$5" pad="4"/>
<contactref element="C12" pad="2"/>
<contactref element="R10" pad="2"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="U3" pad="2"/>
<contactref element="U2" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="U2" pad="3"/>
<contactref element="U3" pad="4"/>
</signal>
<signal name="N$9">
<contactref element="U3" pad="6"/>
<contactref element="U2" pad="5"/>
</signal>
<signal name="DTR">
<contactref element="C4" pad="1"/>
<contactref element="U4" pad="2"/>
</signal>
<signal name="N$18">
<contactref element="U$4" pad="D+"/>
<contactref element="U4" pad="15"/>
</signal>
<signal name="N$19">
<contactref element="U4" pad="16"/>
<contactref element="U$4" pad="D-"/>
</signal>
<signal name="LEDNET">
<contactref element="U1" pad="11"/>
<contactref element="D3" pad="4"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="9V">
<contactref element="BAT1" pad="V+"/>
<contactref element="S1" pad="2"/>
<contactref element="Q2" pad="3"/>
</signal>
<signal name="N$6">
<contactref element="R6" pad="2"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="N$14">
<contactref element="D1" pad="C"/>
<contactref element="U4" pad="22"/>
</signal>
<signal name="N$15">
<contactref element="U4" pad="23"/>
<contactref element="D2" pad="C"/>
</signal>
<signal name="N$16">
<contactref element="D2" pad="A"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="U4" pad="17"/>
<contactref element="C9" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="D3" pad="2"/>
<contactref element="D4" pad="4"/>
</signal>
<signal name="N$20">
<contactref element="D4" pad="2"/>
<contactref element="D5" pad="4"/>
</signal>
<signal name="N$21">
<contactref element="D5" pad="2"/>
<contactref element="D6" pad="4"/>
</signal>
<signal name="N$22">
<contactref element="D6" pad="2"/>
<contactref element="D7" pad="4"/>
</signal>
<signal name="N$24">
<contactref element="D3" pad="1"/>
<contactref element="IC1" pad="1"/>
<contactref element="D4" pad="1"/>
<contactref element="D5" pad="1"/>
<contactref element="D6" pad="1"/>
<contactref element="D7" pad="1"/>
</signal>
<signal name="N$23">
<contactref element="U$2" pad="4"/>
<contactref element="C11" pad="1"/>
</signal>
<signal name="N$25">
<contactref element="U$3" pad="4"/>
<contactref element="C10" pad="1"/>
</signal>
<signal name="TXO">
<contactref element="U1" pad="31"/>
<contactref element="U4" pad="5"/>
</signal>
<signal name="RXI">
<contactref element="U1" pad="30"/>
<contactref element="U4" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="U1" pad="13"/>
<contactref element="R9" pad="1"/>
<contactref element="IC3" pad="4"/>
</signal>
<signal name="N$26">
<contactref element="U$5" pad="2"/>
<contactref element="R10" pad="1"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="N$27">
<contactref element="U$5" pad="3"/>
<contactref element="R11" pad="1"/>
<contactref element="R12" pad="2"/>
</signal>
<signal name="H_DATA">
<contactref element="R13" pad="2"/>
<contactref element="U1" pad="10"/>
</signal>
<signal name="H_CLK">
<contactref element="R12" pad="1"/>
<contactref element="U1" pad="9"/>
</signal>
<signal name="PWR">
<contactref element="U1" pad="12"/>
<contactref element="Q2" pad="1"/>
</signal>
<signal name="POWER_SENSE">
<contactref element="R2" pad="2"/>
<contactref element="C8" pad="+"/>
<contactref element="S1" pad="3"/>
<contactref element="D8" pad="A"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
