<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.2">
<drawing>
<board>
<plain>
<circle x="15.24" y="13.97" radius="13.500284375" width="0.254" layer="20"/>
<text>LED</text>
<text>Power Ring</text>
<text>Citizen </text>
<text>Scientific</text>
<text>Workshop</text>
<text>Design by David Ultis</text>
</plain>
<libraries>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="BATTCOM_20MM_PTH">
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X02/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="LED5MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, round</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="BAT1" library="SparkFun-Electromechanical" package="BATTCOM_20MM_PTH" value=""/>
<element name="BUTTON" library="pinhead" package="1X02/90" value=""/>
<element name="LED1" library="adafruit" package="LED5MM" value=""/>
</elements>
<signals>
<signal name="N$2">
<contactref element="BUTTON" pad="2"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$3">
<contactref element="LED1" pad="K"/>
<contactref element="BAT1" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="BUTTON" pad="1"/>
<contactref element="BAT1" pad="1"/>
</signal>
<signal name="GND">
</signal>
</signals>
</board>
</drawing>
</eagle>
