<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="31.166" y2="0" width="0" layer="20"/>
<wire x1="31.166" y1="0" x2="31.166" y2="20.818" width="0" layer="20"/>
<wire x1="31.166" y1="20.818" x2="0" y2="20.818" width="0" layer="20"/>
<wire x1="0" y1="20.818" x2="0" y2="0" width="0" layer="20"/>
<text>GND</text>
<text>VCC</text>
<text>TDO</text>
<text>TDI</text>
<text>TMS</text>
<text>TCK</text>
<text>TEST
TARGET
DEBUG
BOARD</text>
</plain>
<libraries>
<library name="aray">
<packages>
<package name="SO24W">
<description>&lt;b&gt;Wide Small Outline package&lt;/b&gt; 300 mil</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X04">
</package>
<package name="1X01">
</package>
<package name="1X02">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="aray" package="SO24W" value="BCT8244A">
<attribute name="VALUE"/>
</element>
<element name="1A" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="2A" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="1Y" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="2Y" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="1O" library="SparkFun-Connectors" package="1X01" value="M01PTH">
<attribute name="NAME"/>
</element>
<element name="2O" library="SparkFun-Connectors" package="1X01" value="M01PTH">
<attribute name="NAME"/>
</element>
<element name="PWR1" library="SparkFun-Connectors" package="1X02" value="M02PTH"/>
<element name="JTAG" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="1Y1">
<contactref element="U$1" pad="2"/>
<contactref element="1Y" pad="1"/>
</signal>
<signal name="1Y2">
<contactref element="U$1" pad="3"/>
<contactref element="1Y" pad="2"/>
</signal>
<signal name="1Y3">
<contactref element="U$1" pad="4"/>
<contactref element="1Y" pad="3"/>
</signal>
<signal name="1Y4">
<contactref element="U$1" pad="5"/>
<contactref element="1Y" pad="4"/>
</signal>
<signal name="2Y1">
<contactref element="U$1" pad="7"/>
<contactref element="2Y" pad="1"/>
</signal>
<signal name="2Y2">
<contactref element="U$1" pad="8"/>
<contactref element="2Y" pad="2"/>
</signal>
<signal name="2Y3">
<contactref element="U$1" pad="9"/>
<contactref element="2Y" pad="3"/>
</signal>
<signal name="2Y4">
<contactref element="U$1" pad="10"/>
<contactref element="2Y" pad="4"/>
</signal>
<signal name="2A4">
<contactref element="2A" pad="1"/>
<contactref element="U$1" pad="15"/>
</signal>
<signal name="2A3">
<contactref element="2A" pad="2"/>
<contactref element="U$1" pad="16"/>
</signal>
<signal name="2A2">
<contactref element="2A" pad="3"/>
<contactref element="U$1" pad="17"/>
</signal>
<signal name="2A1">
<contactref element="2A" pad="4"/>
<contactref element="U$1" pad="19"/>
</signal>
<signal name="1A4">
<contactref element="1A" pad="1"/>
<contactref element="U$1" pad="20"/>
</signal>
<signal name="1A3">
<contactref element="1A" pad="2"/>
<contactref element="U$1" pad="21"/>
</signal>
<signal name="1A2">
<contactref element="1A" pad="3"/>
<contactref element="U$1" pad="22"/>
</signal>
<signal name="1A1">
<contactref element="1A" pad="4"/>
<contactref element="U$1" pad="23"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="6"/>
<contactref element="PWR1" pad="1"/>
</signal>
<signal name="1OE_L">
<contactref element="U$1" pad="1"/>
<contactref element="1O" pad="1"/>
</signal>
<signal name="2OE_L">
<contactref element="U$1" pad="24"/>
<contactref element="2O" pad="1"/>
</signal>
<signal name="TDO">
<contactref element="U$1" pad="11"/>
<contactref element="JTAG" pad="1"/>
</signal>
<signal name="5V">
<contactref element="U$1" pad="18"/>
<contactref element="PWR1" pad="2"/>
</signal>
<signal name="TCK">
<contactref element="U$1" pad="13"/>
<contactref element="JTAG" pad="4"/>
</signal>
<signal name="TMS">
<contactref element="U$1" pad="12"/>
<contactref element="JTAG" pad="3"/>
</signal>
<signal name="TDI">
<contactref element="U$1" pad="14"/>
<contactref element="JTAG" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
