<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="76.124" y2="0" width="0" layer="20"/>
<wire x1="76.124" y1="0" x2="76.124" y2="43.17" width="0" layer="20"/>
<wire x1="76.124" y1="43.17" x2="0" y2="43.17" width="0" layer="20"/>
<wire x1="0" y1="43.17" x2="0" y2="0" width="0" layer="20"/>
<text>5V</text>
<text>GND</text>
<text>SERVO_V</text>
<text>/Users/joe/Desktop/soldercat.bmp</text>
<text>/Users/joe/Desktop/soldercat.bmp</text>
<text>/Users/joe/Desktop/soldercat.bmp</text>
<text>/Users/joe/Desktop/soldercat.bmp</text>
<text>12-SERVO</text>
<text>LP-SERVO12 1.1</text>
<text>KROESCHE.ORG</text>
<text>BAT+</text>
<text>6V-12V</text>
<text>5V/5A MAX</text>
<text>STELLARIS</text>
<text>BOOSTERPACK</text>
<text>2013-02</text>
<text>1. CONN X1 IS BATTERY INPUT</text>
<text>NOTES:</text>
<text>-----</text>
<text>6-12V</text>
<text>2. ONBOARD SUPPLY IS 5V/5A</text>
<text>3. JP1 BRIDGED TO POWER</text>
<text>LAUNCHPAD+SERVOS</text>
<text>4. JP1 OPEN TO POWER SERVOS</text>
<text>ONLY</text>
<text>5. J10 FOR SEPARATE</text>
<text>LAUNCHPAD SUPPLY (5V)</text>
<text>6. SxA/B &lt;-&gt; WIDE TIMER xA/B</text>
<text>Copyright (c) 2013 by Joe Kroesche (kroesche.org)
All rights reserved.</text>
<text>This work is licensed under the
Creative Commons Attribution 3.0 Unported License.
To view a copy of this license, visit
http://creativecommons.org/licenses/by/3.0/.</text>
</plain>
<libraries>
<library name="con-molex">
<description>&lt;b&gt;Molex Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="KK-156-2">
<description>&lt;b&gt;KK 156 HEADER&lt;/b&gt;&lt;p&gt;
Source: http://www.molex.com/pdm_docs/sd/026604100_sd.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="STAND-OFF">
<description>&lt;b&gt;Stand Off&lt;/b&gt;&lt;p&gt;
This is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components. SKU : PRT-00447</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02">
</package>
<package name="1X03">
</package>
<package name="EIA3216">
</package>
<package name="0805">
</package>
<package name="1210">
</package>
<package name="1206">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X10">
</package>
</packages>
</library>
<library name="SparkFun-AnalogIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of analog ICs- DACs, ADCs, video chips, op-amps, and others.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SO08">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt; Fits JEDEC packages (narrow SOIC-8)</description>
</package>
</packages>
</library>
<library name="ohw-logo">
<packages>
<package name="OSHW_6X200_NOTEXT">
</package>
</packages>
</library>
<library name="kroesche">
<description>Custom library used for kroesche.org projects</description>
<packages>
<package name="PWP-R-PDSO-G14">
</package>
<package name="VISHAY-IHLP3232DZER">
<description>Vishay-Dale IHLP-3232DZ-11 Inductor Package</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="X1" library="con-molex" package="KK-156-2" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MANF" value="Molex"/>
<attribute name="MANF#" value="76650-0208"/>
<attribute name="MOUSER#" value="538-76650-0208"/>
<attribute name="PARTNO" value="KK-156-2-LOCK-RTANGLE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0805" value="220">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MANF" value="Panasonic"/>
<attribute name="MANF#" value="ERJ-6GEYJ221V"/>
<attribute name="MOUSER#" value="667-ERJ-6GEYJ221V"/>
<attribute name="PARTNO" value="RES_220_20V_10PCT_0805"/>
<attribute name="TOL" value="10%"/>
<attribute name="VOLT" value="50V"/>
<attribute name="SIZE" value="(0805)"/>
</element>
<element name="STANDOFF1" library="SparkFun-Electromechanical" package="STAND-OFF" value="STAND-OFF">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="STANDOFF2" library="SparkFun-Electromechanical" package="STAND-OFF" value="STAND-OFF">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="STANDOFF3" library="SparkFun-Electromechanical" package="STAND-OFF" value="STAND-OFF">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="STANDOFF4" library="SparkFun-Electromechanical" package="STAND-OFF" value="STAND-OFF">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="JP1" library="SparkFun-Passives" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNO" value="68002-202HLF"/>
</element>
<element name="J10" library="SparkFun-Passives" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNO" value="68016-402"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0805" value="220">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNO" value="RES_220_20V_10PCT_0805"/>
<attribute name="SIZE" value="(0805)"/>
<attribute name="VOLT" value="50V"/>
<attribute name="TOL" value="10%"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0805" value="220">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNO" value="RES_220_20V_10PCT_0805"/>
<attribute name="SIZE" value="(0805)"/>
<attribute name="TOL" value="10%"/>
<attribute name="VOLT" value="50V"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="0805" value="220">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNO" value="RES_220_20V_10PCT_0805"/>
<attribute name="SIZE" value="(0805)"/>
<attribute name="TOL" value="10%"/>
<attribute name="VOLT" value="50V"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="0805" value="220">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNO" value="RES_220_20V_10PCT_0805"/>
<attribute name="SIZE" value="(0805)"/>
<attribute name="TOL" value="10%"/>
<attribute name="VOLT" value="50V"/>
</element>
<element name="R6" library="SparkFun-Resistors" package="0805" value="220">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNO" value="RES_220_20V_10PCT_0805"/>
<attribute name="SIZE" value="(0805)"/>
<attribute name="TOL" value="10%"/>
<attribute name="VOLT" value="50V"/>
</element>
<element name="R7" library="SparkFun-Resistors" package="0805" value="220">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNO" value="RES_220_20V_10PCT_0805"/>
<attribute name="SIZE" value="(0805)"/>
<attribute name="TOL" value="10%"/>
<attribute name="VOLT" value="50V"/>
</element>
<element name="R8" library="SparkFun-Resistors" package="0805" value="220">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNO" value="RES_220_20V_10PCT_0805"/>
<attribute name="SIZE" value="(0805)"/>
<attribute name="TOL" value="10%"/>
<attribute name="VOLT" value="50V"/>
</element>
<element name="R9" library="SparkFun-Resistors" package="0805" value="220">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNO" value="RES_220_20V_10PCT_0805"/>
<attribute name="SIZE" value="(0805)"/>
<attribute name="TOL" value="10%"/>
<attribute name="VOLT" value="50V"/>
</element>
<element name="R10" library="SparkFun-Resistors" package="0805" value="220">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNO" value="RES_220_20V_10PCT_0805"/>
<attribute name="SIZE" value="(0805)"/>
<attribute name="TOL" value="10%"/>
<attribute name="VOLT" value="50V"/>
</element>
<element name="R11" library="SparkFun-Resistors" package="0805" value="220">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNO" value="RES_220_20V_10PCT_0805"/>
<attribute name="SIZE" value="(0805)"/>
<attribute name="TOL" value="10%"/>
<attribute name="VOLT" value="50V"/>
</element>
<element name="R12" library="SparkFun-Resistors" package="0805" value="220">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNO" value="RES_220_20V_10PCT_0805"/>
<attribute name="SIZE" value="(0805)"/>
<attribute name="TOL" value="10%"/>
<attribute name="VOLT" value="50V"/>
</element>
<element name="S4A" library="SparkFun-Passives" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNO" value="68002-403HLF"/>
</element>
<element name="S4B" library="SparkFun-Passives" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNO" value="68002-403HLF"/>
</element>
<element name="S2A" library="SparkFun-Passives" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNO" value="68002-403HLF"/>
</element>
<element name="S2B" library="SparkFun-Passives" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNO" value="68002-403HLF"/>
</element>
<element name="S3A" library="SparkFun-Passives" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNO" value="68002-403HLF"/>
</element>
<element name="S3B" library="SparkFun-Passives" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNO" value="68002-403HLF"/>
</element>
<element name="J5" library="SparkFun-Passives" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNO" value="68002-202HLF"/>
</element>
<element name="S0A" library="SparkFun-Passives" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNO" value="68002-403HLF"/>
</element>
<element name="S0B" library="SparkFun-Passives" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNO" value="68002-403HLF"/>
</element>
<element name="S1A" library="SparkFun-Passives" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNO" value="68002-403HLF"/>
</element>
<element name="S1B" library="SparkFun-Passives" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNO" value="68002-403HLF"/>
</element>
<element name="S5A" library="SparkFun-Passives" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNO" value="68002-403HLF"/>
</element>
<element name="S5B" library="SparkFun-Passives" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNO" value="68002-403HLF"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X10" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNO" value="68002-110HLF"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="1X10" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNO" value="68002-110HLF"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X10" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNO" value="68002-110HLF"/>
</element>
<element name="J4" library="SparkFun-Connectors" package="1X10" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNO" value="68002-110HLF"/>
</element>
<element name="C1" library="SparkFun-Passives" package="EIA3216" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNO" value="CAP_10u_20V_20PCT_1206"/>
<attribute name="TOL" value="20%"/>
<attribute name="VOLT" value="20V"/>
<attribute name="SIZE" value="(1206)"/>
<attribute name="TYPE" value="TANT"/>
</element>
<element name="C2" library="SparkFun-Passives" package="EIA3216" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNO" value="CAP_10u_20V_20PCT_1206"/>
<attribute name="TOL" value="20%"/>
<attribute name="VOLT" value="20V"/>
<attribute name="SIZE" value="(1206)"/>
<attribute name="TYPE" value="TANT"/>
</element>
<element name="C3" library="SparkFun-Passives" package="EIA3216" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNO" value="CAP_10u_20V_20PCT_1206"/>
<attribute name="TOL" value="20%"/>
<attribute name="VOLT" value="20V"/>
<attribute name="SIZE" value="(1206)"/>
<attribute name="TYPE" value="TANT"/>
</element>
<element name="C4" library="SparkFun-Passives" package="0805" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNO" value="CAP_1u_20V_20PCT_0805"/>
<attribute name="TOL" value="20%"/>
<attribute name="VOLT" value="20V"/>
<attribute name="SIZE" value="(0805)"/>
</element>
<element name="C5" library="SparkFun-Passives" package="0805" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNO" value="CAP_1u_20V_20PCT_0805"/>
<attribute name="TOL" value="20%"/>
<attribute name="VOLT" value="20V"/>
<attribute name="SIZE" value="(0805)"/>
</element>
<element name="C6" library="SparkFun-Passives" package="0805" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNO" value="CAP_1u_20V_20PCT_0805"/>
<attribute name="TOL" value="20%"/>
<attribute name="VOLT" value="20V"/>
<attribute name="SIZE" value="(0805)"/>
</element>
<element name="U1" library="kroesche" package="PWP-R-PDSO-G14" value="TPS54526PWP">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MOUSER#" value="595-TPS54526PWP"/>
<attribute name="MANF#" value="TPS54526PWP"/>
<attribute name="MANF" value="Texas Instruments"/>
<attribute name="PARTNO" value="TPS54526PWP"/>
</element>
<element name="L1" library="kroesche" package="VISHAY-IHLP3232DZER" value="3.3uH">
<attribute name="MOUSER#" value="70-IHLP3232DZER3R3M11"/>
<attribute name="MANF#" value="IHLP3232DZER3R3M11"/>
<attribute name="MANF" value="Vishay/Dale"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNO" value="IHLP3232DZER3R3M11"/>
<attribute name="TOL" value="20%"/>
<attribute name="LOAD" value="10A"/>
</element>
<element name="C7" library="SparkFun-Passives" package="0805" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNO" value="CAP_100n_25V_10PCT_0805"/>
<attribute name="SIZE" value="(0805)"/>
<attribute name="TOL" value="10%"/>
<attribute name="VOLT" value="25V"/>
<attribute name="TC" value="X7R"/>
</element>
<element name="C8" library="SparkFun-Passives" package="0805" value="22pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNO" value="CAP_22p_50V_10PCT_0805"/>
<attribute name="SIZE" value="(0805)"/>
<attribute name="TOL" value="10%"/>
<attribute name="VOLT" value="50V"/>
<attribute name="TC" value="C0G"/>
</element>
<element name="C9" library="SparkFun-Passives" package="1210" value="22uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNO" value="CAP_22u_16V_10PCT_1210"/>
<attribute name="SIZE" value="(1210)"/>
<attribute name="TOL" value="10%"/>
<attribute name="VOLT" value="16V"/>
<attribute name="TC" value="X5R"/>
</element>
<element name="C10" library="SparkFun-Passives" package="1206" value="22uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNO" value="CAP_22u_16V_20PCT_1206"/>
<attribute name="TOL" value="20%"/>
<attribute name="TC" value="X5R"/>
<attribute name="VOLT" value="16V"/>
<attribute name="SIZE" value="(1206)"/>
</element>
<element name="C11" library="SparkFun-Passives" package="0805" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNO" value="CAP_1u_20V_20PCT_0805"/>
<attribute name="SIZE" value="(0805)"/>
<attribute name="TOL" value="20%"/>
<attribute name="VOLT" value="20V"/>
</element>
<element name="C12" library="SparkFun-Passives" package="0805" value="10nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNO" value="CAP_10n_50V_10PCT_0805"/>
<attribute name="TOL" value="10%"/>
<attribute name="TC" value="X7R"/>
<attribute name="VOLT" value="50V"/>
<attribute name="SIZE" value="(0805)"/>
</element>
<element name="R13" library="SparkFun-Resistors" package="0805" value="124K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="TOL" value="1%"/>
<attribute name="VOLT" value="20V"/>
<attribute name="RATE" value="1/8W"/>
<attribute name="SIZE" value="(0805)"/>
<attribute name="PARTNO" value="RES_124K_20V_1PCT_0805"/>
</element>
<element name="R14" library="SparkFun-Resistors" package="0805" value="22.1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="TOL" value="1%"/>
<attribute name="VOLT" value="20V"/>
<attribute name="RATE" value="1/8W"/>
<attribute name="SIZE" value="(0805)"/>
<attribute name="PARTNO" value="RES_22.1K_20V_1PCT_0805"/>
</element>
<element name="R15" library="SparkFun-Resistors" package="0805" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNO" value="RES_100K_20V_1PCT_0805"/>
<attribute name="RATE" value="1/8W"/>
<attribute name="SIZE" value="(0805)"/>
<attribute name="TOL" value="1%"/>
<attribute name="VOLT" value="20V"/>
</element>
<element name="U2" library="SparkFun-AnalogIC" package="SO08" value="LMV358">
<attribute name="VALUE"/>
<attribute name="NAME"/>
<attribute name="MANF" value="Texas Instruments"/>
<attribute name="MANF#" value="LMV358QDR"/>
<attribute name="MOUSER#" value="595-LMV358QDR"/>
<attribute name="PARTNO" value="LMV358QDR"/>
</element>
<element name="R16" library="SparkFun-Resistors" package="0805" value="30K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="TOL" value="1%"/>
<attribute name="VOLT" value="20V"/>
<attribute name="SIZE" value="(0805)"/>
<attribute name="PARTNO" value="RES_30K_20V_1PCT_0805"/>
</element>
<element name="R17" library="SparkFun-Resistors" package="0805" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="TOL" value="1%"/>
<attribute name="VOLT" value="20V"/>
<attribute name="SIZE" value="(0805)"/>
<attribute name="PARTNO" value="RES_10K_20V_1PCT_0805"/>
</element>
<element name="R18" library="SparkFun-Resistors" package="0805" value="30K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="TOL" value="1%"/>
<attribute name="VOLT" value="20V"/>
<attribute name="SIZE" value="(0805)"/>
<attribute name="PARTNO" value="RES_30K_20V_1PCT_0805"/>
</element>
<element name="R19" library="SparkFun-Resistors" package="0805" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="TOL" value="1%"/>
<attribute name="VOLT" value="20V"/>
<attribute name="SIZE" value="(0805)"/>
<attribute name="PARTNO" value="RES_10K_20V_1PCT_0805"/>
</element>
<element name="R20" library="SparkFun-Resistors" package="0805" value="15K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="TOL" value="1%"/>
<attribute name="VOLT" value="20V"/>
<attribute name="SIZE" value="(0805)"/>
<attribute name="PARTNO" value="RES_15K_20V_1PCT_0805"/>
</element>
<element name="R21" library="SparkFun-Resistors" package="0805" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="TOL" value="1%"/>
<attribute name="VOLT" value="20V"/>
<attribute name="SIZE" value="(0805)"/>
<attribute name="PARTNO" value="RES_10K_20V_1PCT_0805"/>
</element>
<element name="C13" library="SparkFun-Passives" package="0805" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNO" value="CAP_1u_20V_20PCT_0805"/>
<attribute name="TOL" value="20%"/>
<attribute name="VOLT" value="20V"/>
<attribute name="SIZE" value="(0805)"/>
</element>
<element name="C14" library="SparkFun-Passives" package="0805" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNO" value="CAP_1u_20V_20PCT_0805"/>
<attribute name="TOL" value="20%"/>
<attribute name="VOLT" value="20V"/>
<attribute name="SIZE" value="(0805)"/>
</element>
<element name="LOGO2" library="ohw-logo" package="OSHW_6X200_NOTEXT" value="OSHW_LOGO_6MILX0200-NT">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="R22" library="SparkFun-Resistors" package="0805" value="100K">
<attribute name="VOLT" value="20V"/>
<attribute name="RATE" value="1/8W"/>
<attribute name="SIZE" value="(0805)"/>
<attribute name="PARTNO" value="RES_100K_20V_1PCT_0805"/>
<attribute name="TOL" value="1%"/>
<attribute name="DATABASE" value="/Users/joe/Documents/Projects/tronics/boards/lp-servo12/bom/bomex-partsdb.txt"/>
</element>
</elements>
<signals>
<signal name="WT2A">
<contactref element="R3" pad="2"/>
<contactref element="J3" pad="3"/>
</signal>
<signal name="WT2B">
<contactref element="R4" pad="2"/>
<contactref element="J3" pad="4"/>
</signal>
<signal name="WT3A">
<contactref element="R5" pad="2"/>
<contactref element="J3" pad="5"/>
</signal>
<signal name="WT3B">
<contactref element="R6" pad="2"/>
<contactref element="J3" pad="6"/>
</signal>
<signal name="WT0A">
<contactref element="R7" pad="1"/>
<contactref element="J4" pad="4"/>
</signal>
<signal name="WT0B">
<contactref element="R8" pad="1"/>
<contactref element="J4" pad="5"/>
</signal>
<signal name="WT1A">
<contactref element="R9" pad="1"/>
<contactref element="J4" pad="6"/>
</signal>
<signal name="WT1B">
<contactref element="R10" pad="1"/>
<contactref element="J4" pad="7"/>
</signal>
<signal name="WT5A">
<contactref element="R11" pad="1"/>
<contactref element="J4" pad="8"/>
</signal>
<signal name="WT5B">
<contactref element="R12" pad="1"/>
<contactref element="J4" pad="9"/>
</signal>
<signal name="WT4B">
<contactref element="R2" pad="2"/>
<contactref element="J5" pad="2"/>
</signal>
<signal name="GND">
<contactref element="J10" pad="1"/>
<contactref element="S4A" pad="1"/>
<contactref element="S4B" pad="1"/>
<contactref element="S2A" pad="1"/>
<contactref element="S2B" pad="1"/>
<contactref element="S3A" pad="1"/>
<contactref element="S3B" pad="1"/>
<contactref element="S0A" pad="3"/>
<contactref element="S0B" pad="3"/>
<contactref element="S1A" pad="3"/>
<contactref element="S1B" pad="3"/>
<contactref element="S5A" pad="3"/>
<contactref element="S5B" pad="3"/>
<contactref element="J3" pad="2"/>
<contactref element="J2" pad="1"/>
<contactref element="C1" pad="C"/>
<contactref element="C4" pad="2"/>
<contactref element="C2" pad="C"/>
<contactref element="C3" pad="C"/>
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="R14" pad="1"/>
<contactref element="C10" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="U1" pad="5"/>
<contactref element="U1" pad="15"/>
<contactref element="U1" pad="9"/>
<contactref element="U1" pad="8"/>
<contactref element="C9" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="R19" pad="1"/>
<contactref element="R21" pad="1"/>
<contactref element="C14" pad="2"/>
<contactref element="U2" pad="4"/>
<contactref element="U2" pad="4"/>
<contactref element="C13" pad="2"/>
<contactref element="X1" pad="1"/>
</signal>
<signal name="+5V">
<contactref element="J10" pad="2"/>
<contactref element="JP1" pad="2"/>
<contactref element="J3" pad="1"/>
<contactref element="C1" pad="A"/>
<contactref element="C4" pad="1"/>
<contactref element="R20" pad="2"/>
<contactref element="U2" pad="8"/>
<contactref element="C13" pad="1"/>
</signal>
<signal name="SERVO_V">
<contactref element="JP1" pad="1"/>
<contactref element="S4A" pad="2"/>
<contactref element="S4B" pad="2"/>
<contactref element="S2A" pad="2"/>
<contactref element="S2B" pad="2"/>
<contactref element="S3A" pad="2"/>
<contactref element="S3B" pad="2"/>
<contactref element="S0A" pad="2"/>
<contactref element="S0B" pad="2"/>
<contactref element="S1A" pad="2"/>
<contactref element="S1B" pad="2"/>
<contactref element="S5A" pad="2"/>
<contactref element="S5B" pad="2"/>
<contactref element="C2" pad="A"/>
<contactref element="C3" pad="A"/>
<contactref element="C5" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="L1" pad="1"/>
<contactref element="R13" pad="2"/>
<contactref element="C8" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="R1" pad="1"/>
<contactref element="S4A" pad="3"/>
</signal>
<signal name="N$3">
<contactref element="R2" pad="1"/>
<contactref element="S4B" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="R3" pad="1"/>
<contactref element="S2A" pad="3"/>
</signal>
<signal name="N$5">
<contactref element="R4" pad="1"/>
<contactref element="S2B" pad="3"/>
</signal>
<signal name="N$6">
<contactref element="R5" pad="1"/>
<contactref element="S3A" pad="3"/>
</signal>
<signal name="N$10">
<contactref element="R6" pad="1"/>
<contactref element="S3B" pad="3"/>
</signal>
<signal name="WT4A">
<contactref element="R1" pad="2"/>
<contactref element="J5" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="R7" pad="2"/>
<contactref element="S0A" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="R8" pad="2"/>
<contactref element="S0B" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="R9" pad="2"/>
<contactref element="S1A" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="R10" pad="2"/>
<contactref element="S1B" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="R11" pad="2"/>
<contactref element="S5A" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="R12" pad="2"/>
<contactref element="S5B" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="U1" pad="12"/>
<contactref element="C7" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="C7" pad="2"/>
<contactref element="U1" pad="10"/>
<contactref element="U1" pad="11"/>
<contactref element="L1" pad="2"/>
</signal>
<signal name="N$16">
<contactref element="R13" pad="1"/>
<contactref element="R14" pad="2"/>
<contactref element="U1" pad="2"/>
<contactref element="C8" pad="2"/>
</signal>
<signal name="VBAT">
<contactref element="U1" pad="13"/>
<contactref element="C9" pad="1"/>
<contactref element="U1" pad="14"/>
<contactref element="R18" pad="1"/>
<contactref element="R22" pad="1"/>
<contactref element="X1" pad="2"/>
</signal>
<signal name="N$20">
<contactref element="U1" pad="4"/>
<contactref element="C12" pad="1"/>
</signal>
<signal name="N$22">
<contactref element="R15" pad="1"/>
<contactref element="C11" pad="1"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="N$18">
<contactref element="U1" pad="6"/>
<contactref element="R15" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="R17" pad="2"/>
<contactref element="R16" pad="1"/>
<contactref element="U2" pad="6"/>
</signal>
<signal name="N$17">
<contactref element="R18" pad="2"/>
<contactref element="R19" pad="2"/>
<contactref element="U2" pad="5"/>
</signal>
<signal name="N$21">
<contactref element="R17" pad="1"/>
<contactref element="U2" pad="2"/>
<contactref element="U2" pad="1"/>
</signal>
<signal name="N$23">
<contactref element="R20" pad="1"/>
<contactref element="R21" pad="2"/>
<contactref element="U2" pad="3"/>
</signal>
<signal name="AIN2">
<contactref element="J3" pad="7"/>
<contactref element="R16" pad="2"/>
<contactref element="C14" pad="1"/>
<contactref element="U2" pad="7"/>
</signal>
<signal name="N$19">
<contactref element="U1" pad="7"/>
<contactref element="R22" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
