<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.0">
<drawing>
<board>
<plain>
<hole x="-2.54" y="5.08" drill="3.2"/>
<hole x="33.02" y="5.08" drill="3.2"/>
<hole x="-2.54" y="43.18" drill="3.2"/>
<hole x="33.02" y="43.18" drill="3.2"/>
<wire x1="-5.08" y1="2.54" x2="35.56" y2="2.54" width="0.4064" layer="20"/>
<wire x1="35.56" y1="2.54" x2="35.56" y2="45.72" width="0.4064" layer="20"/>
<wire x1="35.56" y1="45.72" x2="-5.08" y2="45.72" width="0.4064" layer="20"/>
<wire x1="-5.08" y1="45.72" x2="-5.08" y2="2.54" width="0.4064" layer="20"/>
<text>jamescadman.com</text>
<text>Jay_uk's RGB Shield</text>
<text>12v</text>
<text>+</text>
<text>R</text>
<text>G</text>
<text>B</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X04_LOCK">
</package>
<package name="SCREWTERMINAL-5MM-2">
</package>
</packages>
</library>
<library name="SparkFun-Boards">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find boards and modules: Arduino footprints, breadboards, non-RF modules, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="ARDUINO_MINI">
</package>
</packages>
</library>
<library name="linear">
<description>&lt;b&gt;Linear Devices&lt;/b&gt;&lt;p&gt;
Operational amplifiers,  comparators, voltage regulators, ADCs, DACs, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO220V">
<description>&lt;b&gt;TO 200 vertical&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="transistor-power">
<description>&lt;b&gt;Power Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO126AV">
<description>&lt;b&gt;Molded Package&lt;/b&gt;&lt;p&gt;
grid 2.3 mm</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="RGBSTRIP" library="SparkFun-Connectors" package="1X04_LOCK" value=""/>
<element name="U$1" library="SparkFun-Boards" package="ARDUINO_MINI" value="ARDUINO_MINI"/>
<element name="JP1" library="SparkFun-Connectors" package="SCREWTERMINAL-5MM-2" value="M025MM">
<attribute name="STOREFRONT_ID" value="PRT-08432"/>
</element>
<element name="IC1" library="linear" package="TO220V" value="7805TV"/>
<element name="Q1" library="transistor-power" package="TO126AV" value="BD139"/>
<element name="Q2" library="transistor-power" package="TO126AV" value="BD139"/>
<element name="Q3" library="transistor-power" package="TO126AV" value="BD139"/>
</elements>
<signals>
<signal name="VCC">
<contactref element="RGBSTRIP" pad="4"/>
<contactref element="JP1" pad="1"/>
<contactref element="IC1" pad="1"/>
</signal>
<signal name="GND">
<contactref element="JP1" pad="2"/>
<contactref element="IC1" pad="2"/>
<contactref element="U$1" pad="23"/>
<contactref element="Q1" pad="C"/>
<contactref element="Q2" pad="C"/>
<contactref element="Q3" pad="C"/>
</signal>
<signal name="N$1">
<contactref element="RGBSTRIP" pad="3"/>
<contactref element="Q1" pad="E"/>
</signal>
<signal name="N$2">
<contactref element="RGBSTRIP" pad="2"/>
<contactref element="Q2" pad="E"/>
</signal>
<signal name="N$3">
<contactref element="RGBSTRIP" pad="1"/>
<contactref element="Q3" pad="E"/>
</signal>
<signal name="N$4">
<contactref element="U$1" pad="8"/>
<contactref element="Q1" pad="B"/>
</signal>
<signal name="N$5">
<contactref element="U$1" pad="9"/>
<contactref element="Q2" pad="B"/>
</signal>
<signal name="N$6">
<contactref element="U$1" pad="6"/>
<contactref element="Q3" pad="B"/>
</signal>
<signal name="N$7">
<contactref element="U$1" pad="21"/>
<contactref element="IC1" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
