<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<text>AC 1.2A</text>
<text>+12V</text>
<text>+12V</text>
<text>GND</text>
<text>GND</text>
<text>DC12V</text>
<text>RF IR Automation Board V2
Scott Martin 7/2014</text>
<wire x1="0" y1="0" x2="54.61" y2="0" width="0.4064" layer="20"/>
<wire x1="54.61" y1="0" x2="54.61" y2="54.61" width="0.4064" layer="20"/>
<wire x1="54.61" y1="54.61" x2="0" y2="54.61" width="0.4064" layer="20"/>
<wire x1="0" y1="54.61" x2="0" y2="0" width="0.254" layer="20"/>
<hole x="5.08" y="5.08" drill="5.334"/>
<hole x="49.53" y="5.08" drill="5.334"/>
<hole x="49.53" y="36.83" drill="5.334"/>
<hole x="5.08" y="36.83" drill="5.334"/>
<text>GND</text>
<text>+12V</text>
<text>0 OHM
FOR IRQ-&gt;</text>
</plain>
<libraries>
<library name="SparkFun-Boards">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find boards and modules: Arduino footprints, breadboards, non-RF modules, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="ARDUINO_MINI">
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="CHIP-LED0603MP">
<description>&lt;b&gt;LED 0603&lt;/b&gt;&lt;p&gt;
micro-pitch</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="POWER_JACK_PTH_LOCK">
</package>
<package name="SCREWTERMINAL-3.5MM-2_LOCK">
</package>
<package name="1X12_LOCK">
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="RF_IR">
<packages>
<package name="8-SMD">
</package>
<package name="2X4">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-RES">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="D1" library="led" package="CHIP-LED0603MP" value="IR">
<attribute name="LABEL" value=""/>
<attribute name="NAME"/>
</element>
<element name="D2" library="led" package="CHIP-LED0603MP" value="IR">
<attribute name="LABEL" value=""/>
<attribute name="NAME"/>
</element>
<element name="D3" library="led" package="CHIP-LED0603MP" value="IR">
<attribute name="LABEL" value=""/>
<attribute name="NAME"/>
</element>
<element name="D4" library="led" package="CHIP-LED0603MP" value="IR">
<attribute name="LABEL" value=""/>
<attribute name="NAME"/>
</element>
<element name="D5" library="led" package="CHIP-LED0603MP" value="IR">
<attribute name="LABEL" value=""/>
<attribute name="NAME"/>
</element>
<element name="D6" library="led" package="CHIP-LED0603MP" value="IR">
<attribute name="LABEL" value=""/>
<attribute name="NAME"/>
</element>
<element name="D7" library="led" package="CHIP-LED0603MP" value="IR">
<attribute name="LABEL" value=""/>
<attribute name="NAME"/>
</element>
<element name="D8" library="led" package="CHIP-LED0603MP" value="IR">
<attribute name="LABEL" value=""/>
<attribute name="NAME"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="POWER_JACK_PTH_LOCK" value="POWER_JACKPTH_LOCK">
<attribute name="PROD_ID" value="PRT-00119"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-2_LOCK" value="M023.5MM_LOCK"/>
<element name="JP3" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-2_LOCK" value="M023.5MM_LOCK"/>
<element name="R6" library="SparkFun-Passives" package="0603-RES" value="39k">
<attribute name="NAME"/>
</element>
<element name="R7" library="SparkFun-Passives" package="0603-RES" value="39k">
<attribute name="NAME"/>
</element>
<element name="R8" library="SparkFun-Passives" package="0603-RES" value="39k">
<attribute name="NAME"/>
</element>
<element name="R9" library="SparkFun-Passives" package="0603-RES" value="180">
<attribute name="NAME"/>
</element>
<element name="U$4" library="SparkFun-Boards" package="ARDUINO_MINI" value="ARDUINO_MINI"/>
<element name="Q1" library="SparkFun-DiscreteSemi" package="SOT23" value="MOSFET-NCHANNELBSS138">
<attribute name="PROD_ID" value="TRANS-00830"/>
<attribute name="NAME"/>
</element>
<element name="Q2" library="SparkFun-DiscreteSemi" package="SOT23" value="MOSFET-NCHANNELBSS138">
<attribute name="PROD_ID" value="TRANS-00830"/>
<attribute name="NAME"/>
</element>
<element name="Q3" library="SparkFun-DiscreteSemi" package="SOT23" value="MOSFET-NCHANNELBSS138">
<attribute name="PROD_ID" value="TRANS-00830"/>
<attribute name="NAME"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-2_LOCK" value="M023.5MM_LOCK"/>
<element name="U$1" library="RF_IR" package="8-SMD" value="AQH3223A"/>
<element name="R5" library="SparkFun-Passives" package="0603-RES" value="560"/>
<element name="R1" library="SparkFun-Passives" package="0603-RES" value="560">
<attribute name="NAME"/>
</element>
<element name="R2" library="SparkFun-Passives" package="0603-RES" value="560">
<attribute name="NAME"/>
</element>
<element name="R10" library="SparkFun-Passives" package="0603-RES" value="560">
<attribute name="NAME"/>
</element>
<element name="R11" library="SparkFun-Passives" package="0603-RES" value="560">
<attribute name="NAME"/>
</element>
<element name="R12" library="SparkFun-Passives" package="0603-RES" value="560">
<attribute name="NAME"/>
</element>
<element name="R13" library="SparkFun-Passives" package="0603-RES" value="560">
<attribute name="NAME"/>
</element>
<element name="R14" library="SparkFun-Passives" package="0603-RES" value="560">
<attribute name="NAME"/>
</element>
<element name="JP4" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-2_LOCK" value="M023.5MM_LOCK"/>
<element name="R15" library="SparkFun-Passives" package="0603-RES" value="39k">
<attribute name="NAME"/>
</element>
<element name="Q4" library="SparkFun-DiscreteSemi" package="SOT23" value="MOSFET-NCHANNELBSS138">
<attribute name="PROD_ID" value="TRANS-00830"/>
<attribute name="NAME"/>
</element>
<element name="NRF24L01" library="RF_IR" package="2X4" value="NRF24L01"/>
<element name="JP5" library="SparkFun-Connectors" package="1X12_LOCK" value="M12LOCK">
<attribute name="NAME"/>
</element>
<element name="JP6" library="SparkFun-Connectors" package="1X12_LOCK" value="M12LOCK">
<attribute name="NAME"/>
</element>
<element name="R3" library="SparkFun-Passives" package="0603-RES" value="0"/>
</elements>
<signals>
<signal name="3.3V">
<contactref element="U$4" pad="21"/>
<contactref element="JP6" pad="4"/>
<contactref element="NRF24L01" pad="VCC"/>
</signal>
<signal name="GND">
<contactref element="R7" pad="2"/>
<contactref element="J1" pad="GND"/>
<contactref element="R8" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="U$4" pad="23"/>
<contactref element="U$4" pad="4"/>
<contactref element="Q1" pad="2"/>
<contactref element="Q2" pad="2"/>
<contactref element="Q3" pad="2"/>
<contactref element="R9" pad="2"/>
<contactref element="R15" pad="2"/>
<contactref element="Q4" pad="2"/>
<contactref element="NRF24L01" pad="GND"/>
<contactref element="JP5" pad="9"/>
<contactref element="JP6" pad="2"/>
</signal>
<signal name="VIN">
<contactref element="J1" pad="PWR"/>
<contactref element="JP3" pad="1"/>
<contactref element="JP2" pad="1"/>
<contactref element="U$4" pad="24"/>
<contactref element="R5" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="R10" pad="2"/>
<contactref element="R11" pad="2"/>
<contactref element="R12" pad="2"/>
<contactref element="R13" pad="2"/>
<contactref element="R14" pad="2"/>
<contactref element="JP4" pad="1"/>
<contactref element="JP6" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="D5" pad="C"/>
<contactref element="D6" pad="C"/>
<contactref element="D7" pad="C"/>
<contactref element="D8" pad="C"/>
<contactref element="D1" pad="C"/>
<contactref element="D4" pad="C"/>
<contactref element="D3" pad="C"/>
<contactref element="D2" pad="C"/>
<contactref element="Q3" pad="3"/>
</signal>
<signal name="RF_SCK">
<contactref element="U$4" pad="16"/>
<contactref element="NRF24L01" pad="SCK"/>
<contactref element="JP6" pad="9"/>
</signal>
<signal name="RF_MISO">
<contactref element="U$4" pad="15"/>
<contactref element="NRF24L01" pad="MISO"/>
<contactref element="JP6" pad="10"/>
</signal>
<signal name="P_RELAY">
<contactref element="U$4" pad="7"/>
<contactref element="U$1" pad="2"/>
<contactref element="JP5" pad="6"/>
</signal>
<signal name="P_FET1">
<contactref element="R7" pad="1"/>
<contactref element="U$4" pad="8"/>
<contactref element="Q1" pad="1"/>
<contactref element="JP5" pad="5"/>
</signal>
<signal name="P_FET2">
<contactref element="R8" pad="1"/>
<contactref element="U$4" pad="9"/>
<contactref element="Q2" pad="1"/>
<contactref element="JP5" pad="4"/>
</signal>
<signal name="P_IR">
<contactref element="R6" pad="1"/>
<contactref element="U$4" pad="6"/>
<contactref element="Q3" pad="1"/>
<contactref element="JP5" pad="7"/>
</signal>
<signal name="RF_MOSI">
<contactref element="U$4" pad="14"/>
<contactref element="NRF24L01" pad="MOSI"/>
<contactref element="JP6" pad="11"/>
</signal>
<signal name="N$16">
<contactref element="R9" pad="1"/>
<contactref element="U$1" pad="3"/>
</signal>
<signal name="N$12">
<contactref element="JP3" pad="2"/>
<contactref element="Q1" pad="3"/>
</signal>
<signal name="N$14">
<contactref element="JP2" pad="2"/>
<contactref element="Q2" pad="3"/>
</signal>
<signal name="N$1">
<contactref element="U$1" pad="8"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="U$1" pad="6"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="D1" pad="A"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="D2" pad="A"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="D3" pad="A"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="D4" pad="A"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="D5" pad="A"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="D6" pad="A"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="D7" pad="A"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="D8" pad="A"/>
<contactref element="R14" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="JP4" pad="2"/>
<contactref element="Q4" pad="3"/>
</signal>
<signal name="P_FET3">
<contactref element="R15" pad="1"/>
<contactref element="Q4" pad="1"/>
<contactref element="U$4" pad="12"/>
<contactref element="JP5" pad="1"/>
</signal>
<signal name="RF_CE">
<contactref element="NRF24L01" pad="CE"/>
<contactref element="U$4" pad="11"/>
<contactref element="JP5" pad="2"/>
</signal>
<signal name="RF_CSN">
<contactref element="NRF24L01" pad="CSN"/>
<contactref element="U$4" pad="10"/>
<contactref element="JP5" pad="3"/>
</signal>
<signal name="RF_IRQ">
<contactref element="NRF24L01" pad="IRQ"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="A3">
<contactref element="U$4" pad="20"/>
<contactref element="JP6" pad="5"/>
</signal>
<signal name="A2">
<contactref element="U$4" pad="19"/>
<contactref element="JP6" pad="6"/>
</signal>
<signal name="A1">
<contactref element="U$4" pad="18"/>
<contactref element="JP6" pad="7"/>
</signal>
<signal name="A0">
<contactref element="U$4" pad="17"/>
<contactref element="JP6" pad="8"/>
</signal>
<signal name="D10">
<contactref element="U$4" pad="13"/>
<contactref element="JP6" pad="12"/>
</signal>
<signal name="D2">
<contactref element="U$4" pad="5"/>
<contactref element="JP5" pad="8"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="RST">
<contactref element="U$4" pad="3"/>
<contactref element="U$4" pad="22"/>
<contactref element="JP5" pad="10"/>
<contactref element="JP6" pad="3"/>
</signal>
<signal name="RXI">
<contactref element="U$4" pad="2"/>
<contactref element="JP5" pad="11"/>
</signal>
<signal name="TXO">
<contactref element="U$4" pad="1"/>
<contactref element="JP5" pad="12"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
