<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="12.7" y2="0" width="0" layer="20"/>
<wire x1="12.7" y1="0" x2="12.7" y2="27.94" width="0" layer="20"/>
<wire x1="12.7" y1="27.94" x2="0" y2="27.94" width="0" layer="20"/>
<wire x1="0" y1="27.94" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X10">
</package>
</packages>
</library>
<library name="con-hirose">
<description>&lt;b&gt;Hirose Connectors&lt;/b&gt;&lt;p&gt;
www.hirose.co.jp&lt;p&gt;
Include : &lt;br&gt;
con-hirose-df12d(3.0)60dp0.5v80.lbr from Bob Starr &amp;lt;rtzaudio@mindspring.com&amp;gt;&lt;br&gt;
con-hirose.lbr from Bob Starr &amp;lt;rtzaudio@mindspring.com&amp;gt;&lt;br&gt;</description>
<packages>
<package name="FH21-10S-1DSA">
<description>&lt;b&gt;FPC Connector&lt;/b&gt;&lt;p&gt;
1 MM, vertical</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="SparkFun-Connectors" package="1X10" value="M10&quot;"/>
<element name="X1" library="con-hirose" package="FH21-10S-1DSA" value="FH21-10S-1DSA">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="X1" pad="10"/>
<contactref element="JP1" pad="10"/>
</signal>
<signal name="N$2">
<contactref element="X1" pad="9"/>
<contactref element="JP1" pad="9"/>
</signal>
<signal name="N$3">
<contactref element="X1" pad="8"/>
<contactref element="JP1" pad="8"/>
</signal>
<signal name="N$4">
<contactref element="X1" pad="7"/>
<contactref element="JP1" pad="7"/>
</signal>
<signal name="N$5">
<contactref element="X1" pad="6"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="N$6">
<contactref element="X1" pad="5"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="N$7">
<contactref element="X1" pad="4"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="N$8">
<contactref element="X1" pad="3"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="N$9">
<contactref element="X1" pad="2"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="X1" pad="1"/>
<contactref element="JP1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
