<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<description>Mountable board for the Alps Thru-hole 5-way Navigation Switch (SKQUCAA010) from adafruit. Uses a 2x3 pin header for connection to another board.</description>
<plain>
<wire x1="2.54" y1="0" x2="29.21" y2="0" width="0" layer="20"/>
<wire x1="29.21" y1="0" x2="31.75" y2="2.54" width="0" layer="20" curve="90"/>
<wire x1="31.75" y1="2.54" x2="31.75" y2="29.21" width="0" layer="20"/>
<wire x1="31.75" y1="29.21" x2="29.21" y2="31.75" width="0" layer="20" curve="90"/>
<wire x1="29.21" y1="31.75" x2="2.54" y2="31.75" width="0" layer="20"/>
<wire x1="2.54" y1="31.75" x2="0" y2="29.21" width="0" layer="20" curve="90"/>
<wire x1="0" y1="29.21" x2="0" y2="2.54" width="0" layer="20"/>
<wire x1="0" y1="2.54" x2="2.54" y2="0" width="0" layer="20" curve="90"/>
<text>SKQUCAA010</text>
<text>Basco Eng</text>
<text>v1</text>
<text>CNTR</text>
<text>RIGHT</text>
<text>COM</text>
<text>DOWN</text>
<text>LEFT</text>
<text>UP</text>
</plain>
<libraries>
<library name="gamaral">
<description>Miscellaneous components used by &lt;b&gt;gamaral&lt;/b&gt;</description>
<packages>
<package name="SKQU">
</package>
</packages>
</library>
<library name="holes">
<description>&lt;b&gt;Mounting Holes and Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="3,3">
<description>&lt;b&gt;MOUNTING HOLE&lt;/b&gt; 3.3 mm with drill center</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="2X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
<attribute name="PROJ_DESC" value="Mountable board for the Alps Thru-hole 5-way Navigation Switch (SKQUCAA010) from adafruit. Uses a 2x3 pin header for connection to another board."/>
<attribute name="PROJ_NAME" value="Alps Thru-hole 5-way Navigation Switch (SKQUCAA010)"/>
<attribute name="PROJ_VERSION" value="1"/>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="SW" library="gamaral" package="SKQU" value="SKQUCAA010">
<attribute name="OC_MOUSER" value="688-SKQUCA"/>
<attribute name="OC_NEWARK" value="59M1983"/>
<attribute name="MF" value="ALPS"/>
<attribute name="OC_ADAFRUIT" value="504"/>
</element>
<element name="HDR" library="pinhead" package="2X03" value=""/>
<element name="U$6" library="holes" package="3,3" value=""/>
<element name="U$2" library="holes" package="3,3" value=""/>
<element name="U$3" library="holes" package="3,3" value=""/>
<element name="U$4" library="holes" package="3,3" value=""/>
</elements>
<signals>
<signal name="N$1">
<contactref element="SW" pad="UP"/>
<contactref element="HDR" pad="5"/>
</signal>
<signal name="N$2">
<contactref element="SW" pad="LEFT"/>
<contactref element="HDR" pad="3"/>
</signal>
<signal name="N$3">
<contactref element="SW" pad="DOWN"/>
<contactref element="HDR" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="SW" pad="CENTER"/>
<contactref element="HDR" pad="6"/>
</signal>
<signal name="N$5">
<contactref element="SW" pad="RIGHT"/>
<contactref element="HDR" pad="4"/>
</signal>
<signal name="N$6">
<contactref element="SW" pad="COMMON"/>
<contactref element="HDR" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
