<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.0">
<drawing>
<board>
<plain>
<text>W</text>
<text>G</text>
<text>Y</text>
<text>Rc</text>
<text>C</text>
<text>O/B</text>
<wire x1="79.756" y1="0" x2="0" y2="0" width="0" layer="20"/>
<wire x1="0" y1="0" x2="0" y2="49.022" width="0" layer="20"/>
<wire x1="0" y1="49.022" x2="79.756" y2="49.022" width="0" layer="20"/>
<wire x1="79.756" y1="49.022" x2="79.756" y2="0" width="0" layer="20"/>
<text>Spark Core</text>
<wire x1="45.532" y1="10.30420625" x2="45.532" y2="29.9318625" width="0" layer="20"/>
<wire x1="45.532" y1="29.9318625" x2="42.9518625" y2="32.512" width="0" layer="20" curve="90"/>
<wire x1="42.9518625" y1="32.512" x2="38.439571875" y2="32.512" width="0" layer="20"/>
<wire x1="38.439571875" y1="32.512" x2="35.58" y2="29.652428125" width="0" layer="20" curve="90"/>
<wire x1="35.58" y1="29.652428125" x2="35.58" y2="10.244665625" width="0" layer="20"/>
<wire x1="35.58" y1="10.244665625" x2="37.784665625" y2="8.04" width="0" layer="20" curve="90"/>
<wire x1="37.784665625" y1="8.04" x2="43.26779375" y2="8.04" width="0" layer="20"/>
<wire x1="43.26779375" y1="8.04" x2="45.532" y2="10.30420625" width="0" layer="20" curve="90"/>
<text>Cutout</text>
<text>Rh</text>
<text>Fan</text>
<text>Cool</text>
<text>Heat</text>
<text>Rev</text>
<text>T_CS</text>
<text>LCD_CS</text>
<text>CuriousTech.net</text>
<text>Rc/Rh</text>
<text>Spark-O-Stat</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X04">
</package>
<package name="1X12_LOCK">
</package>
<package name="1X14_LOCK">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
<package name="DR1030">
<description>For Coiltronics/Cooper DR1030 series inductors</description>
</package>
</packages>
</library>
<library name="relay">
<description>&lt;b&gt;Relays&lt;/b&gt;&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;Eichhoff
&lt;li&gt;Finder
&lt;li&gt;Fujitsu
&lt;li&gt;HAMLIN
&lt;li&gt;OMRON
&lt;li&gt;Matsushita
&lt;li&gt;NAiS
&lt;li&gt;Siemens
&lt;li&gt;Schrack
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOP04">
<description>&lt;b&gt;SOP 04 - 4.3x4.4mm RM 2.54mm&lt;/b&gt; AQY21, AQY22, AQY61 Series NAiS&lt;p&gt;Source: http://www.mew-europe.com/..  pti_en.pdf</description>
</package>
</packages>
</library>
<library name="rectifier">
<description>&lt;b&gt;Rectifiers&lt;/b&gt;&lt;p&gt;
General Instrument, Semikron, Diotec, Fagor&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DFS">
<description>&lt;b&gt;Surface Mount Glass Passivated Bridge Rectifiers&lt;/hb&gt;&lt;p&gt;
Source: Comchip Bridge Rectifiers DF005S-G thru DF10S-G.pdf</description>
</package>
</packages>
</library>
<library name="con-weidmueller-sl35">
<description>&lt;b&gt;Weidmueller Clamp Connectors&lt;/b&gt;&lt;p&gt;
Type SL3.5&lt;p&gt; 
Grid 3.5 mm&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="180-7">
<description>&lt;b&gt;WEIDMUELLER CLAMP CONNECTOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="PANASONIC_C">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package E&lt;/b&gt;</description>
</package>
<package name="PANASONIC_D">
</package>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SMA-DIODE">
<description>&lt;B&gt;Diode&lt;/B&gt;&lt;p&gt;
Basic SMA packaged diode. Good for reverse polarization protection. Common part #: MBRA140</description>
</package>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="v-reg">
<description>&lt;b&gt;Voltage Regulators&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SO-08">
<description>&lt;B&gt;Small Outline Narrow Plastic Gull Wing&lt;/B&gt;&lt;p&gt;
150-mil body, package type SN</description>
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="BUZZER-12MM-NS">
</package>
</packages>
</library>
<library name="jumper">
<description>&lt;b&gt;Jumpers&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SJ">
<description>&lt;b&gt;Solder jumper&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="CuriousTech">
<description>CuriousTech custom misc parts</description>
<packages>
<package name="ROTORY_ENC">
<description>Panasonic EVEGA1F1524M or other EVE</description>
</package>
</packages>
</library>
<library name="Capacitor-Wima-SMD1812-100v">
<packages>
<package name="L4,8">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="B1" library="rectifier" package="DFS" value="DF206S-G"/>
<element name="_" library="con-weidmueller-sl35" package="180-7" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="AM2302" library="SparkFun-Connectors" package="1X04" value="AM2302"/>
<element name="K4" library="relay" package="SOP04" value="AQY282EHA">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="JP6" library="SparkFun-Connectors" package="1X12_LOCK" value=""/>
<element name="JP7" library="SparkFun-Connectors" package="1X12_LOCK" value=""/>
<element name="K1" library="relay" package="SOP04" value="AQY282EHA">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="K2" library="relay" package="SOP04" value="AQY282EHA">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="K3" library="relay" package="SOP04" value="AQY282EHA">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="D1" library="SparkFun-DiscreteSemi" package="SMA-DIODE" value="B260A-13-F"/>
<element name="R1" library="SparkFun-Passives" package="0805" value="470"/>
<element name="R2" library="SparkFun-Passives" package="0805" value="470"/>
<element name="R3" library="SparkFun-Passives" package="0805" value="470"/>
<element name="R4" library="SparkFun-Passives" package="0805" value="470"/>
<element name="LCD" library="SparkFun-Connectors" package="1X14_LOCK" value="2.4TouchLCD"/>
<element name="IC1" library="v-reg" package="SO-08" value="MIC4680-5.0YM"/>
<element name="C1" library="SparkFun-Capacitors" package="PANASONIC_C" value="UWD1V150MCL1"/>
<element name="C2" library="SparkFun-Capacitors" package="PANASONIC_D" value="UCL1A221MCL1GS"/>
<element name="L1" library="SparkFun-Passives" package="DR1030" value="SRU1048-680Y"/>
<element name="SG1" library="SparkFun-Electromechanical" package="BUZZER-12MM-NS" value="BUZZER"/>
<element name="Q1" library="SparkFun-DiscreteSemi" package="SOT23" value="NPN"/>
<element name="R5" library="SparkFun-Passives" package="0805" value="200"/>
<element name="C3" library="SparkFun-Capacitors" package="0805" value="0.1uF"/>
<element name="C4" library="SparkFun-Capacitors" package="0805" value="0.1uF"/>
<element name="SJ1" library="jumper" package="SJ" value=""/>
<element name="C5" library="SparkFun-Capacitors" package="0805" value="0.01uF"/>
<element name="ENC" library="CuriousTech" package="ROTORY_ENC" value="ROTARY_ENCODER"/>
<element name="C6" library="SparkFun-Capacitors" package="0805" value="0.01uF"/>
<element name="F1" library="Capacitor-Wima-SMD1812-100v" package="L4,8" value="1.5"/>
</elements>
<signals>
<signal name="N$20">
<contactref element="B1" pad="AC2"/>
<contactref element="_" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="K1" pad="3"/>
<contactref element="_" pad="3"/>
</signal>
<signal name="N$13">
<contactref element="K2" pad="3"/>
<contactref element="_" pad="4"/>
</signal>
<signal name="N$19">
</signal>
<signal name="N$21">
</signal>
<signal name="N$12">
</signal>
<signal name="GND">
<contactref element="B1" pad="-"/>
<contactref element="AM2302" pad="1"/>
<contactref element="JP6" pad="11"/>
<contactref element="JP7" pad="9"/>
<contactref element="K1" pad="2"/>
<contactref element="K2" pad="2"/>
<contactref element="K3" pad="2"/>
<contactref element="K4" pad="2"/>
<contactref element="D1" pad="A"/>
<contactref element="LCD" pad="13"/>
<contactref element="IC1" pad="5"/>
<contactref element="IC1" pad="8"/>
<contactref element="IC1" pad="7"/>
<contactref element="IC1" pad="6"/>
<contactref element="IC1" pad="1"/>
<contactref element="C1" pad="-"/>
<contactref element="C2" pad="-"/>
<contactref element="Q1" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="ENC" pad="C"/>
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="2"/>
</signal>
<signal name="+5V">
<contactref element="JP6" pad="12"/>
<contactref element="AM2302" pad="4"/>
<contactref element="LCD" pad="14"/>
<contactref element="IC1" pad="4"/>
<contactref element="C2" pad="+"/>
<contactref element="L1" pad="2"/>
<contactref element="SG1" pad="-"/>
<contactref element="C4" pad="1"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="N$24">
<contactref element="B1" pad="+"/>
<contactref element="IC1" pad="2"/>
<contactref element="C1" pad="+"/>
</signal>
<signal name="N$9">
<contactref element="B1" pad="AC1"/>
<contactref element="K1" pad="4"/>
<contactref element="K2" pad="4"/>
<contactref element="K3" pad="4"/>
<contactref element="SJ1" pad="2"/>
<contactref element="F1" pad="P$2"/>
</signal>
<signal name="N$29">
<contactref element="K3" pad="3"/>
<contactref element="_" pad="5"/>
</signal>
<signal name="N$3">
<contactref element="K4" pad="3"/>
<contactref element="_" pad="6"/>
</signal>
<signal name="+3V3">
<contactref element="JP7" pad="12"/>
</signal>
<signal name="N$2">
<contactref element="D1" pad="C"/>
<contactref element="IC1" pad="3"/>
<contactref element="L1" pad="1"/>
</signal>
<signal name="N$5">
</signal>
<signal name="N$6">
</signal>
<signal name="N$8">
</signal>
<signal name="N$4">
<contactref element="R1" pad="1"/>
<contactref element="K1" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="K2" pad="1"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="K3" pad="1"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="K4" pad="1"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="R3" pad="2"/>
<contactref element="JP7" pad="7"/>
</signal>
<signal name="N$17">
<contactref element="R2" pad="2"/>
<contactref element="JP7" pad="6"/>
</signal>
<signal name="N$26">
<contactref element="JP6" pad="10"/>
<contactref element="LCD" pad="12"/>
</signal>
<signal name="N$27">
<contactref element="LCD" pad="10"/>
<contactref element="JP6" pad="8"/>
</signal>
<signal name="N$22">
<contactref element="JP6" pad="6"/>
<contactref element="LCD" pad="9"/>
<contactref element="LCD" pad="3"/>
</signal>
<signal name="N$23">
<contactref element="JP6" pad="5"/>
<contactref element="LCD" pad="6"/>
<contactref element="LCD" pad="2"/>
</signal>
<signal name="N$25">
<contactref element="JP6" pad="9"/>
<contactref element="LCD" pad="11"/>
</signal>
<signal name="N$30">
<contactref element="JP6" pad="7"/>
<contactref element="LCD" pad="7"/>
</signal>
<signal name="N$33">
<contactref element="JP7" pad="2"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$34">
<contactref element="SG1" pad="+"/>
<contactref element="Q1" pad="3"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="N$39">
<contactref element="Q1" pad="1"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$28">
<contactref element="LCD" pad="8"/>
<contactref element="JP6" pad="4"/>
<contactref element="LCD" pad="5"/>
</signal>
<signal name="N$1">
<contactref element="LCD" pad="1"/>
<contactref element="JP6" pad="1"/>
</signal>
<signal name="N$36">
<contactref element="K4" pad="4"/>
<contactref element="SJ1" pad="1"/>
<contactref element="_" pad="7"/>
</signal>
<signal name="N$38">
</signal>
<signal name="N$42">
<contactref element="ENC" pad="B"/>
<contactref element="C5" pad="1"/>
<contactref element="JP7" pad="4"/>
</signal>
<signal name="N$43">
<contactref element="ENC" pad="A"/>
<contactref element="C6" pad="1"/>
<contactref element="JP7" pad="3"/>
</signal>
<signal name="N$14">
<contactref element="JP7" pad="8"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$18">
<contactref element="R1" pad="2"/>
<contactref element="JP7" pad="5"/>
</signal>
<signal name="N$32">
<contactref element="_" pad="2"/>
<contactref element="F1" pad="P$1"/>
</signal>
<signal name="N$35">
<contactref element="JP6" pad="3"/>
<contactref element="LCD" pad="4"/>
</signal>
<signal name="N$31">
<contactref element="JP6" pad="2"/>
<contactref element="AM2302" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
